<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="71.12" y2="0" width="0" layer="20"/>
<wire x1="71.12" y1="0" x2="71.12" y2="114.3" width="0" layer="20"/>
<wire x1="71.12" y1="114.3" x2="0" y2="114.3" width="0" layer="20"/>
<wire x1="0" y1="114.3" x2="0" y2="0" width="0" layer="20"/>
<hole x="63.119" y="107.95" drill="3.556"/>
<hole x="44.45" y="6.35" drill="3.556"/>
<hole x="63.5" y="6.35" drill="3.556"/>
<hole x="6.35" y="107.95" drill="3.556"/>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>3.3V</text>
<text>3.3V</text>
<text>3.3V</text>
<text>3.3V</text>
<text>RESET_N</text>
<text>RESET_N</text>
<text>SPI1_CE0_N</text>
<text>SPI1_CE0_N</text>
<text>STCLK</text>
<text>STCLK</text>
<text>D1_BUSY_N</text>
<text>D1_BUSY_N</text>
<text>SPI0_MOSI</text>
<text>SPI0_MOSI</text>
<text>SPI0_MISO</text>
<text>SPI0_MISO</text>
<text>SPI0_SCLK</text>
<text>SPI0_SCLK</text>
<text>GREEN</text>
<text>GREEN</text>
<text>RED</text>
<text>SPI1_MISO</text>
<text>SPI1_MISO</text>
<text>FLAG_N</text>
<text>FLAG_N</text>
<text>BLUE</text>
<text>SPI1_SCLK</text>
<text>SPI1_SCLK</text>
<text>SPI1_MOSI</text>
<text>SPI1_MOSI</text>
<text>SPI0_CE0_N</text>
<text>SPI0_CE0_N</text>
<text>D3_BUSY_N</text>
<text>D3_BUSY_N</text>
<text>D2_BUSY_N</text>
<text>SPI0_CE1_N</text>
<text>SPI0_CE1_N</text>
<text>GPIO2</text>
<text>GPIO2</text>
<text>GPIO3</text>
<text>GPIO3</text>
<text>GPIO14</text>
<text>GPIO14</text>
<text>GPIO15</text>
<text>GPIO15</text>
<text>VIN</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>D1_SW</text>
<text>D2_SW</text>
<text>D3_SW</text>
<text>GPIO15</text>
<text>GPIO14</text>
<text>GPIO3</text>
<text>GPIO2</text>
<text>D3_SW</text>
<text>D2_SW</text>
<text>D1_SW</text>
<text>GPIO15</text>
<text>GPIO14</text>
<text>GPIO3</text>
<text>GPIO2</text>
<text>Kappler</text>
<text>Step Zero</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="NIC_10X10.5_CAP">
<description>Some old package in our library</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="RPI-Zero">
<description>Generated from &lt;b&gt;TMC2660-test-with-grbl.brd&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="RASPBERRYPI_BASTELSTUBE_V13_RASPI_BOARD_B+_FULL">
<description>Raspberry Pi board model B+, full outline with position of big connectors &amp;amp; drill holes</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="GM1WA55311A">
<description>&lt;b&gt;Chip LED RGB&lt;/b&gt;&lt;p&gt;
Source: http://document.sharpsma.com/files/GM1WA55311A_SS.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="r-78xx_10">
<description>&lt;b&gt;Recom Innoline R-78xx Switching Regulators&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Version 1.0&lt;br&gt;
(c) 2015 Samuel Lourenço</description>
<packages>
<package name="SIP3V">
<description>&lt;b&gt;SIP3 Package&lt;/b&gt; - Vertical option&lt;br&gt;
&lt;br&gt;
Source: &lt;a href="http://www.recom-international.com/pdf/Innoline/R-78Bxx-1.0_L.pdf"&gt;http://www.recom-international.com/pdf/Innoline/R-78Bxx-1.0_L.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Special-Function">
<description>&lt;h3&gt;SparkFun Special Function ICs&lt;/h3&gt;
This library contains ICs that do not really fit into the other, more generic categories.  Basically, anything that serves some function but has a bunch of brains or special bias circuitry that prevents it from being used as a general part qualifies for this category.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;555 timers&lt;/li&gt;
&lt;li&gt;LED drivers&lt;/li&gt;
&lt;li&gt;H-Bridge drivers&lt;/li&gt;
&lt;li&gt;Motor drivers&lt;/li&gt;
&lt;li&gt;Waveform generators&lt;/li&gt;
&lt;li&gt;Crypto&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HTSSOP28">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="10nF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-00867"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603" value="0.22uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MC0805B224K500A5.08MM"/>
<attribute name="OC_NEWARK" value="46P6280"/>
<attribute name="PROD_ID" value="CAP-07822"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="NIC_10X10.5_CAP" value="100uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-08362"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="200mA/70V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="DIO-10647"/>
<attribute name="VALUE" value="200mA/70V"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="6A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="47k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="RES-07871"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="RES-07857"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="RES-07857"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="RES-07857"/>
</element>
<element name="U$1" library="RPI-Zero" package="RASPBERRYPI_BASTELSTUBE_V13_RASPI_BOARD_B+_FULL" value="RPI-ZERO">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="U2" library="SparkFun-IC-Special-Function" package="HTSSOP28" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="IC-10648"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="U1" library="SparkFun-IC-Special-Function" package="HTSSOP28" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="IC-10648"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="200mA/70V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="DIO-10647"/>
<attribute name="VALUE" value="200mA/70V"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603" value="10nF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-00867"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0603" value="0.22uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MC0805B224K500A5.08MM"/>
<attribute name="OC_NEWARK" value="46P6280"/>
<attribute name="PROD_ID" value="CAP-07822"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="47k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="RES-07871"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="RES-07857"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="RES-07857"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="U3" library="SparkFun-IC-Special-Function" package="HTSSOP28" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="IC-10648"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="200mA/70V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="DIO-10647"/>
<attribute name="VALUE" value="200mA/70V"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0603" value="10nF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-00867"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0603" value="0.22uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MC0805B224K500A5.08MM"/>
<attribute name="OC_NEWARK" value="46P6280"/>
<attribute name="PROD_ID" value="CAP-07822"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603" value="47k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="RES-07871"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="RES-07857"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="RES-07857"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="6A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="IC1" library="r-78xx_10" package="SIP3V" value="R-78B5.0-1.5">
<attribute name="MF" value="Recom"/>
<attribute name="MPN" value="R-78B5.0-1.5"/>
<attribute name="OC_FARNELL" value="1793163"/>
<attribute name="OC_NEWARK" value="62X9484"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="LED1" library="led" package="GM1WA55311A" value="GM1WA55311A"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="600mA/40V">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="600mA/40V">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="600mA/40V">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0603" value="100">
<attribute name="PROD_ID" value="RES-07863"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0603" value="100">
<attribute name="PROD_ID" value="RES-07863"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0603" value="100">
<attribute name="PROD_ID" value="RES-07863"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R20" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="NIC_10X10.5_CAP" value="100uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-08362"/>
</element>
<element name="C16" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C17" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C4" pad="2"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="34"/>
<contactref element="U$1" pad="25"/>
<contactref element="U$1" pad="39"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="20"/>
<contactref element="U$1" pad="30"/>
<contactref element="C3" pad="-"/>
<contactref element="C5" pad="2"/>
<contactref element="U2" pad="9"/>
<contactref element="U2" pad="21"/>
<contactref element="U2" pad="27"/>
<contactref element="U2" pad="13"/>
<contactref element="R6" pad="1"/>
<contactref element="J6" pad="2"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="27"/>
<contactref element="U3" pad="GND@PAD"/>
<contactref element="R9" pad="1"/>
<contactref element="J9" pad="2"/>
<contactref element="U3" pad="9"/>
<contactref element="U3" pad="21"/>
<contactref element="U3" pad="27"/>
<contactref element="U3" pad="13"/>
<contactref element="J10" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="C15" pad="-"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="U2" pad="GND@PAD"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="GND@PAD"/>
<contactref element="U1" pad="GND@10"/>
<contactref element="U1" pad="GND@11"/>
<contactref element="U1" pad="GND@12"/>
<contactref element="U1" pad="GND@13"/>
<contactref element="U1" pad="GND@14"/>
<contactref element="U1" pad="GND@15"/>
<contactref element="U1" pad="GND@16"/>
<contactref element="U1" pad="GND@17"/>
<contactref element="U1" pad="GND@18"/>
<contactref element="U1" pad="GND@19"/>
<contactref element="U1" pad="GND@20"/>
<contactref element="U1" pad="GND@21"/>
<contactref element="U1" pad="GND@22"/>
<contactref element="U1" pad="GND@23"/>
<contactref element="U1" pad="GND@24"/>
<contactref element="U1" pad="GND@25"/>
<contactref element="U1" pad="GND@26"/>
<contactref element="U1" pad="GND@27"/>
<contactref element="U1" pad="GND@28"/>
<contactref element="U1" pad="GND@29"/>
<contactref element="U1" pad="GND@30"/>
<contactref element="U2" pad="GND@10"/>
<contactref element="U2" pad="GND@11"/>
<contactref element="U2" pad="GND@12"/>
<contactref element="U2" pad="GND@13"/>
<contactref element="U2" pad="GND@14"/>
<contactref element="U2" pad="GND@15"/>
<contactref element="U2" pad="GND@16"/>
<contactref element="U2" pad="GND@17"/>
<contactref element="U2" pad="GND@18"/>
<contactref element="U2" pad="GND@19"/>
<contactref element="U2" pad="GND@20"/>
<contactref element="U2" pad="GND@21"/>
<contactref element="U2" pad="GND@22"/>
<contactref element="U2" pad="GND@23"/>
<contactref element="U2" pad="GND@24"/>
<contactref element="U2" pad="GND@25"/>
<contactref element="U2" pad="GND@26"/>
<contactref element="U2" pad="GND@27"/>
<contactref element="U2" pad="GND@28"/>
<contactref element="U2" pad="GND@29"/>
<contactref element="U2" pad="GND@30"/>
<contactref element="U3" pad="GND@10"/>
<contactref element="U3" pad="GND@11"/>
<contactref element="U3" pad="GND@12"/>
<contactref element="U3" pad="GND@13"/>
<contactref element="U3" pad="GND@14"/>
<contactref element="U3" pad="GND@15"/>
<contactref element="U3" pad="GND@16"/>
<contactref element="U3" pad="GND@17"/>
<contactref element="U3" pad="GND@18"/>
<contactref element="U3" pad="GND@19"/>
<contactref element="U3" pad="GND@20"/>
<contactref element="U3" pad="GND@21"/>
<contactref element="U3" pad="GND@22"/>
<contactref element="U3" pad="GND@23"/>
<contactref element="U3" pad="GND@24"/>
<contactref element="U3" pad="GND@25"/>
<contactref element="U3" pad="GND@26"/>
<contactref element="U3" pad="GND@27"/>
<contactref element="U3" pad="GND@28"/>
<contactref element="U3" pad="GND@29"/>
<contactref element="U3" pad="GND@30"/>
</signal>
<signal name="SPI0_MOSI">
<contactref element="U$1" pad="19"/>
<contactref element="U2" pad="20"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="SPI0_CE0_N">
<contactref element="U$1" pad="24"/>
<contactref element="U2" pad="23"/>
</signal>
<signal name="SPI0_MISO">
<contactref element="U$1" pad="21"/>
<contactref element="U2" pad="18"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="SPI0_SCLK">
<contactref element="U$1" pad="23"/>
<contactref element="U2" pad="19"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="RESET_N">
<contactref element="U$1" pad="13"/>
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="3"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="FLAG_N">
<contactref element="U2" pad="24"/>
<contactref element="U$1" pad="37"/>
<contactref element="U1" pad="24"/>
<contactref element="R3" pad="1"/>
<contactref element="U3" pad="24"/>
</signal>
<signal name="D1_BUSY_N">
<contactref element="U2" pad="22"/>
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="D1_CPC">
<contactref element="C1" pad="1"/>
<contactref element="D1" pad="3"/>
</signal>
<signal name="D1_CP">
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="D1_VBOOT">
<contactref element="D1" pad="2"/>
<contactref element="U2" pad="11"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="D1_ADCIN">
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="D1_O1A">
<contactref element="U2" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="D1_O2A">
<contactref element="J1" pad="2"/>
<contactref element="U2" pad="28"/>
</signal>
<signal name="D1_O1B">
<contactref element="U2" pad="14"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="D1_O2B">
<contactref element="U2" pad="15"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="17"/>
<contactref element="U$1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U2" pad="17"/>
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="17"/>
<contactref element="R10" pad="2"/>
<contactref element="U3" pad="17"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="IC1" pad="3"/>
<contactref element="LED1" pad="4"/>
</signal>
<signal name="VIN">
<contactref element="U2" pad="2"/>
<contactref element="D1" pad="1"/>
<contactref element="U2" pad="26"/>
<contactref element="U2" pad="12"/>
<contactref element="U2" pad="16"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="+"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="D2" pad="1"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="16"/>
<contactref element="C7" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="D3" pad="1"/>
<contactref element="U3" pad="26"/>
<contactref element="U3" pad="12"/>
<contactref element="U3" pad="16"/>
<contactref element="C9" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="J10" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C15" pad="+"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="D1_SW">
<contactref element="U2" pad="4"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="STCLK">
<contactref element="U2" pad="25"/>
<contactref element="U1" pad="25"/>
<contactref element="U3" pad="25"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="D2_BUSY_N">
<contactref element="U1" pad="22"/>
<contactref element="R8" pad="1"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="D2_CPC">
<contactref element="C6" pad="1"/>
<contactref element="D2" pad="3"/>
</signal>
<signal name="D2_SW">
<contactref element="U1" pad="4"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="D2_CP">
<contactref element="C6" pad="2"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="D2_VBOOT">
<contactref element="D2" pad="2"/>
<contactref element="U1" pad="11"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="D2_O1A">
<contactref element="U1" pad="1"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="D2_O2A">
<contactref element="J4" pad="2"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="D2_O1B">
<contactref element="U1" pad="14"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="D2_O2B">
<contactref element="U1" pad="15"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="D2_ADCIN">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="SPI0_CE1_N">
<contactref element="U1" pad="23"/>
<contactref element="U$1" pad="26"/>
</signal>
<signal name="D3_BUSY_N">
<contactref element="U3" pad="22"/>
<contactref element="R10" pad="1"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="D3_CPC">
<contactref element="C8" pad="1"/>
<contactref element="D3" pad="3"/>
</signal>
<signal name="D3_SW">
<contactref element="U3" pad="4"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="D3_CP">
<contactref element="C8" pad="2"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="D3_VBOOT">
<contactref element="D3" pad="2"/>
<contactref element="U3" pad="11"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="D3_O1A">
<contactref element="U3" pad="1"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="D3_O2A">
<contactref element="J7" pad="2"/>
<contactref element="U3" pad="28"/>
</signal>
<signal name="D3_O1B">
<contactref element="U3" pad="14"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="D3_O2B">
<contactref element="U3" pad="15"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="D3_ADCIN">
<contactref element="R7" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="SPI1_CE0_N">
<contactref element="U$1" pad="12"/>
<contactref element="U3" pad="23"/>
</signal>
<signal name="SPI1_MISO">
<contactref element="U$1" pad="35"/>
<contactref element="U3" pad="18"/>
</signal>
<signal name="SPI1_SCLK">
<contactref element="U$1" pad="40"/>
<contactref element="U3" pad="19"/>
</signal>
<signal name="SPI1_MOSI">
<contactref element="U$1" pad="38"/>
<contactref element="U3" pad="20"/>
</signal>
<signal name="D1_VREG">
<contactref element="U2" pad="6"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="D2_VREG">
<contactref element="U1" pad="6"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="D3_VREG">
<contactref element="U3" pad="6"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="2"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="3"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LED1" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R11" pad="2"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R12" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R13" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LED1" pad="3"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R16" pad="1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="R14" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="LED_GREEN_CTL">
<contactref element="U$1" pad="33"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="LED_RED_CTL">
<contactref element="U$1" pad="32"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="LED_BLUE_CTL">
<contactref element="U$1" pad="22"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="GPIO14">
<contactref element="U$1" pad="8"/>
<contactref element="J11" pad="2"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="GPIO15">
<contactref element="U$1" pad="10"/>
<contactref element="J11" pad="1"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="GPIO2">
<contactref element="U$1" pad="3"/>
<contactref element="J12" pad="2"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="GPIO3">
<contactref element="U$1" pad="5"/>
<contactref element="J12" pad="1"/>
<contactref element="R18" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
