<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="-0.3175" y1="0.9525" x2="36.1825" y2="0.9525" width="0" layer="20"/>
<wire x1="36.1825" y1="0.9525" x2="36.1825" y2="17.135" width="0" layer="20"/>
<wire x1="36.1825" y1="17.135" x2="-0.3175" y2="17.135" width="0" layer="20"/>
<wire x1="-0.3175" y1="17.135" x2="-0.3175" y2="0.9525" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="1X02_LOCK">
</package>
</packages>
</library>
<library name="custom">
<packages>
<package name="BANANAFEMALE-10.8-5.7">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="USB-A-H" value="USB-A-H">
<attribute name="PROD_ID" value="CONN-08367"/>
</element>
<element name="U$1" library="custom" package="BANANAFEMALE-10.8-5.7" value="BANANAFEMAIL-10.8-5.7"/>
<element name="U$2" library="custom" package="BANANAFEMALE-10.8-5.7" value="BANANAFEMAIL-10.8-5.7"/>
<element name="JP3" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="USB-A-H" value="USB-A-H">
<attribute name="PROD_ID" value="CONN-08367"/>
</element>
</elements>
<signals>
<signal name="5VA">
<contactref element="U$2" pad="P$1"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP1" pad="GND"/>
</signal>
<signal name="5VB">
<contactref element="U$1" pad="P$1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="GND"/>
</signal>
<signal name="N$1">
<contactref element="JP2" pad="D-"/>
<contactref element="JP1" pad="D-"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="D+"/>
<contactref element="JP2" pad="D+"/>
</signal>
<signal name="GND">
<contactref element="JP2" pad="VBUS"/>
<contactref element="JP1" pad="VBUS"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
