<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.48" y2="0" width="0.4064" layer="20"/>
<wire x1="30.48" y1="0" x2="30.48" y2="76.2" width="0.4064" layer="20"/>
<wire x1="30.48" y1="76.2" x2="0" y2="76.2" width="0.4064" layer="20"/>
<wire x1="0" y1="76.2" x2="0" y2="0" width="0.4064" layer="20"/>
<hole x="15.24" y="13.081" drill="2.8"/>
<hole x="15.24" y="63.119" drill="2.8"/>
<text>  RV-Project.Com
LED Automation v2.0</text>
<text>Batt NEG</text>
<text>Batt POS</text>
<text>Option 1</text>
<text>Option 2</text>
<text>Option 1</text>
<text>Option 1</text>
<text>Option 2</text>
<text>POS</text>
<text>RED</text>
<text>GRN</text>
<text>BLU</text>
<text>MONO</text>
<text>Option 1: Monochrome Version
Option 2: RGB Version</text>
<text>Daylight
Sens Adj.</text>
</plain>
<libraries>
<library name="alsstuff">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="RADIAL_ELECTROLYTIC_100MIL">
<description>Generic Electrolytic Capacitor 0.100 spacing 0.200 diameter.</description>
</package>
<package name="GENERIC_0100_DEVICE_100_SPACING">
<description>&lt;h3&gt;Small Capacitor&lt;/h3&gt;
Commonly used for small ceramic capacitors 0100 spacing.</description>
</package>
<package name="1/4W_AXIAL">
<description>Standard Axial 1/4Watt Resistor&lt;p&gt;0.45" footprint</description>
</package>
<package name="BOURNS3362_P">
<description>Standard Bourns Cermet Trimmer
&lt;p&gt;&lt;a href="http://www.mouser.com/ds/2/54/3362-55248.pdf"&gt;Data Sheet&lt;/a&gt;</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="SCREWTERMINAL-3.5MM-4">
</package>
</packages>
</library>
<library name="photo-elements">
<description>&lt;b&gt;Photocells&lt;/b&gt;&lt;p&gt;
Manufakturer: PerkinElmer Optoelektronics&lt;br&gt;
www.perkinelmer.com/opto</description>
<packages>
<package name="D11XX">
<description>&lt;b&gt;Photo Sensor&lt;/b&gt; Oil Burner Control Applications&lt;p&gt;
Source: http://optoelectronics.perkinelmer.com/content/Datasheets/DTS_PhotocellsD1160.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-04">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="alsstuff" package="RADIAL_ELECTROLYTIC_100MIL" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="VOLTAGE" value="25v"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="alsstuff" package="RADIAL_ELECTROLYTIC_100MIL" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="VOLTAGE" value="25v"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="alsstuff" package="GENERIC_0100_DEVICE_100_SPACING" value="0.1UF">
<attribute name="MARKING" value="104 (100nF)"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-4" value="">
<attribute name="PROD_ID" value="Combine 2x8399"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PH1" library="photo-elements" package="D11XX" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="BC338">
<attribute name="PROD_ID" value="TRANS-09536"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92" value="BC338">
<attribute name="PROD_ID" value="TRANS-09536"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="TO-92" value="BC338">
<attribute name="PROD_ID" value="TRANS-09536"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="alsstuff" package="1/4W_AXIAL" value="22K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="alsstuff" package="1/4W_AXIAL" value="33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="alsstuff" package="1/4W_AXIAL" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="alsstuff" package="BOURNS3362_P" value="10k">
<attribute name="MARKING" value="103"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="alsstuff" package="DIP08" value="ATTiny85">
<attribute name="PROD_ID" value="IC-09445"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="linear" package="TO92" value="78L33Z">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="special" package="EDG-04" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R9" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="Q1" pad="3"/>
<contactref element="PH1" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="3"/>
<contactref element="SW1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="R7" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="Q1" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="PH1" pad="1"/>
<contactref element="R8" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="SW1" pad="5"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="SW1" pad="6"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R3" pad="2"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R6" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="SW1" pad="7"/>
</signal>
<signal name="N$11">
<contactref element="J2" pad="3"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="J2" pad="4"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="1"/>
<contactref element="SW1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
