<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="104.14" y2="0" width="0.4064" layer="20"/>
<wire x1="104.14" y1="0" x2="104.14" y2="15.24" width="0.4064" layer="20"/>
<wire x1="104.14" y1="15.24" x2="0" y2="15.24" width="0.4064" layer="20"/>
<wire x1="0" y1="15.24" x2="0" y2="0" width="0.4064" layer="20"/>
<hole x="27.94" y="2.54" drill="2.8"/>
<hole x="101.6" y="12.7" drill="2.8"/>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="3386U">
<description>&lt;h3&gt;TSR-3386U Trimpot&lt;/h3&gt;
Trimpot with a knob&lt;br&gt;
For COM-09806 in the SparkFun catalog&lt;br&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="D2" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="D3" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="D4" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="D5" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="D6" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="PROD_ID" value="CONN-08197"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="470"/>
<element name="R2" library="SparkFun-Electromechanical" package="3386U" value="TSR-3386">
<attribute name="PROD_ID" value="RES-09730"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="GND"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R2" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="PWR"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D6" pad="K"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="D5" pad="K"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="D4" pad="K"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="D3" pad="K"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="D2" pad="K"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="D1" pad="K"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="VOUT">
<contactref element="R2" pad="2"/>
<contactref element="D6" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
