<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="-0.9525" y1="-0.9525" x2="31.4125" y2="-0.9525" width="0" layer="20"/>
<wire x1="31.4125" y1="-0.9525" x2="31.445" y2="27.6025" width="0" layer="20"/>
<wire x1="31.445" y1="27.6025" x2="-0.9525" y2="27.61" width="0" layer="20"/>
<wire x1="-0.9525" y1="27.61" x2="-0.9525" y2="-0.9525" width="0" layer="20"/>
<wire x1="-0.9525" y1="-0.9525" x2="31.4325" y2="-0.9525" width="0.4064" layer="46"/>
<wire x1="31.4325" y1="-0.9525" x2="31.4325" y2="27.6225" width="0.4064" layer="46"/>
<wire x1="31.4325" y1="27.6225" x2="-0.9525" y2="27.6225" width="0.4064" layer="46"/>
<wire x1="-0.9525" y1="27.6225" x2="-0.9525" y2="-0.9525" width="0.4064" layer="46"/>
<hole x="30.1625" y="26.035" drill="1.6"/>
<hole x="0.3175" y="26.035" drill="1.6"/>
<text>DIM1</text>
<text>DIM2</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
<description>&lt;h3&gt;RJ45 Socket with PCB Mounting Posts&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Prototyping/04908.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;RJ45-8&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="dwayne_custom">
<packages>
<package name="LEDVOLTPADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="RJ45-8" value="RJ45">
<attribute name="SF_ID" value="PRT-00643"/>
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="RJ45-8" value="RJ45">
<attribute name="SF_ID" value="PRT-00643"/>
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="U$1" library="dwayne_custom" package="LEDVOLTPADS" value="LEDVOLTMETER"/>
<element name="U$2" library="dwayne_custom" package="LEDVOLTPADS" value="LEDVOLTMETER"/>
</elements>
<signals>
<signal name="DIM2">
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="3"/>
<contactref element="U$2" pad="P$3"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="4"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="VCC">
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="5"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="DIM1">
<contactref element="J2" pad="6"/>
<contactref element="J1" pad="6"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="N$7">
<contactref element="J2" pad="7"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="J2" pad="8"/>
<contactref element="J1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
