<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="44.882" y2="0" width="0" layer="20"/>
<wire x1="44.882" y1="0" x2="44.882" y2="30.216" width="0" layer="20"/>
<wire x1="44.882" y1="30.216" x2="0" y2="30.216" width="0" layer="20"/>
<wire x1="0" y1="30.216" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>+5V</text>
<text>RESET</text>
<text>RX</text>
<text>TX</text>
<text>+5V</text>
<text>GND</text>
<text>GND</text>
<text>6-12V</text>
<text>A5</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>SDA</text>
<text>SCL</text>
<text>D12</text>
<text>D11</text>
<text>D10</text>
<text>D9</text>
<text>D8</text>
<text>D7</text>
<text>D6</text>
<text>D5</text>
<text>AMS1117</text>
<text>10uF</text>
<text>10uF</text>
<text>RESET</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>C1</text>
<text>C2</text>
<text>1N4002</text>
<text>D1</text>
<text>D2</text>
<text>ATMEGA328P</text>
<text>Verzija 1.0</text>
<text>ATMEL</text>
<text>ATMEGA328P</text>
<text>Slobodan Pajic</text>
<text>Minimum Board</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="NX3225">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-SMD">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO-214AC">
<description>&lt;b&gt;SURFACE MOUNT GENERAL RECTIFIER&lt;/b&gt; JEDEC DO-214AC molded platic body&lt;p&gt;
Method 2026&lt;br&gt;
Source: http://www.kingtronics.com/SMD_M7/M7_SMD_4007.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_ROUND">
</package>
<package name="1X05">
</package>
<package name="1X04">
</package>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="22pf"/>
<element name="C2" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="22pf"/>
<element name="ATMEGA328P" library="atmel" package="TQFP32-08" value="328P-PU"/>
<element name="LED1" library="adafruit" package="CHIP-LED0603" value="">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="adafruit" package="NX3225" value=""/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="220R"/>
<element name="S1" library="SparkFun-Retired" package="TACTILE-SWITCH-SMD" value="Switch-RST">
<attribute name="PROD_ID" value="SWCH-08247"/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="SOT223" value="">
<attribute name="PROD_ID" value="VREG-08170"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="1" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO-214AC" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="LED2" library="adafruit" package="CHIP-LED0603" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="220R"/>
<element name="J1" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="ATMEGA328P" pad="3"/>
<contactref element="ATMEGA328P" pad="5"/>
<contactref element="ATMEGA328P" pad="21"/>
<contactref element="C4" pad="C"/>
<contactref element="C2" pad="C"/>
<contactref element="U1" pad="1"/>
<contactref element="1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="J6" pad="2"/>
<contactref element="J6" pad="1"/>
<contactref element="J4" pad="4"/>
<contactref element="J4" pad="3"/>
<contactref element="J4" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="J7" pad="8"/>
<contactref element="J7" pad="7"/>
<contactref element="J7" pad="6"/>
<contactref element="J7" pad="5"/>
<contactref element="J7" pad="4"/>
<contactref element="J7" pad="3"/>
<contactref element="J7" pad="2"/>
<contactref element="J7" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="Q1" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="XTAL1">
<contactref element="Q1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="ATMEGA328P" pad="7"/>
</signal>
<signal name="XTAL2">
<contactref element="Q1" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="ATMEGA328P" pad="8"/>
</signal>
<signal name="N$5">
<contactref element="1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="VIN">
<contactref element="C4" pad="A"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="ATMEGA328P" pad="6"/>
<contactref element="ATMEGA328P" pad="4"/>
<contactref element="ATMEGA328P" pad="18"/>
<contactref element="ATMEGA328P" pad="20"/>
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J8" pad="4"/>
<contactref element="J8" pad="1"/>
<contactref element="J8" pad="2"/>
<contactref element="J8" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="3"/>
<contactref element="C2" pad="A"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="2"/>
<contactref element="ATMEGA328P" pad="17"/>
</signal>
<signal name="N$9">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="LED2" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="A0">
<contactref element="ATMEGA328P" pad="23"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="A1">
<contactref element="ATMEGA328P" pad="24"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="A2">
<contactref element="ATMEGA328P" pad="25"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="A3">
<contactref element="ATMEGA328P" pad="26"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="A4">
<contactref element="ATMEGA328P" pad="27"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="A5">
<contactref element="ATMEGA328P" pad="28"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="A6">
<contactref element="ATMEGA328P" pad="19"/>
</signal>
<signal name="A7">
<contactref element="ATMEGA328P" pad="22"/>
</signal>
<signal name="RX">
<contactref element="ATMEGA328P" pad="30"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="TX">
<contactref element="ATMEGA328P" pad="31"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="D2">
<contactref element="ATMEGA328P" pad="32"/>
</signal>
<signal name="D3">
<contactref element="ATMEGA328P" pad="1"/>
</signal>
<signal name="D4">
<contactref element="ATMEGA328P" pad="2"/>
</signal>
<signal name="D5">
<contactref element="ATMEGA328P" pad="9"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="D6">
<contactref element="ATMEGA328P" pad="10"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="D7">
<contactref element="ATMEGA328P" pad="11"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="D8">
<contactref element="ATMEGA328P" pad="12"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="D9">
<contactref element="ATMEGA328P" pad="13"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="D10">
<contactref element="ATMEGA328P" pad="14"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="D11">
<contactref element="ATMEGA328P" pad="15"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="D12">
<contactref element="ATMEGA328P" pad="16"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="ATMEGA328P" pad="29"/>
<contactref element="S1" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="J2" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
