<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="19.304" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="31.73" y2="0" width="0" layer="20"/>
<wire x1="31.73" y1="0" x2="33" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="33" y1="1.27" x2="33" y2="19.304" width="0" layer="20"/>
<wire x1="33" y1="19.304" x2="31.73" y2="20.574" width="0" layer="20" curve="90"/>
<wire x1="31.73" y1="20.574" x2="28.702" y2="20.574" width="0" layer="20"/>
<wire x1="28.702" y1="20.574" x2="21.59" y2="26.924" width="0" layer="20"/>
<wire x1="21.59" y1="26.924" x2="11.43" y2="26.924" width="0" layer="20"/>
<wire x1="11.43" y1="26.924" x2="4.318" y2="20.574" width="0" layer="20"/>
<wire x1="4.318" y1="20.574" x2="1.27" y2="20.574" width="0" layer="20"/>
<wire x1="1.27" y1="20.574" x2="0" y2="19.304" width="0" layer="20" curve="90"/>
<text>XBee Skin
MicroPython pyboard
v1.2 Rob Faludi
faludi.com</text>
<text>TX</text>
<text>RTS</text>
<text>CTS</text>
<text>3.3V</text>
<text>GND</text>
<text>RESET</text>
<text>SLEEP RQ</text>
<text>STATUS</text>
<text>RX</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="XBEE-1">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ASSC" library="SparkFun-LED" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RSSI" library="SparkFun-LED" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="PYBOARD_RESET" library="SparkFun-Electromechanical" package="TACTILE_SWITCH_SMD" value="TS-1188E">
<attribute name="NAME"/>
</element>
<element name="U$1" library="SparkFun-RF" package="XBEE-1" value="XBEE-1B1"/>
</elements>
<signals>
<signal name="XBEE_RX">
<contactref element="JP1" pad="8"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="XBEE_TX">
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="RTS">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="CTS">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="3.3V">
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="JP2" pad="3"/>
<contactref element="U$1" pad="10"/>
<contactref element="ASSC" pad="C"/>
<contactref element="RSSI" pad="C"/>
<contactref element="PYBOARD_RESET" pad="3"/>
</signal>
<signal name="SLP_CTRL">
<contactref element="JP2" pad="5"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="SLP_STATUS">
<contactref element="JP2" pad="6"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="ASSC">
<contactref element="U$1" pad="15"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="RSSI">
<contactref element="U$1" pad="6"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="ASSC" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="JP2" pad="4"/>
<contactref element="PYBOARD_RESET" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="RSSI" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
