<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="77.153575" y1="67.63010625" x2="94.710340625" y2="67.597440625" width="0" layer="20"/>
<wire x1="94.710340625" y1="67.597440625" x2="94.716378125" y2="80.016825" width="0" layer="20"/>
<wire x1="94.716378125" y1="80.016825" x2="77.153575" y2="80.025565625" width="0" layer="20"/>
<wire x1="77.153575" y1="80.025565625" x2="77.153575" y2="67.63010625" width="0" layer="20"/>
<text>GND</text>
<text>VGND</text>
<text>VCH</text>
<text>Copyright (C) Roger J Parkinson
Connector for Beaglebone to Chime</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_NO_SILK_YES_STOP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="adafruit" package="CHIP-LED0603" value="-ve">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X06_NO_SILK_YES_STOP" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X06_NO_SILK_YES_STOP" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="R0603" value="47M">
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R0603" value="4.7K">
<attribute name="VALUE"/>
</element>
<element name="T2" library="adafruit" package="TO92-EBC-OVAL" value="2N2222"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP6" pad="1"/>
<contactref element="T2" pad="E"/>
</signal>
<signal name="CHIME_V">
<contactref element="JP5" pad="4"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="JP5" pad="6"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="CHIME_G">
<contactref element="JP6" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="T2" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="R5" pad="2"/>
<contactref element="T2" pad="B"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
