<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="44.12" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="2.54" y2="-1.27" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="-1.27" x2="59.67" y2="-1.27" width="0" layer="20"/>
<wire x1="59.67" y1="-1.27" x2="62.21" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="62.21" y1="1.27" x2="62.21" y2="44.12" width="0" layer="20"/>
<wire x1="62.21" y1="44.12" x2="59.67" y2="46.66" width="0" layer="20" curve="90"/>
<wire x1="59.67" y1="46.66" x2="2.54" y2="46.66" width="0" layer="20"/>
<wire x1="2.54" y1="46.66" x2="0" y2="44.12" width="0" layer="20" curve="90"/>
<hole x="14.078" y="13.532" drill="3.264"/>
<hole x="2.648" y="44.012" drill="3.264"/>
<text>3RD</text>
<text>MN</text>
<text>APO</text>
<text>GND</text>
<text>+</text>
<text>VP BATT</text>
<text>PT</text>
<text>PM</text>
<text>PD</text>
<hole x="47.098" y="13.532" drill="3.264"/>
<hole x="59.562" y="44.012" drill="3.264"/>
<text>ST</text>
<text>SM</text>
<text>ST</text>
<text>3RD</text>
<text>MN</text>
<text>APO</text>
<text>GND</text>
<text>+</text>
<text>VS BATT</text>
<text>VS SWTCH</text>
<text>VP SWTCH</text>
<text>+</text>
<text>+</text>
<text>_</text>
<text>_</text>
<text>VP</text>
<text>VS</text>
<text>CRW</text>
<text>RAVEN PCB
v1.0
--------
Tom Teper</text>
</plain>
<libraries>
<library name="2023-12-19_19-33-24_Library">
<packages>
<package name="CONN2_710002_WRE">
</package>
</packages>
</library>
<library name="2023-12-19_19-38-56_Library">
<packages>
<package name="CONN_1935190_PXC">
</package>
</packages>
</library>
<library name="2023-12-19_19-41-36_Library">
<packages>
<package name="CONN_1935200_PXC">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="VP_BAT_IN" library="2023-12-19_19-33-24_Library" package="CONN2_710002_WRE" value="691137710002CONN2_710002_WRE">
<attribute name="COPYRIGHT" value="Copyright (C) 2023 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="691137710002"/>
<attribute name="MFR_NAME" value="Wurth Electronics"/>
<attribute name="NAME"/>
</element>
<element name="VP_BLUE_RAVEN" library="2023-12-19_19-38-56_Library" package="CONN_1935190_PXC" value="1935190CONN_1935190_PXC">
<attribute name="COPYRIGHT" value="Copyright (C) 2023 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="1935190"/>
<attribute name="MFR_NAME" value="Phoenix Contact"/>
<attribute name="NAME"/>
</element>
<element name="VP_SWTCH" library="2023-12-19_19-33-24_Library" package="CONN2_710002_WRE" value="691137710002CONN2_710002_WRE">
<attribute name="COPYRIGHT" value="Copyright (C) 2023 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="691137710002"/>
<attribute name="MFR_NAME" value="Wurth Electronics"/>
</element>
<element name="VP_OUT" library="2023-12-19_19-41-36_Library" package="CONN_1935200_PXC" value="1935200CONN_1935200_PXC">
<attribute name="COPYRIGHT" value="Copyright (C) 2023 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="1935200"/>
<attribute name="MFR_NAME" value="Phoenix Contact"/>
<attribute name="NAME"/>
</element>
<element name="VS_BAT_IN" library="2023-12-19_19-33-24_Library" package="CONN2_710002_WRE" value="691137710002CONN2_710002_WRE">
<attribute name="COPYRIGHT" value="Copyright (C) 2023 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="691137710002"/>
<attribute name="MFR_NAME" value="Wurth Electronics"/>
<attribute name="NAME"/>
</element>
<element name="VS_SWTCH" library="2023-12-19_19-33-24_Library" package="CONN2_710002_WRE" value="691137710002CONN2_710002_WRE">
<attribute name="COPYRIGHT" value="Copyright (C) 2023 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="691137710002"/>
<attribute name="MFR_NAME" value="Wurth Electronics"/>
<attribute name="NAME"/>
</element>
<element name="VS_OUT" library="2023-12-19_19-41-36_Library" package="CONN_1935200_PXC" value="1935200CONN_1935200_PXC">
<attribute name="COPYRIGHT" value="Copyright (C) 2023 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="1935200"/>
<attribute name="MFR_NAME" value="Phoenix Contact"/>
<attribute name="NAME"/>
</element>
<element name="VS_BLUE_RAVEN" library="2023-12-19_19-38-56_Library" package="CONN_1935190_PXC" value="1935190CONN_1935190_PXC">
<attribute name="COPYRIGHT" value="Copyright (C) 2023 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="1935190"/>
<attribute name="MFR_NAME" value="Phoenix Contact"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="VP_BAT_IN" pad="1"/>
<contactref element="VP_BLUE_RAVEN" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="VP_BAT_IN" pad="2"/>
<contactref element="VP_SWTCH" pad="1"/>
</signal>
<signal name="VP+">
<contactref element="VP_SWTCH" pad="2"/>
<contactref element="VP_BLUE_RAVEN" pad="5"/>
<contactref element="VP_OUT" pad="2"/>
<contactref element="VP_OUT" pad="4"/>
<contactref element="VP_OUT" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="VP_OUT" pad="5"/>
<contactref element="VP_BLUE_RAVEN" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="VP_OUT" pad="3"/>
<contactref element="VP_BLUE_RAVEN" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="VP_OUT" pad="1"/>
<contactref element="VP_BLUE_RAVEN" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="VS_BAT_IN" pad="1"/>
<contactref element="VS_BLUE_RAVEN" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="VS_BAT_IN" pad="2"/>
<contactref element="VS_SWTCH" pad="1"/>
</signal>
<signal name="VS+">
<contactref element="VS_SWTCH" pad="2"/>
<contactref element="VS_BLUE_RAVEN" pad="5"/>
<contactref element="VS_OUT" pad="2"/>
<contactref element="VS_OUT" pad="4"/>
<contactref element="VS_OUT" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="VS_OUT" pad="5"/>
<contactref element="VS_BLUE_RAVEN" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="VS_OUT" pad="3"/>
<contactref element="VS_BLUE_RAVEN" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="VS_OUT" pad="1"/>
<contactref element="VS_BLUE_RAVEN" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
