<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>VCC</text>
<text>PB0</text>
<text>PB1</text>
<text>PB3</text>
<text>PB2</text>
<text>PA7</text>
<text>PA6</text>
<text>GND</text>
<text>PA0</text>
<text>PA1</text>
<text>PA2</text>
<text>PA3</text>
<text>PA4</text>
<text>PA5</text>
<wire x1="0" y1="18.034" x2="15.494" y2="18.034" width="0" layer="20"/>
<wire x1="15.494" y1="18.034" x2="15.494" y2="0" width="0" layer="20"/>
<wire x1="15.494" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="18.034" width="0" layer="20"/>
<text>MISO</text>
<text>+5V</text>
<text>SCK</text>
<text>MOSI</text>
<text>RESET</text>
<text>GND</text>
</plain>
<libraries>
<library name="Colin's Library">
<packages>
<package name="SOIC14">
</package>
<package name="JP7_RND">
</package>
<package name="JP7">
</package>
<package name="COLIN_7_5MM_GOLD">
</package>
<package name="ATMEL_7.5MM">
</package>
<package name="ATTINY841_7.5MM">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Colin's Library" package="SOIC14" value="ATTINY841_SOIC14"/>
<element name="U$2" library="Colin's Library" package="JP7" value="JP7"/>
<element name="U$3" library="Colin's Library" package="JP7_RND" value="JP7ALL_ROUND"/>
<element name="J1" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PRG_6PTH"/>
<element name="U$4" library="Colin's Library" package="COLIN_7_5MM_GOLD" value=""/>
<element name="U$6" library="Colin's Library" package="ATMEL_7.5MM" value=""/>
<element name="U$5" library="Colin's Library" package="ATTINY841_7.5MM" value=""/>
</elements>
<signals>
<signal name="PA6">
<contactref element="U$1" pad="7"/>
<contactref element="U$2" pad="7"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="PA7">
<contactref element="U$1" pad="6"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="PB2">
<contactref element="U$1" pad="5"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="PB3">
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="4"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="PB0">
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="14"/>
<contactref element="U$3" pad="7"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="PA0">
<contactref element="U$1" pad="13"/>
<contactref element="U$3" pad="6"/>
</signal>
<signal name="PA1">
<contactref element="U$1" pad="12"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="PA2">
<contactref element="U$3" pad="4"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="PA3">
<contactref element="U$1" pad="10"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="PA4">
<contactref element="U$1" pad="9"/>
<contactref element="U$3" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="PA5">
<contactref element="U$1" pad="8"/>
<contactref element="U$3" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="PB1">
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
