<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>Programmer Shield v2.0.1
spark.io</text>
<hole x="59.69" y="35.56" drill="3.2"/>
<hole x="59.69" y="3.81" drill="3.2"/>
<hole x="3.81" y="3.81" drill="3.2"/>
<hole x="3.81" y="35.56" drill="3.2"/>
<wire x1="2.54" y1="0" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="36.83" x2="2.54" y2="39.37" width="0" layer="20"/>
<wire x1="63.5" y1="36.83" x2="60.96" y2="39.37" width="0" layer="20"/>
<wire x1="60.96" y1="0" x2="63.5" y2="2.54" width="0" layer="20"/>
<wire x1="2.54" y1="0" x2="60.96" y2="0" width="0" layer="20"/>
<wire x1="63.5" y1="2.54" x2="63.5" y2="36.83" width="0" layer="20"/>
<wire x1="2.54" y1="39.37" x2="60.96" y2="39.37" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="0" y2="36.83" width="0" layer="20"/>
<text>Reference Designs ARE PROVIDED "AS IS" AND "WITH ALL FAULTS. SPARK LABS, INC 
("SPARK") DISCLAIMS ALL OTHER WARRANTIES, EXPRESS OR IMPLIED, REGARDING 
PRODUCTS OR THE REFERENCE DESIGNS, INCLUDING BUT NOT LIMITED TO, ANY 
IMPLIED WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE,
OR NON-INFRINGEMENT.

Spark may make changes to specifications and product descriptions at any 
time, without notice. The Customer must not rely on the absence or 
characteristics of any features or instructions marked "reserved" or 
"undefined." Spark reserves these for future definition and shall have 
no responsibility whatsoever for conflicts or incompatibilities arising 
from future changes to them. The product information on the Web Site or 
Materials is subject to change without notice. Do not finalize a design 
with this information. 
Spark is a registered trademark.</text>
</plain>
<libraries>
<library name="con-harting-ml">
<packages>
<package name="ML20">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Spark">
<packages>
<package name="SPARK_LOGO_PLUS_PLANE">
</package>
<package name="SPARK_CORE_STACKABLE">
</package>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="con-harting-ml" package="ML20" value=""/>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.3" value="10K"/>
<element name="R6" library="SparkFun-Passives" package="AXIAL-0.3" value="10K"/>
<element name="R7" library="SparkFun-Passives" package="AXIAL-0.3" value="10K"/>
<element name="R8" library="SparkFun-Passives" package="AXIAL-0.3" value="10K"/>
<element name="E$1" library="Spark" package="SPARK_LOGO_PLUS_PLANE" value=""/>
<element name="U$1" library="Spark" package="SPARK_CORE_STACKABLE" value="SPARK_CORE"/>
<element name="LOGO1" library="Spark" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
</elements>
<signals>
<signal name="+3V3">
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="R8" pad="P$2"/>
<contactref element="U$1" pad="@24"/>
<contactref element="U$1" pad="24"/>
<contactref element="U$1" pad="#24"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="10"/>
<contactref element="J1" pad="12"/>
<contactref element="J1" pad="14"/>
<contactref element="J1" pad="16"/>
<contactref element="J1" pad="18"/>
<contactref element="J1" pad="20"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="U$1" pad="@2"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="@21"/>
<contactref element="U$1" pad="21"/>
<contactref element="U$1" pad="@2"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="@21"/>
<contactref element="U$1" pad="21"/>
<contactref element="U$1" pad="#21"/>
<contactref element="U$1" pad="#2"/>
</signal>
<signal name="N$13">
<contactref element="J1" pad="19"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="J1" pad="17"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="J1" pad="11"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="TRST">
<contactref element="J1" pad="3"/>
<contactref element="U$1" pad="16"/>
<contactref element="U$1" pad="@16"/>
<contactref element="U$1" pad="#16"/>
</signal>
<signal name="TDI">
<contactref element="J1" pad="5"/>
<contactref element="U$1" pad="@18"/>
<contactref element="U$1" pad="18"/>
<contactref element="U$1" pad="#18"/>
</signal>
<signal name="TMS">
<contactref element="J1" pad="7"/>
<contactref element="U$1" pad="20"/>
<contactref element="U$1" pad="@20"/>
<contactref element="U$1" pad="#20"/>
</signal>
<signal name="TCK">
<contactref element="J1" pad="9"/>
<contactref element="U$1" pad="@19"/>
<contactref element="U$1" pad="19"/>
<contactref element="U$1" pad="#19"/>
</signal>
<signal name="TDO">
<contactref element="J1" pad="13"/>
<contactref element="R8" pad="P$1"/>
<contactref element="U$1" pad="@17"/>
<contactref element="U$1" pad="17"/>
<contactref element="U$1" pad="#17"/>
</signal>
<signal name="!RST">
<contactref element="J1" pad="15"/>
<contactref element="U$1" pad="23"/>
<contactref element="U$1" pad="@23"/>
<contactref element="U$1" pad="#23"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="@1"/>
<contactref element="U$1" pad="#1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="@3"/>
<contactref element="U$1" pad="#3"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="@4"/>
<contactref element="U$1" pad="#4"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="@5"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="#5"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="@6"/>
<contactref element="U$1" pad="#6"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="7"/>
<contactref element="U$1" pad="@7"/>
<contactref element="U$1" pad="#7"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="@8"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$1" pad="#8"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="@9"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="#9"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="10"/>
<contactref element="U$1" pad="@10"/>
<contactref element="U$1" pad="#10"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="11"/>
<contactref element="U$1" pad="@11"/>
<contactref element="U$1" pad="#11"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="12"/>
<contactref element="U$1" pad="@12"/>
<contactref element="U$1" pad="#12"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="@13"/>
<contactref element="U$1" pad="13"/>
<contactref element="U$1" pad="#13"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="@14"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="#14"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="15"/>
<contactref element="U$1" pad="@15"/>
<contactref element="U$1" pad="#15"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="22"/>
<contactref element="U$1" pad="@22"/>
<contactref element="U$1" pad="#22"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
