<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="44.45" x2="45.39" y2="44.45" width="0" layer="20"/>
<wire x1="45.39" y1="44.45" x2="45.39" y2="80" width="0" layer="20"/>
<wire x1="45.39" y1="80" x2="2.54" y2="80" width="0" layer="20"/>
<wire x1="2.54" y1="80" x2="2.54" y2="44.45" width="0" layer="20"/>
<hole x="5.08" y="77.47" drill="3.2" locked="yes"/>
<hole x="41.91" y="77.47" drill="3.2" locked="yes"/>
<hole x="41.91" y="46.99" drill="3.2" locked="yes"/>
<hole x="5.08" y="46.99" drill="3.2" locked="yes"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X5-SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Teensy_3_and_LC_Series_Boards_v1.4">
<packages>
<package name="TEENSY_3.0-3.2&amp;LC_DIL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="2X5-SHROUDED" value="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="2X5-SHROUDED" value="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
</element>
<element name="U$1" library="Teensy_3_and_LC_Series_Boards_v1.4" package="TEENSY_3.0-3.2&amp;LC_DIL" value="TEENSY_3.1-3.2_DIL"/>
</elements>
<signals>
<signal name="AGND">
<contactref element="U$1" pad="AGND"/>
</signal>
<signal name="VIN">
<contactref element="U$1" pad="VIN"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="3.3V"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="3"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="4"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="7"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="8"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="9"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="10"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="J2" pad="1"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="N$10">
<contactref element="J2" pad="2"/>
<contactref element="U$1" pad="14/A0"/>
</signal>
<signal name="N$11">
<contactref element="J2" pad="3"/>
<contactref element="U$1" pad="15/A1"/>
</signal>
<signal name="N$12">
<contactref element="J2" pad="4"/>
<contactref element="U$1" pad="16/A2"/>
</signal>
<signal name="N$13">
<contactref element="J2" pad="7"/>
<contactref element="U$1" pad="17/A3"/>
</signal>
<signal name="N$14">
<contactref element="J2" pad="8"/>
<contactref element="U$1" pad="18/A4"/>
</signal>
<signal name="N$15">
<contactref element="J2" pad="9"/>
<contactref element="U$1" pad="19/A5"/>
</signal>
<signal name="N$16">
<contactref element="J2" pad="10"/>
<contactref element="U$1" pad="20/A6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
