<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<text>VCC</text>
<text>H</text>
<text>C</text>
<text>GND</text>
<text>DAT</text>
<text>VCC</text>
<text>GND</text>
<text>DOOR</text>
<text>GND</text>
<text>VCC</text>
<text>DAT</text>
<text>DAT</text>
<text>VCC</text>
<text>GND</text>
<text>DAT</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>C</text>
<text>H</text>
<text>VCC</text>
<text>ONE_WIRE</text>
<text>ONE_WIRE</text>
<text>ONE_WIRE</text>
<text>RELAY</text>
<text>DOOR</text>
<text>8</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>RJ45 Pinout:
1 -          5 - GND
2 -          6 - DOOR
3 - VCC    7 - COOL
4 - DATA  8 - HEAT</text>
<wire x1="29.337" y1="41.402" x2="-1.397" y2="41.402" width="0.0762" layer="20"/>
<wire x1="-1.397" y1="41.402" x2="-1.397" y2="91.059" width="0.0762" layer="20"/>
<wire x1="-1.397" y1="91.059" x2="29.337" y2="91.059" width="0.0762" layer="20"/>
<wire x1="29.337" y1="91.059" x2="29.337" y2="41.402" width="0.0762" layer="20"/>
<text>HEAT</text>
<text>COOL</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_3MM">
<description>&lt;h3&gt;LED 3MM PTH&lt;/h3&gt;

3 mm, round.

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-4">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
<package name="W237-103">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-tycoelectronics">
<description>&lt;b&gt;Tyco Electronics Connector&lt;/b&gt;&lt;p&gt;
http://catalog.tycoelectronics.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RJ45-NO-SHIELD">
<description>&lt;b&gt;RJ45 Low Profile&lt;/b&gt; No Shield&lt;p&gt;
For all RJ45 N and Z Series Models&lt;br&gt;
Source: www.tycoelectronics.com .. ENG_DS_1654001_1099_RJ_L_0507.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-LED" package="LED_3MM" value="HINV">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED_3MM" value="HNON">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED_3MM" value="CINV">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED_3MM" value="CNON">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="DOOR" library="SparkFun-Connectors" package="1X02" value="2-PIN"/>
<element name="ONE_WIRE2" library="SparkFun-Connectors" package="1X03" value="3-PIN">
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
<element name="ONE_WIRE1" library="SparkFun-Connectors" package="1X03" value="3-PIN">
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
<element name="ONE_WIRE3" library="SparkFun-Connectors" package="1X03" value="3-PIN">
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3" value="220Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3" value="220Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY" library="SparkFun-Connectors" package="1X04" value="4-PIN">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="RELAY_TERM" library="con-wago-500" package="W237-4" value="4TERM">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X2" library="con-wago-500" package="W237-102" value="4TERM">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
</element>
<element name="X3" library="con-wago-500" package="W237-103" value="3TERM">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-103"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="18M7116"/>
</element>
<element name="X1" library="con-tycoelectronics" package="RJ45-NO-SHIELD" value="RJ45-8X">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RJ45-8X"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6101"/>
</element>
<element name="X5" library="con-wago-500" package="W237-103" value="3TERM">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-103"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="18M7116"/>
</element>
<element name="X4" library="con-wago-500" package="W237-103" value="3TERM">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-103"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="18M7116"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="X1" pad="3"/>
<contactref element="RELAY_TERM" pad="4"/>
<contactref element="RELAY" pad="4"/>
<contactref element="D1" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="ONE_WIRE1" pad="2"/>
<contactref element="ONE_WIRE2" pad="2"/>
<contactref element="ONE_WIRE3" pad="2"/>
<contactref element="X5" pad="2"/>
<contactref element="X3" pad="2"/>
<contactref element="X4" pad="2"/>
</signal>
<signal name="DATA">
<contactref element="X1" pad="4"/>
<contactref element="ONE_WIRE1" pad="3"/>
<contactref element="ONE_WIRE2" pad="3"/>
<contactref element="ONE_WIRE3" pad="3"/>
<contactref element="X5" pad="1"/>
<contactref element="X3" pad="1"/>
<contactref element="X4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="5"/>
<contactref element="RELAY_TERM" pad="1"/>
<contactref element="RELAY" pad="1"/>
<contactref element="D2" pad="K"/>
<contactref element="D4" pad="K"/>
<contactref element="X2" pad="2"/>
<contactref element="DOOR" pad="1"/>
<contactref element="ONE_WIRE1" pad="1"/>
<contactref element="ONE_WIRE2" pad="1"/>
<contactref element="ONE_WIRE3" pad="1"/>
<contactref element="X5" pad="3"/>
<contactref element="X3" pad="3"/>
<contactref element="X4" pad="3"/>
</signal>
<signal name="DOOR">
<contactref element="X1" pad="6"/>
<contactref element="X2" pad="1"/>
<contactref element="DOOR" pad="2"/>
</signal>
<signal name="COOL">
<contactref element="X1" pad="7"/>
<contactref element="RELAY_TERM" pad="2"/>
<contactref element="RELAY" pad="2"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="HEAT">
<contactref element="X1" pad="8"/>
<contactref element="RELAY_TERM" pad="3"/>
<contactref element="RELAY" pad="3"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="K"/>
<contactref element="D2" pad="A"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="D3" pad="K"/>
<contactref element="D4" pad="A"/>
<contactref element="R2" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
