<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="19.812" y1="0" x2="0.635" y2="0" width="0" layer="20"/>
<wire x1="0.635" y1="0" x2="0" y2="0.635" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="0.635" x2="0" y2="14.859" width="0" layer="20"/>
<wire x1="40.005" y1="14.859" x2="40.005" y2="0.635" width="0" layer="20"/>
<wire x1="40.005" y1="0.635" x2="39.37" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="39.37" y1="0" x2="19.812" y2="0" width="0" layer="20"/>
<wire x1="0" y1="14.859" x2="0.635" y2="15.494" width="0" layer="20" curve="-90"/>
<wire x1="0.635" y1="15.494" x2="5.8674" y2="15.494" width="0" layer="20"/>
<wire x1="5.8674" y1="15.494" x2="6.5024" y2="14.859" width="0" layer="20" curve="-90"/>
<wire x1="6.5024" y1="14.859" x2="6.5024" y2="4.3942" width="0" layer="20"/>
<wire x1="6.5024" y1="4.3942" x2="7.7724" y2="3.1242" width="0" layer="20" curve="90"/>
<wire x1="7.7724" y1="3.1242" x2="32.2326" y2="3.1242" width="0" layer="20"/>
<wire x1="32.2326" y1="3.1242" x2="33.5026" y2="4.3942" width="0" layer="20" curve="90"/>
<wire x1="33.5026" y1="4.3942" x2="33.5026" y2="14.859" width="0" layer="20"/>
<wire x1="33.5026" y1="14.859" x2="34.1376" y2="15.494" width="0" layer="20" curve="-90"/>
<wire x1="34.1376" y1="15.494" x2="39.37" y2="15.494" width="0" layer="20"/>
<wire x1="39.37" y1="15.494" x2="40.005" y2="14.859" width="0" layer="20" curve="-90"/>
<text>D2</text>
<text>D1</text>
<text>R1</text>
<text>L+</text>
<text>L-</text>
<text>UNI-T_UT61E_
BKLT_0.1</text>
<text>L-</text>
<text>L+</text>
<text>R2</text>
<text>goo.gl/pAmFpu
20151124</text>
<wire x1="6.5024" y1="4.3942" x2="7.7724" y2="3.1242" width="0" layer="20" curve="90"/>
<text>UNI-T_UT61E_
BKLT_0.1</text>
<text>goo.gl/pAmFpu
20151124</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-1.5X4.5">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP2" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="LED+"/>
<element name="JP3" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="LED-"/>
<element name="LED1" library="SparkFun-LED" package="LED-1206" value=""/>
<element name="LED2" library="SparkFun-LED" package="LED-1206" value=""/>
<element name="R1" library="SparkFun-Passives" package="0805" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="LED+"/>
<element name="JP4" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="LED-"/>
<element name="R2" library="SparkFun-Passives" package="0805" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="JP2" pad="P$1"/>
<contactref element="JP1" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="JP3" pad="P$1"/>
<contactref element="JP4" pad="P$1"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
