<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.6024" y2="0" width="0" layer="20"/>
<wire x1="17.6024" y1="0" x2="17.6024" y2="12.436" width="0" layer="20"/>
<wire x1="17.6024" y1="12.436" x2="0" y2="12.436" width="0" layer="20"/>
<wire x1="0" y1="12.436" x2="0" y2="0" width="0" layer="20"/>
<text>RX2</text>
<text>TX2</text>
<text>RX2</text>
<text>TX2</text>
<text>TX1</text>
<text>TX1</text>
<text>RX1</text>
<text>RX1</text>
<text>VCC</text>
<text>GND</text>
<text>RX1</text>
<text>TX1</text>
<text>TX2</text>
<text>RX2</text>
<text>RX1</text>
<text>TX1</text>
<text>TX2</text>
<text>RX2</text>
<text>VCC</text>
<text>GND</text>
<text>LOGIC</text>
<text>RS-232</text>
</plain>
<libraries>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TSSOP16">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 16&lt;/b&gt;&lt;p&gt;
http://www.maxim-ic.com .. MAX3223-MAX3243.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MAX3232" library="maxim" package="TSSOP16" value="MAX3232CUE">
<attribute name="OC_NEWARK" value="68K4629"/>
<attribute name="MPN" value="MAX3232CUE+"/>
<attribute name="MF" value="MAXIM"/>
<attribute name="OC_FARNELL" value="1593350"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="MAX3232" pad="15"/>
<contactref element="C5" pad="2"/>
<contactref element="MAX3232" pad="15"/>
<contactref element="JP3" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="MAX3232" pad="6"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="MAX3232" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="MAX3232" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="MAX3232" pad="3"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="MAX3232" pad="4"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="MAX3232" pad="5"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="MAX3232" pad="16"/>
<contactref element="C5" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="TX1">
<contactref element="MAX3232" pad="11"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="TX2">
<contactref element="MAX3232" pad="10"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="RX1">
<contactref element="MAX3232" pad="12"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="RX2">
<contactref element="MAX3232" pad="9"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="RS_RX2">
<contactref element="MAX3232" pad="8"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="RS_RX1">
<contactref element="MAX3232" pad="13"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="RS_TX2">
<contactref element="MAX3232" pad="7"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="RS_TX1">
<contactref element="MAX3232" pad="14"/>
<contactref element="JP2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
