<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.3875" y2="0" width="0" layer="20"/>
<wire x1="25.3875" y1="0" x2="25.3875" y2="50.79" width="0" layer="20"/>
<wire x1="25.3875" y1="50.79" x2="0" y2="50.79" width="0" layer="20"/>
<wire x1="0" y1="50.79" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.81" y="3.81" drill="3.175"/>
<hole x="21.59" y="46.99" drill="3.175"/>
<hole x="3.81" y="46.99" drill="3.175"/>
<hole x="21.59" y="3.81" drill="3.175"/>
<text>VCC</text>
<text>IN</text>
<text>OUT</text>
<text>GND</text>
<text>NOT</text>
<text>GATE</text>
</plain>
<libraries>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35Z10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="diode" package="DO35Z10" value="1N821">
<attribute name="NAME"/>
</element>
<element name="D2" library="diode" package="DO35Z10" value="1N821">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3" value=""/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3" value=""/>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.3" value=""/>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.3" value=""/>
<element name="T1" library="transistor" package="TO92" value="BC547">
<attribute name="NAME"/>
</element>
<element name="T2" library="transistor" package="TO92" value="BC547">
<attribute name="NAME"/>
</element>
<element name="T3" library="transistor" package="TO92" value="BC547">
<attribute name="NAME"/>
</element>
<element name="T4" library="transistor" package="TO92" value="BC547">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP1" pad="1"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="4"/>
<contactref element="R4" pad="P$1"/>
<contactref element="T4" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="C"/>
<contactref element="T4" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="P$1"/>
<contactref element="T2" pad="3"/>
<contactref element="T3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="P$1"/>
<contactref element="T1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="T1" pad="3"/>
<contactref element="T2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="P$1"/>
<contactref element="T3" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="D2" pad="A"/>
<contactref element="T3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="C"/>
<contactref element="JP1" pad="2"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="T2" pad="1"/>
<contactref element="R4" pad="P$2"/>
<contactref element="T4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
