<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="3" y1="3" x2="24.86" y2="3" width="0" layer="20"/>
<wire x1="24.86" y1="3" x2="24.86" y2="42.5" width="0" layer="20"/>
<wire x1="24.86" y1="42.5" x2="3" y2="42.5" width="0" layer="20"/>
<wire x1="3" y1="42.5" x2="3" y2="3" width="0" layer="20"/>
<text>Orlando S. Hoilett
CalvaryEng, IICEPD
ADPD103 Breakout</text>
<text>INT</text>
<text>PDSO</text>
<text>DVDD</text>
<text>AGND</text>
<text>VREF</text>
<text>AVDD</text>
<text>PD1</text>
<text>PD2</text>
<text>PD3</text>
<text>PD4</text>
<text>PDC</text>
<text>PD5</text>
<text>PD6</text>
<text>PD7</text>
<text>PD8</text>
<text>NIC1</text>
<text>NIC2</text>
<text>NIC3</text>
<text>NIC4</text>
<text>NIC5</text>
<text>NIC6</text>
<text>NIC7</text>
<text>LEDX1</text>
<text>LEDX3</text>
<text>LEDX2</text>
<text>LGND</text>
<text>SCL</text>
<text>SDA</text>
<text>EPAD</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X14">
</package>
<package name="1X15">
</package>
</packages>
</library>
<library name="Orlando">
<packages>
<package name="28-LFCSP">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X14" value="M14"/>
<element name="U$1" library="Orlando" package="28-LFCSP" value="ADPD103">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X15" value="M15"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
</elements>
<signals>
<signal name="N$8">
<contactref element="U$1" pad="8"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="9"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="10"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="11"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="12"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="13"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="14"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="15"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="16"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="17"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="18"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="19"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="20"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="21"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="22"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="EPAD"/>
<contactref element="JP3" pad="15"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="28"/>
<contactref element="JP3" pad="14"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="27"/>
<contactref element="JP3" pad="13"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="26"/>
<contactref element="JP3" pad="12"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="25"/>
<contactref element="JP3" pad="11"/>
</signal>
<signal name="N$28">
<contactref element="U$1" pad="24"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="N$29">
<contactref element="U$1" pad="23"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="14"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="2"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="3"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="4"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="5"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="6"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="7"/>
<contactref element="JP1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
