<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="47.25" y1="10" x2="50.5" y2="10" width="0.154" layer="20"/>
<wire x1="-46.25" y1="10" x2="-49.5" y2="10" width="0.154" layer="20"/>
<wire x1="-49.5" y1="10" x2="-49.5" y2="26.5" width="0.154" layer="20"/>
<wire x1="50.5" y1="10" x2="50.5" y2="29.5" width="0.154" layer="20"/>
<wire x1="-49.5" y1="26.5" x2="-48" y2="26.5" width="0.154" layer="20"/>
<wire x1="50.5" y1="29.5" x2="49" y2="29.5" width="0.154" layer="20"/>
<wire x1="-48" y1="26.5" x2="-48" y2="32.5" width="0.154" layer="20"/>
<wire x1="-48" y1="32.5" x2="-44.5" y2="32.5" width="0.154" layer="20"/>
<wire x1="-44.5" y1="32.5" x2="-44.5" y2="34" width="0.154" layer="20"/>
<wire x1="49" y1="29.5" x2="49" y2="34" width="0.154" layer="20"/>
<wire x1="-44.5" y1="34" x2="49" y2="34" width="0.154" layer="20"/>
<text>27c128/256/512</text>
<text>27c128/256/512</text>
<text>PRG</text>
<text>CHR</text>
<text>H</text>
<text>V</text>
<text>NROM</text>
<text>AVRCIC</text>
</plain>
<libraries>
<library name="NES 72 Pin Cartridge Edge">
<packages>
<package name="NES_72-PIN_CONNECTOR">
<description>72-Pin Cartridge Edge Connector for NES Cartridges (Based on jero32 measurements)</description>
</package>
</packages>
</library>
<library name="microchip-3">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL28-6">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="DIL8">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
</packages>
</library>
<library name="3-Pin Jumper">
<packages>
<package name="3-PIN_JUMPER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$1" library="NES 72 Pin Cartridge Edge" package="NES_72-PIN_CONNECTOR" value=""/>
<element name="E$3" library="microchip-3" package="DIL28-6" value="">
<attribute name="VALUE"/>
</element>
<element name="E$2" library="microchip-3" package="DIL28-6" value="">
<attribute name="VALUE"/>
</element>
<element name="E$5" library="3-Pin Jumper" package="3-PIN_JUMPER" value=""/>
<element name="E$4" library="microchip-3" package="DIL8" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$2">
</signal>
<signal name="S$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
