<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="55.88" y1="53.34" x2="82.53" y2="53.34" width="0" layer="20"/>
<wire x1="82.53" y1="53.34" x2="82.53" y2="84.76" width="0" layer="20"/>
<wire x1="82.53" y1="84.76" x2="55.88" y2="84.76" width="0" layer="20"/>
<wire x1="55.88" y1="84.76" x2="55.88" y2="53.34" width="0" layer="20"/>
</plain>
<libraries>
<library name="Resistor">
<description>&lt;B&gt;Resistors, Potentiometers, TrimPot</description>
<packages>
<package name="PV36Z">
<description>PV36Z</description>
</package>
</packages>
</library>
<library name="IC_Linear">
<description>&lt;B&gt;Amplifiers, OpAmp, Comparators, Video-processing</description>
<packages>
<package name="DIP826W53P254L959H508Q8B">
<description>8-DIP, 2.54 mm (0.10 in) pitch, 8.26 mm (0.33 in) span, 9.59 X 6.35 X 5.08 mm body
&lt;p&gt;8-pin DIP package with 2.54 mm (0.10 in) pitch, 8.26 mm (0.33 in) span with body size 9.59 X 6.35 X 5.08 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C2.5-3">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 3 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="term-block-1725669">
<packages>
<package name="PHOENIX_1725669">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="Resistor" package="PV36Z" value="">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="DESCRIPTION" value="Lead Sealed Type Multiturn PV36 Series"/>
<attribute name="MANUFACTURER" value="BOURNS"/>
<attribute name="MPN" value="PV36Z"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMPERATURE" value=" -55 to +125 °C"/>
<attribute name="PART_STATUS" value="Active"/>
<attribute name="ROHS_COMPLIANCE" value="RoHS Compliant"/>
<attribute name="SERIES" value="PV36"/>
<attribute name="SUB-CATEGORY" value="Trimpot"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="Lead Sealed"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="IC_Linear" package="DIP826W53P254L959H508Q8B" value="LM393_DIP">
<attribute name="CATEGORY" value="Analog Comparators"/>
<attribute name="DESCRIPTION" value="Differential Dual Comparator"/>
<attribute name="MANUFACTURER" value="Generic"/>
<attribute name="MPN" value="Generic"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value="LM393"/>
<attribute name="SUB-CATEGORY" value="Comparator"/>
<attribute name="TYPE" value="Dual"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="term-block-1725669" package="PHOENIX_1725669" value="1725669">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 3 Position Wire to Board Terminal Block Horizontal with Board 0.100 (2.54mm) Through Hole "/>
<attribute name="MF" value="Phoenix Contact"/>
<attribute name="MP" value="1725669"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="capacitor-wima" package="C2.5-3" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="38"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="capacitor-wima" package="C2.5-3" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="38"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="term-block-1725669" package="PHOENIX_1725669" value="1725669">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 3 Position Wire to Board Terminal Block Horizontal with Board 0.100 (2.54mm) Through Hole "/>
<attribute name="MF" value="Phoenix Contact"/>
<attribute name="MP" value="1725669"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VS+">
<contactref element="R1" pad="3"/>
<contactref element="J1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="VREF">
<contactref element="IC1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="OUT2">
<contactref element="IC1" pad="7"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="OUT1">
<contactref element="IC1" pad="1"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="IN1">
<contactref element="IC1" pad="3"/>
<contactref element="J1" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="IN2">
<contactref element="IC1" pad="5"/>
</signal>
<signal name="0">
<contactref element="IC1" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
