<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="101.6" y2="0" width="0" layer="20"/>
<wire x1="101.6" y1="0" x2="101.6" y2="50.8" width="0" layer="20"/>
<wire x1="101.6" y1="50.8" x2="0" y2="50.8" width="0" layer="20"/>
<wire x1="0" y1="50.8" x2="0" y2="0" width="0" layer="20"/>
<text>+/-</text>
<text>GND</text>
<text>S4</text>
<text>S3</text>
<text>S2</text>
<text>S1</text>
<text>ON</text>
<text>+/-</text>
<text>S1</text>
<text>S2</text>
<text>S3</text>
<text>S4</text>
<text>Rocket 
Board
GNS
140104</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="2X4">
</package>
<package name="2X13">
</package>
<package name="1X05">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH-SPDT">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="transistors">
<packages>
<package name="TO220-ADJ">
<description>This is the sparkfun TO-220 package but completely vertical rather than bent</description>
</package>
</packages>
</library>
<library name="VoltageRegulators">
<packages>
<package name="TO220-ADJ">
<description>This is the standard sparkfun TO220 package but completely vertical rather than bent</description>
</package>
</packages>
</library>
<library name="Diodes">
<packages>
<package name="DIODE-SB540">
<description>footprint for Schotky Diode SB540-E3/54 Digikey Part #&lt;a href="http://www.digikey.com/product-detail/en/SB540-E3%2F54/SB540-E3%2F54GICT-ND/190378"&gt;SB540-E3/54GICT-ND&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH"/>
<element name="S1" library="SparkFun-Electromechanical" package="SWITCH-SPDT" value=""/>
<element name="PWR" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="7V" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="12V" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="STANDOFF1" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF3" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF4" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM"/>
<element name="JP2" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM"/>
<element name="JP3" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM"/>
<element name="JP4" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM"/>
<element name="7V_RAIL" library="SparkFun-Connectors" package="2X4" value="M04X2"/>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="1000"/>
<element name="R2_A" library="SparkFun-Resistors" package="AXIAL-0.3" value="1800"/>
<element name="R3_A" library="SparkFun-Resistors" package="AXIAL-0.3" value="3000"/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="400"/>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="750"/>
<element name="R_S1" library="SparkFun-Resistors" package="AXIAL-0.3" value="2200"/>
<element name="R_S2" library="SparkFun-Resistors" package="AXIAL-0.3" value="2200"/>
<element name="R_S3" library="SparkFun-Resistors" package="AXIAL-0.3" value="2200"/>
<element name="R_S4" library="SparkFun-Resistors" package="AXIAL-0.3" value="2200"/>
<element name="R3_O" library="SparkFun-Resistors" package="AXIAL-0.3" value="390"/>
<element name="R2_O" library="SparkFun-Resistors" package="AXIAL-0.3" value="380"/>
<element name="5V" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="400"/>
<element name="R1_O" library="SparkFun-Resistors" package="AXIAL-0.3" value="330"/>
<element name="R1.1_O" library="SparkFun-Resistors" package="AXIAL-0.3" value="7"/>
<element name="R1_A" library="SparkFun-Resistors" package="AXIAL-0.3" value="1000"/>
<element name="5V_RAIL" library="SparkFun-Connectors" package="2X13" value="M13X22X13"/>
<element name="TIP102_1" library="transistors" package="TO220-ADJ" value=""/>
<element name="TIP102_3" library="transistors" package="TO220-ADJ" value=""/>
<element name="TIP102_2" library="transistors" package="TO220-ADJ" value=""/>
<element name="TIP102_4" library="transistors" package="TO220-ADJ" value=""/>
<element name="VREG_1" library="VoltageRegulators" package="TO220-ADJ" value="5V"/>
<element name="VREG_2" library="VoltageRegulators" package="TO220-ADJ" value="7V"/>
<element name="VREG_3" library="VoltageRegulators" package="TO220-ADJ" value="12V"/>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="C4" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="C3" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="SOLENOID_CTRL" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="D-1" library="Diodes" package="DIODE-SB540" value="SCHOTTKY"/>
<element name="D_S1" library="Diodes" package="DIODE-SB540" value="SCHOTTKY"/>
<element name="D_S2" library="Diodes" package="DIODE-SB540" value="SCHOTTKY"/>
<element name="D_S3" library="Diodes" package="DIODE-SB540" value="SCHOTTKY"/>
<element name="D_S4" library="Diodes" package="DIODE-SB540" value="SCHOTTKY"/>
</elements>
<signals>
<signal name="3.3V">
<contactref element="J1" pad="GND"/>
<contactref element="7V_RAIL" pad="8"/>
<contactref element="7V_RAIL" pad="6"/>
<contactref element="7V_RAIL" pad="4"/>
<contactref element="7V_RAIL" pad="2"/>
<contactref element="R5" pad="P$1"/>
<contactref element="R2_A" pad="P$2"/>
<contactref element="R3_A" pad="P$2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R1_A" pad="P$1"/>
<contactref element="5V_RAIL" pad="20"/>
<contactref element="5V_RAIL" pad="26"/>
<contactref element="5V_RAIL" pad="24"/>
<contactref element="5V_RAIL" pad="22"/>
<contactref element="5V_RAIL" pad="18"/>
<contactref element="5V_RAIL" pad="16"/>
<contactref element="5V_RAIL" pad="14"/>
<contactref element="5V_RAIL" pad="12"/>
<contactref element="5V_RAIL" pad="10"/>
<contactref element="5V_RAIL" pad="8"/>
<contactref element="5V_RAIL" pad="6"/>
<contactref element="5V_RAIL" pad="4"/>
<contactref element="5V_RAIL" pad="2"/>
<contactref element="TIP102_1" pad="EMITTER"/>
<contactref element="TIP102_2" pad="EMITTER"/>
<contactref element="TIP102_3" pad="EMITTER"/>
<contactref element="TIP102_4" pad="EMITTER"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="SOLENOID_CTRL" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="S1" pad="2"/>
<contactref element="PWR" pad="A"/>
<contactref element="VREG_1" pad="IN"/>
<contactref element="VREG_2" pad="IN"/>
<contactref element="VREG_3" pad="IN"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R2_A" pad="P$1"/>
<contactref element="VREG_2" pad="ADJ"/>
<contactref element="R2_O" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="R3_A" pad="P$1"/>
<contactref element="VREG_3" pad="ADJ"/>
<contactref element="R3_O" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="R_S1" pad="P$2"/>
<contactref element="TIP102_1" pad="BASE"/>
</signal>
<signal name="12V">
<contactref element="12V" pad="A"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="R3_O" pad="P$2"/>
<contactref element="VREG_3" pad="OUT"/>
<contactref element="C4" pad="1"/>
<contactref element="D_S1" pad="C"/>
<contactref element="D_S2" pad="C"/>
<contactref element="D_S3" pad="C"/>
<contactref element="D_S4" pad="C"/>
</signal>
<signal name="S1-">
<contactref element="JP1" pad="2"/>
<contactref element="TIP102_1" pad="COLLECTOR"/>
<contactref element="D_S1" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="R_S2" pad="P$2"/>
<contactref element="TIP102_2" pad="BASE"/>
</signal>
<signal name="S1-1">
<contactref element="JP2" pad="2"/>
<contactref element="TIP102_2" pad="COLLECTOR"/>
<contactref element="D_S2" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="R_S3" pad="P$2"/>
<contactref element="TIP102_3" pad="BASE"/>
</signal>
<signal name="S1-2">
<contactref element="JP3" pad="2"/>
<contactref element="TIP102_3" pad="COLLECTOR"/>
<contactref element="D_S3" pad="A"/>
</signal>
<signal name="N$23">
<contactref element="R_S4" pad="P$2"/>
<contactref element="TIP102_4" pad="BASE"/>
</signal>
<signal name="S1-3">
<contactref element="JP4" pad="2"/>
<contactref element="TIP102_4" pad="COLLECTOR"/>
<contactref element="D_S4" pad="A"/>
</signal>
<signal name="SCTRL1">
<contactref element="R_S1" pad="P$1"/>
<contactref element="SOLENOID_CTRL" pad="1"/>
</signal>
<signal name="SCTRL2">
<contactref element="R_S2" pad="P$1"/>
<contactref element="SOLENOID_CTRL" pad="2"/>
</signal>
<signal name="SCTRL3">
<contactref element="R_S3" pad="P$1"/>
<contactref element="SOLENOID_CTRL" pad="3"/>
</signal>
<signal name="SCTRL4">
<contactref element="R_S4" pad="P$1"/>
<contactref element="SOLENOID_CTRL" pad="4"/>
</signal>
<signal name="7V">
<contactref element="7V_RAIL" pad="1"/>
<contactref element="7V_RAIL" pad="3"/>
<contactref element="7V_RAIL" pad="5"/>
<contactref element="7V_RAIL" pad="7"/>
<contactref element="7V" pad="A"/>
<contactref element="R2_O" pad="P$2"/>
<contactref element="VREG_2" pad="OUT"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="S1" pad="3"/>
<contactref element="D-1" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="PWR"/>
<contactref element="D-1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="PWR" pad="K"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="7V" pad="K"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$12">
<contactref element="12V" pad="K"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="5V">
<contactref element="5V" pad="A"/>
<contactref element="R1_O" pad="P$1"/>
<contactref element="5V_RAIL" pad="1"/>
<contactref element="5V_RAIL" pad="3"/>
<contactref element="5V_RAIL" pad="5"/>
<contactref element="5V_RAIL" pad="7"/>
<contactref element="5V_RAIL" pad="9"/>
<contactref element="5V_RAIL" pad="11"/>
<contactref element="5V_RAIL" pad="13"/>
<contactref element="5V_RAIL" pad="15"/>
<contactref element="5V_RAIL" pad="17"/>
<contactref element="5V_RAIL" pad="19"/>
<contactref element="5V_RAIL" pad="21"/>
<contactref element="5V_RAIL" pad="23"/>
<contactref element="5V_RAIL" pad="25"/>
<contactref element="VREG_1" pad="OUT"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="5V" pad="K"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$21">
<contactref element="R1_O" pad="P$2"/>
<contactref element="R1.1_O" pad="P$1"/>
</signal>
<signal name="N$22">
<contactref element="R1.1_O" pad="P$2"/>
<contactref element="R1_A" pad="P$2"/>
<contactref element="VREG_1" pad="ADJ"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
