<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<polygon width="0.4064" layer="20">
<vertex x="39.793" y="52.7045"/>
<vertex x="43.73" y="52.7045"/>
<vertex x="43.73" y="29.2265"/>
<vertex x="39.793" y="29.2265"/>
</polygon>
<text>CUT OUT</text>
<text>REV 3</text>
<text>Squats &amp; Science</text>
<text>OpenBarbell V0.31</text>
<wire x1="1.181" y1="27.408" x2="49.1074" y2="27.1414" width="0" layer="20" curve="93.072955"/>
<text>VREG</text>
<text>STEP-UP</text>
<wire x1="1.181" y1="27.408" x2="1.181" y2="28.819" width="0" layer="20"/>
<wire x1="1.181" y1="28.819" x2="0" y2="30" width="0" layer="20" curve="90"/>
<wire x1="0" y1="30" x2="-3" y2="33" width="0" layer="20" curve="-90"/>
<wire x1="-3" y1="33" x2="0" y2="36" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="36" x2="1" y2="37" width="0" layer="20" curve="90"/>
<wire x1="1" y1="37" x2="1" y2="61" width="0" layer="20"/>
<wire x1="1" y1="61" x2="0" y2="62" width="0" layer="20" curve="90"/>
<wire x1="0" y1="62" x2="-3" y2="65" width="0" layer="20" curve="-90"/>
<wire x1="-3" y1="65" x2="0" y2="68" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="68" x2="1" y2="69" width="0" layer="20" curve="90"/>
<wire x1="1" y1="69" x2="1" y2="72" width="0" layer="20"/>
<wire x1="49.1074" y1="27.1414" x2="49.106" y2="28.553" width="0" layer="20"/>
<wire x1="49.106" y1="28.553" x2="50.287" y2="29.734" width="0" layer="20" curve="-90"/>
<wire x1="50.287" y1="29.734" x2="53.287" y2="32.734" width="0" layer="20" curve="90"/>
<wire x1="53.287" y1="32.734" x2="50.287" y2="35.734" width="0" layer="20" curve="90"/>
<wire x1="50.287" y1="35.734" x2="49.287" y2="36.734" width="0" layer="20" curve="-90"/>
<wire x1="49.287" y1="36.734" x2="49.287" y2="60.734" width="0" layer="20"/>
<wire x1="49.287" y1="60.734" x2="50.287" y2="61.734" width="0" layer="20" curve="-90"/>
<wire x1="50.287" y1="61.734" x2="53.287" y2="64.734" width="0" layer="20" curve="90"/>
<wire x1="53.287" y1="64.734" x2="50.287" y2="67.734" width="0" layer="20" curve="90"/>
<wire x1="50.287" y1="67.734" x2="49.287" y2="68.734" width="0" layer="20" curve="-90"/>
<wire x1="49.287" y1="68.734" x2="49.29" y2="71.97" width="0" layer="20"/>
<wire x1="1" y1="72" x2="19.32" y2="80.96" width="0" layer="20" curve="-33.680851"/>
<wire x1="49.29" y1="71.97" x2="31.34" y2="80.96" width="0" layer="20" curve="33.680851"/>
<wire x1="19.32" y1="80.96" x2="19.4" y2="80.96" width="0" layer="20"/>
<wire x1="19.4" y1="80.96" x2="20.38" y2="81.94" width="0" layer="20" curve="90"/>
<wire x1="20.38" y1="81.94" x2="21.1" y2="82.66" width="0" layer="20" curve="-90"/>
<wire x1="29.57" y1="82.66" x2="21.1" y2="82.66" width="0" layer="20"/>
<wire x1="30.29" y1="81.94" x2="29.57" y2="82.66" width="0" layer="20" curve="90"/>
<wire x1="31.34" y1="80.96" x2="30.29" y2="81.94" width="0" layer="20" curve="-90"/>
<circle x="25.38" y="74.2116" radius="1.488" width="0" layer="20"/>
<circle x="-0.32" y="65.0016" radius="1.488" width="0" layer="20"/>
<circle x="-0.34" y="32.9916" radius="1.488" width="0" layer="20"/>
<circle x="25.4" y="19.9016" radius="1.488" width="0" layer="20"/>
<circle x="50.59" y="32.7316" radius="1.488" width="0" layer="20"/>
<circle x="50.62" y="64.7416" radius="1.488" width="0" layer="20"/>
<circle x="37.9428" y="29.9796" radius="1" width="0" layer="20"/>
<polygon width="0.4064" layer="46">
<vertex x="39.793" y="52.7045"/>
<vertex x="43.73" y="52.7045"/>
<vertex x="43.73" y="29.2265"/>
<vertex x="39.793" y="29.2265"/>
</polygon>
</plain>
<libraries>
<library name="OpenBarbell 1x4">
<packages>
<package name="1X03-CLEANBIG">
</package>
</packages>
</library>
<library name="GeekAmmo">
<description>&lt;h3&gt;GeekAmmo  Library&lt;/h3&gt;

These are parts used by the GeekAmmo company (now part of SparkFun Electronics)!

 If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RFD22301">
<description>&lt;b&gt;RFD22301 Core of RFDuino&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TDFN-8">
<description>TDFN - 8pin, 2mmx3mm</description>
</package>
</packages>
</library>
<library name="NCP1402_5V_step-up-v10">
<description>Generated from &lt;b&gt;NCP1402_5V_step-up-v10.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="SPARKFUN_SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SPARKFUN_OSHW-LOGO-L">
</package>
<package name="SPARKFUN_EIA3528">
</package>
<package name="SPARKFUN_CR54">
</package>
</packages>
</library>
<library name="LiPo-Shield-v13">
<description>Generated from &lt;b&gt;LiPo-Shield-v13.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="SPARKFUN_JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="SPARKFUN_SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="SOD-123">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-B-MICRO-SMD_V03">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH-SPDT-SMD">
</package>
</packages>
</library>
<library name="USB3131-30-0230-A">
<packages>
<package name="USB-MICRO-B-VERTICAL-SMD">
</package>
</packages>
</library>
<library name="20151206_2341_OpenBarbellSwitches">
<packages>
<package name="MOM_">
</package>
<package name="SPDT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="GeekAmmo" package="RFD22301" value="RF22301">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="OLED" library="OpenBarbell 1x4" package="1X03-CLEANBIG" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-PowerIC" package="TDFN-8" value="MAX1704X">
<attribute name="PROD-ID" value="IC-10399"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="IC1" library="NCP1402_5V_step-up-v10" package="SPARKFUN_SOT23-5" value="">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="45J1846"/>
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="NCP1402SN33T1G"/>
</element>
<element name="U$4" library="NCP1402_5V_step-up-v10" package="SPARKFUN_OSHW-LOGO-L" value="SPARKFUN_OSHW-LOGOL">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="C2" library="NCP1402_5V_step-up-v10" package="SPARKFUN_EIA3528" value="68uF">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="94W4852"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="T520B686M006ATE025"/>
</element>
<element name="L1" library="NCP1402_5V_step-up-v10" package="SPARKFUN_CR54" value="47uH">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="14T0991"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="SRF1280-470M"/>
</element>
<element name="JP2" library="LiPo-Shield-v13" package="SPARKFUN_JST-2-SMD" value="">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="38K8067"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="S2B-PH-SM4-TB(LF)(SN)"/>
</element>
<element name="U1" library="LiPo-Shield-v13" package="SPARKFUN_SOT23-5" value="SPARKFUN_MCP73831">
<attribute name="OC_NEWARK" value="84R6271"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCP73831T-2DCI/OT"/>
</element>
<element name="U3" library="LiPo-Shield-v13" package="SPARKFUN_SOT23-5" value="SPARKFUN_V_REG_LDOSMD">
<attribute name="OC_NEWARK" value="26R6805"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MIC5205-3.3YM5 TR"/>
</element>
<element name="R2" library="adafruit" package="R0805" value="2k">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="01N7037"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCHP05W4F4701T5E"/>
</element>
<element name="R4" library="adafruit" package="R0805" value="100">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="01N7024"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCHP05W4F3300T5E"/>
</element>
<element name="R6" library="adafruit" package="R0805" value="4.7k">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="01N7037"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCHP05W4F4701T5E"/>
</element>
<element name="R5" library="adafruit" package="R0805" value="1k">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="28K0916"/>
<attribute name="MF" value="OUTSOURCE ITEM"/>
<attribute name="MPN" value="RR1220P-102-D"/>
</element>
<element name="R8" library="adafruit" package="R0805" value="100">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="01N7024"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCHP05W4F3300T5E"/>
</element>
<element name="R9" library="adafruit" package="R0805" value="10k">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="01N6989"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCHP05W4F1002T5E"/>
</element>
<element name="R7" library="adafruit" package="R0805" value="10k">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="01N6989"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCHP05W4F1002T5E"/>
</element>
<element name="C8" library="adafruit" package="C0805" value="1uF">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="64K2895"/>
<attribute name="MF" value="KEMET"/>
<attribute name="MPN" value="C0805C105M4VACTU"/>
</element>
<element name="C3" library="adafruit" package="C0805" value="10nF">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="06R3737"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MC0805B103M500CT"/>
</element>
<element name="C4" library="adafruit" package="C0805" value="0.1uF">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="06R3744"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MC0805B104M160CT"/>
</element>
<element name="C9" library="adafruit" package="C0805" value="1nF">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="33R0628"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MC0805B102K101CT"/>
</element>
<element name="LED3" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="14N9384"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCL034SBLC"/>
</element>
<element name="ENCODER" library="OpenBarbell 1x4" package="1X03-CLEANBIG" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="adafruit" package="R0805" value="600">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="89R3122"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MMZ2012S601A"/>
</element>
<element name="V+" library="adafruit" package="1X01" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="adafruit" package="1X01" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="USB-B-MICRO-SMD_V03" value="">
<attribute name="PROD_ID" value="CONN-11752"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="DIODE" library="adafruit" package="SOD-123" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="GRN" library="led" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="RED" library="led" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="S3" library="SparkFun-Electromechanical" package="SWITCH-SPDT-SMD" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="JUST4PADS" library="LiPo-Shield-v13" package="SPARKFUN_JST-2-SMD" value="">
<attribute name="MPN" value="S2B-PH-SM4-TB(LF)(SN)"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="OC_NEWARK" value="38K8067"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="adafruit" package="C0805" value="4.7uF">
<attribute name="MPN" value="MC0805B102K101CT"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="33R0628"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C0805" value="4.7uF">
<attribute name="MPN" value="MC0805B102K101CT"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="33R0628"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="adafruit" package="C0805" value="10uF">
<attribute name="MPN" value="MC0805B102K101CT"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="33R0628"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="adafruit" package="C0805" value="10uF">
<attribute name="MPN" value="MC0805B102K101CT"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="33R0628"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C0805" value="10uF">
<attribute name="MPN" value="MC0805B102K101CT"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="33R0628"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="USB3131-30-0230-A" package="USB-MICRO-B-VERTICAL-SMD" value="USB-MICRO-B-VERTICAL_SMD"/>
<element name="U$1" library="20151206_2341_OpenBarbellSwitches" package="MOM_" value="MOM_OB">
<attribute name="VALUE"/>
</element>
<element name="U$5" library="20151206_2341_OpenBarbellSwitches" package="MOM_" value="MOM_OB">
<attribute name="VALUE"/>
</element>
<element name="U$6" library="20151206_2341_OpenBarbellSwitches" package="SPDT" value="SPDT">
<attribute name="VALUE"/>
</element>
<element name="U$7" library="20151206_2341_OpenBarbellSwitches" package="MOM_" value="MOM_OB">
<attribute name="VALUE"/>
</element>
<element name="U$8" library="20151206_2341_OpenBarbellSwitches" package="MOM_" value="MOM_OB">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="C2" pad="C"/>
<contactref element="OLED" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="EP"/>
<contactref element="JP2" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="LED3" pad="K"/>
<contactref element="ENCODER" pad="2"/>
<contactref element="GND" pad="1"/>
<contactref element="JP4" pad="GND1"/>
<contactref element="GRN" pad="C"/>
<contactref element="S3" pad="3"/>
<contactref element="JUST4PADS" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U$3" pad="GND"/>
<contactref element="U$6" pad="SW3"/>
</signal>
<signal name="TACH">
<contactref element="U$2" pad="5"/>
<contactref element="ENCODER" pad="1"/>
</signal>
<signal name="DIR">
<contactref element="U$2" pad="4"/>
<contactref element="ENCODER" pad="4"/>
</signal>
<signal name="GND3">
<contactref element="U$2" pad="2"/>
</signal>
<signal name="GND4">
<contactref element="U$2" pad="8"/>
</signal>
<signal name="GND6">
<contactref element="U$2" pad="18"/>
</signal>
<signal name="GND7">
<contactref element="U$2" pad="19"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="5"/>
<contactref element="L1" pad="P$2"/>
<contactref element="DIODE" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="6"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="U2" pad="8"/>
<contactref element="U$2" pad="7"/>
<contactref element="OLED" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="U2" pad="7"/>
<contactref element="U$2" pad="6"/>
<contactref element="OLED" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U2" pad="3"/>
<contactref element="U3" pad="5"/>
<contactref element="C3" pad="1"/>
<contactref element="L1" pad="P$1"/>
<contactref element="U$2" pad="13"/>
<contactref element="C4" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$5" pad="T4"/>
<contactref element="U$7" pad="T4"/>
<contactref element="U$1" pad="T4"/>
<contactref element="U$8" pad="T4"/>
</signal>
<signal name="12345">
<contactref element="JP2" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="U3" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="V+" pad="1"/>
<contactref element="S3" pad="1"/>
<contactref element="JUST4PADS" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="U$6" pad="SW1"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="4"/>
<contactref element="JP4" pad="VBUS1"/>
<contactref element="RED" pad="A"/>
<contactref element="C5" pad="1"/>
<contactref element="U$3" pad="VCC"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="1"/>
<contactref element="RED" pad="C"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R8" pad="2"/>
<contactref element="GRN" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="U3" pad="3"/>
<contactref element="S3" pad="2"/>
<contactref element="U$6" pad="SW2"/>
</signal>
<signal name="GND5">
<contactref element="U$2" pad="9"/>
<contactref element="U$2" pad="10"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="N$6">
<contactref element="R10" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$21">
</signal>
<signal name="5V">
<contactref element="C2" pad="A"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="OLED" pad="2"/>
<contactref element="ENCODER" pad="3"/>
<contactref element="R10" pad="2"/>
<contactref element="DIODE" pad="C"/>
</signal>
<signal name="N$13">
<contactref element="U$2" pad="3"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="JP4" pad="ID1"/>
<contactref element="U$2" pad="14"/>
<contactref element="U$3" pad="ID"/>
</signal>
<signal name="N$16">
<contactref element="JP4" pad="D+1"/>
<contactref element="U$2" pad="16"/>
<contactref element="R7" pad="2"/>
<contactref element="U$3" pad="D+"/>
<contactref element="U$5" pad="T2"/>
<contactref element="U$7" pad="T2"/>
</signal>
<signal name="N$17">
<contactref element="JP4" pad="D-1"/>
<contactref element="R9" pad="2"/>
<contactref element="U$2" pad="17"/>
<contactref element="U$3" pad="D-"/>
<contactref element="U$1" pad="T2"/>
<contactref element="U$8" pad="T2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
