<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="15.875" y1="27.14625" x2="0.17875" y2="27.14625" width="0" layer="20"/>
<wire x1="0.17875" y1="27.14625" x2="0.17875" y2="0.33" width="0" layer="20"/>
<wire x1="0.17875" y1="0.33" x2="15.875" y2="0.33" width="0" layer="20"/>
<wire x1="15.875" y1="0.33" x2="15.875" y2="27.14625" width="0" layer="20"/>
<text>David DeFilippis
Nov. 2018
Micro SD V1.1</text>
<text>David DeFilippis
Nov. 2018
Micro SD V1.1</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="MICROSD">
</package>
</packages>
</library>
<library name="MCP1700T-3302E_TT">
<packages>
<package name="SOT95P237X112-3N">
</package>
</packages>
</library>
<library name="CD74HC4050PWR">
<packages>
<package name="PW16">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE"/>
</element>
<element name="SS___MOSI__MISO__CLK__GND__VIN" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="680">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08474"/>
<attribute name="VALUE"/>
</element>
<element name="MICRO_SD" library="adafruit" package="MICROSD" value="MICROSD">
<attribute name="NAME"/>
</element>
<element name="U2" library="MCP1700T-3302E_TT" package="SOT95P237X112-3N" value="MCP1700-3302">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" MCP1700 Series 250 mA 3.3 V Fixed Output LDO Voltage Regulator - SOT-23 "/>
<attribute name="MF" value="Microchip"/>
<attribute name="MP" value="MCP1700T-3302E/TT"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-3 Microchip"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="CD74HC4050" library="CD74HC4050PWR" package="PW16" value="CD74HC4050PWR">
<attribute name="MANUFACTURER_PART_NUMBER" value="CD74HC4050PWR"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Vendor"/>
</element>
<element name="D1" library="led" package="SML0805" value="&gt;|">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VIN">
<contactref element="SS___MOSI__MISO__CLK__GND__VIN" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="SS___MOSI__MISO__CLK__GND__VIN" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="CD74HC4050" pad="8"/>
<contactref element="MICRO_SD" pad="6"/>
<contactref element="MICRO_SD" pad="MT2"/>
<contactref element="MICRO_SD" pad="MT1"/>
<contactref element="CD74HC4050" pad="11"/>
<contactref element="CD74HC4050" pad="14"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="CD74HC4050" pad="1"/>
<contactref element="MICRO_SD" pad="4"/>
</signal>
<signal name="CLK">
<contactref element="SS___MOSI__MISO__CLK__GND__VIN" pad="3"/>
<contactref element="CD74HC4050" pad="3"/>
<contactref element="CD74HC4050" pad="9"/>
</signal>
<signal name="MISO1">
<contactref element="SS___MOSI__MISO__CLK__GND__VIN" pad="4"/>
<contactref element="MICRO_SD" pad="7"/>
</signal>
<signal name="MOSI1">
<contactref element="SS___MOSI__MISO__CLK__GND__VIN" pad="5"/>
<contactref element="CD74HC4050" pad="5"/>
</signal>
<signal name="SS1">
<contactref element="SS___MOSI__MISO__CLK__GND__VIN" pad="6"/>
<contactref element="CD74HC4050" pad="7"/>
</signal>
<signal name="SCLK2">
<contactref element="MICRO_SD" pad="5"/>
<contactref element="CD74HC4050" pad="2"/>
</signal>
<signal name="MOSI2">
<contactref element="MICRO_SD" pad="3"/>
<contactref element="CD74HC4050" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="CD74HC4050" pad="10"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="SS2">
<contactref element="MICRO_SD" pad="2"/>
<contactref element="CD74HC4050" pad="6"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
