<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="105.39" y2="0" width="0" layer="20"/>
<wire x1="105.39" y1="0" x2="105.39" y2="98.73" width="0" layer="20"/>
<wire x1="105.39" y1="98.73" x2="0" y2="98.73" width="0" layer="20"/>
<wire x1="0" y1="98.73" x2="0" y2="0" width="0" layer="20"/>
<hole x="5.08" y="22.86" drill="3.048"/>
<hole x="99.695" y="22.86" drill="3.048"/>
<hole x="5.08" y="93.98" drill="3.048"/>
<hole x="99.695" y="93.98" drill="3.048"/>
<text>TEC1</text>
<text>TEC2</text>
<text>I2C
3.3V</text>
<text>I2C
GND</text>
<text>I2C
SDA</text>
<text>I2C
SCL</text>
<text>optX imaging systems</text>
<text>PN: 170091081-01</text>
</plain>
<libraries>
<library name="5787082-2">
<description>&lt;0.050 Receptacle,r/a,PCB,26way&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="57870822">
<description>&lt;b&gt;5787082-2-10&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="684M5W5103L461">
<description>&lt;D-Sub Mixed Contact Connectors STD POWER-D 5W5 40A R/A MALE&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="684M5W5103L461">
<description>&lt;b&gt;684M5W5103L461-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="350209-1">
<description>&lt;02P CMNL HDR ASSY PC NATL&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="3502091">
<description>&lt;b&gt;350209-1-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="0855135013">
<description>&lt;Conn RJ-45 F 8 POS 1.27mm Solder ST SMD 8 Terminal 1 Port Cat 3 T/R&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="0855135013">
<description>&lt;b&gt;0855135013-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="501940-0403">
<description>&lt;Headers &amp; Wire Housings 1mm PicoClasp SMT SR 4CKT VRT HDR GLD PLT&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="5019400403">
<description>&lt;b&gt;501940-0403-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="1X09_ROUND_70">
</package>
</packages>
</library>
<library name="UJ2-AV-4-SMT-TR">
<description>&lt;USB Connectors USB Jack 2.0 A type 4pin Vert SMT&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="UJ2AV4SMTTR">
<description>&lt;b&gt;UJ2-AV-4-SMT-TR-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X20_SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x20 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Dev/RaspberryPi/B-D-xx1X.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="DSUB-SIGNAL" library="5787082-2" package="57870822" value="5787082-2">
<attribute name="ARROW_PART_NUMBER" value="5787082-2"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/5787082-2/te-connectivity"/>
<attribute name="DESCRIPTION" value="0.050 Receptacle,r/a,PCB,26way"/>
<attribute name="HEIGHT" value="10.44mm"/>
<attribute name="MANUFACTURER_NAME" value="TE Connectivity"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="5787082-2"/>
<attribute name="MOUSER_PART_NUMBER" value="571-5787082-2"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=571-5787082-2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DSUB-POWER" library="684M5W5103L461" package="684M5W5103L461" value="684M5W5103L461">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="D-Sub Mixed Contact Connectors STD POWER-D 5W5 40A R/A MALE"/>
<attribute name="HEIGHT" value="12.75mm"/>
<attribute name="MANUFACTURER_NAME" value="NorComp"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="684M5W5103L461"/>
<attribute name="MOUSER_PART_NUMBER" value="636-684M5W5103L461"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/NorComp/684M5W5103L461?qs=ih500mUifaX5K3Ch3GkspA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER-1" library="350209-1" package="3502091" value="350209-1">
<attribute name="ARROW_PART_NUMBER" value="350209-1"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/350209-1/te-connectivity"/>
<attribute name="DESCRIPTION" value="02P CMNL HDR ASSY PC NATL"/>
<attribute name="HEIGHT" value="9.52mm"/>
<attribute name="MANUFACTURER_NAME" value="TE Connectivity"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="350209-1"/>
<attribute name="MOUSER_PART_NUMBER" value="571-3502091"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/TE-Connectivity/350209-1?qs=wtYpWE7xRjlBq8XX7XRt4g%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER-2" library="350209-1" package="3502091" value="350209-1">
<attribute name="ARROW_PART_NUMBER" value="350209-1"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/350209-1/te-connectivity"/>
<attribute name="DESCRIPTION" value="02P CMNL HDR ASSY PC NATL"/>
<attribute name="HEIGHT" value="9.52mm"/>
<attribute name="MANUFACTURER_NAME" value="TE Connectivity"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="350209-1"/>
<attribute name="MOUSER_PART_NUMBER" value="571-3502091"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/TE-Connectivity/350209-1?qs=wtYpWE7xRjlBq8XX7XRt4g%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RJ45" library="0855135013" package="0855135013" value="0855135013">
<attribute name="ARROW_PART_NUMBER" value="0855135013"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/0855135013/molex?region=nac"/>
<attribute name="DESCRIPTION" value="Conn RJ-45 F 8 POS 1.27mm Solder ST SMD 8 Terminal 1 Port Cat 3 T/R"/>
<attribute name="HEIGHT" value="12.85mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="0855135013"/>
<attribute name="MOUSER_PART_NUMBER" value="N/A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Molex/0855135013?qs=PBcRNPEHKsqqBdjWJUBeEw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C-3" library="501940-0403" package="5019400403" value="501940-0403">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="Headers &amp; Wire Housings 1mm PicoClasp SMT SR 4CKT VRT HDR GLD PLT"/>
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="501940-0403"/>
<attribute name="MOUSER_PART_NUMBER" value="538-501940-0403"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Molex/501940-0403?qs=5aG0NVq1C4zjiDr4N5g%252Bxw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C-2" library="501940-0403" package="5019400403" value="501940-0403">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="Headers &amp; Wire Housings 1mm PicoClasp SMT SR 4CKT VRT HDR GLD PLT"/>
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="501940-0403"/>
<attribute name="MOUSER_PART_NUMBER" value="538-501940-0403"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Molex/501940-0403?qs=5aG0NVq1C4zjiDr4N5g%252Bxw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C-1" library="501940-0403" package="5019400403" value="501940-0403">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="Headers &amp; Wire Housings 1mm PicoClasp SMT SR 4CKT VRT HDR GLD PLT"/>
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="501940-0403"/>
<attribute name="MOUSER_PART_NUMBER" value="538-501940-0403"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Molex/501940-0403?qs=5aG0NVq1C4zjiDr4N5g%252Bxw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GPS" library="microbuilder" package="1X09_ROUND_70" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB-2" library="UJ2-AV-4-SMT-TR" package="UJ2AV4SMTTR" value="UJ2-AV-4-SMT-TR">
<attribute name="ARROW_PART_NUMBER" value="UJ2-AV-4-SMT-TR"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/uj2-av-4-smt-tr/cui-devices?region=nac"/>
<attribute name="DESCRIPTION" value="USB Connectors USB Jack 2.0 A type 4pin Vert SMT"/>
<attribute name="HEIGHT" value="15.2mm"/>
<attribute name="MANUFACTURER_NAME" value="CUI Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="UJ2-AV-4-SMT-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="490-UJ2-AV-4-SMT-TR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/CUI-Devices/UJ2-AV-4-SMT-TR?qs=%2FacZuiyY%252B4aDJKJlKEvGmw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB-1" library="UJ2-AV-4-SMT-TR" package="UJ2AV4SMTTR" value="UJ2-AV-4-SMT-TR">
<attribute name="ARROW_PART_NUMBER" value="UJ2-AV-4-SMT-TR"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/uj2-av-4-smt-tr/cui-devices?region=nac"/>
<attribute name="DESCRIPTION" value="USB Connectors USB Jack 2.0 A type 4pin Vert SMT"/>
<attribute name="HEIGHT" value="15.2mm"/>
<attribute name="MANUFACTURER_NAME" value="CUI Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="UJ2-AV-4-SMT-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="490-UJ2-AV-4-SMT-TR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/CUI-Devices/UJ2-AV-4-SMT-TR?qs=%2FacZuiyY%252B4aDJKJlKEvGmw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="40-PIN-GPIO" library="SparkFun-Connectors" package="2X20_SHROUDED" value="RASPBERRYPI-40-PIN-GPIO_PTH">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-12263"/>
<attribute name="SF_ID" value="PRT-13054"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="DSUB-POWER" pad="A1"/>
<contactref element="POWER-1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="POWER-1" pad="1"/>
<contactref element="DSUB-POWER" pad="A2"/>
</signal>
<signal name="N$3">
<contactref element="DSUB-POWER" pad="A3"/>
<contactref element="POWER-2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="DSUB-POWER" pad="A4"/>
<contactref element="POWER-2" pad="1"/>
</signal>
<signal name="FIX">
<contactref element="GPS" pad="6"/>
</signal>
<signal name="GND">
<contactref element="GPS" pad="3"/>
<contactref element="40-PIN-GPIO" pad="25"/>
<contactref element="40-PIN-GPIO" pad="20"/>
<contactref element="40-PIN-GPIO" pad="14"/>
<contactref element="40-PIN-GPIO" pad="30"/>
<contactref element="40-PIN-GPIO" pad="34"/>
<contactref element="40-PIN-GPIO" pad="39"/>
<contactref element="40-PIN-GPIO" pad="9"/>
</signal>
<signal name="3.3V">
<contactref element="GPS" pad="9"/>
</signal>
<signal name="ENABLE">
<contactref element="GPS" pad="8"/>
</signal>
<signal name="VIN">
<contactref element="GPS" pad="2"/>
<contactref element="40-PIN-GPIO" pad="17"/>
</signal>
<signal name="VBACKUP">
<contactref element="GPS" pad="7"/>
</signal>
<signal name="1PPS">
<contactref element="GPS" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="GPS" pad="5"/>
<contactref element="40-PIN-GPIO" pad="10"/>
</signal>
<signal name="N$6">
<contactref element="GPS" pad="4"/>
<contactref element="40-PIN-GPIO" pad="8"/>
</signal>
<signal name="5V">
<contactref element="40-PIN-GPIO" pad="4"/>
<contactref element="40-PIN-GPIO" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="I2C-3" pad="1"/>
<contactref element="I2C-2" pad="1"/>
<contactref element="I2C-1" pad="1"/>
<contactref element="40-PIN-GPIO" pad="1"/>
<contactref element="DSUB-SIGNAL" pad="16"/>
</signal>
<signal name="N$14">
<contactref element="I2C-1" pad="2"/>
<contactref element="I2C-2" pad="2"/>
<contactref element="I2C-3" pad="2"/>
<contactref element="40-PIN-GPIO" pad="6"/>
<contactref element="DSUB-SIGNAL" pad="17"/>
</signal>
<signal name="N$15">
<contactref element="I2C-1" pad="3"/>
<contactref element="I2C-2" pad="3"/>
<contactref element="I2C-3" pad="3"/>
<contactref element="40-PIN-GPIO" pad="3"/>
<contactref element="DSUB-SIGNAL" pad="15"/>
</signal>
<signal name="N$16">
<contactref element="I2C-1" pad="4"/>
<contactref element="I2C-2" pad="4"/>
<contactref element="I2C-3" pad="4"/>
<contactref element="40-PIN-GPIO" pad="5"/>
<contactref element="DSUB-SIGNAL" pad="18"/>
</signal>
<signal name="N$7">
<contactref element="RJ45" pad="8"/>
<contactref element="DSUB-SIGNAL" pad="19"/>
</signal>
<signal name="N$8">
<contactref element="RJ45" pad="7"/>
<contactref element="DSUB-SIGNAL" pad="20"/>
</signal>
<signal name="N$9">
<contactref element="RJ45" pad="6"/>
<contactref element="DSUB-SIGNAL" pad="21"/>
</signal>
<signal name="N$10">
<contactref element="RJ45" pad="5"/>
<contactref element="DSUB-SIGNAL" pad="22"/>
</signal>
<signal name="N$11">
<contactref element="RJ45" pad="4"/>
<contactref element="DSUB-SIGNAL" pad="23"/>
</signal>
<signal name="N$12">
<contactref element="RJ45" pad="3"/>
<contactref element="DSUB-SIGNAL" pad="24"/>
</signal>
<signal name="N$17">
<contactref element="RJ45" pad="2"/>
<contactref element="DSUB-SIGNAL" pad="25"/>
</signal>
<signal name="N$18">
<contactref element="RJ45" pad="1"/>
<contactref element="DSUB-SIGNAL" pad="26"/>
</signal>
<signal name="N$19">
<contactref element="DSUB-SIGNAL" pad="13"/>
<contactref element="USB-2" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="DSUB-SIGNAL" pad="12"/>
<contactref element="USB-2" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="USB-2" pad="3"/>
<contactref element="DSUB-SIGNAL" pad="11"/>
</signal>
<signal name="N$22">
<contactref element="DSUB-SIGNAL" pad="10"/>
<contactref element="USB-2" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="DSUB-SIGNAL" pad="9"/>
<contactref element="USB-1" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="USB-1" pad="2"/>
<contactref element="DSUB-SIGNAL" pad="8"/>
</signal>
<signal name="N$25">
<contactref element="DSUB-SIGNAL" pad="7"/>
<contactref element="USB-1" pad="3"/>
</signal>
<signal name="N$26">
<contactref element="USB-1" pad="4"/>
<contactref element="DSUB-SIGNAL" pad="6"/>
</signal>
<signal name="TEC2">
<contactref element="DSUB-SIGNAL" pad="4"/>
</signal>
<signal name="TEC1">
<contactref element="DSUB-SIGNAL" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
