<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="12.7" y2="0" width="0" layer="20"/>
<wire x1="12.7" y1="0" x2="12.7" y2="7.62" width="0" layer="20"/>
<wire x1="12.7" y1="7.62" x2="0" y2="7.62" width="0" layer="20"/>
<wire x1="0" y1="7.62" x2="0" y2="0" width="0" layer="20"/>
<text>P</text>
<text>R1</text>
<text>R2</text>
<text>NPN</text>
<text>GND</text>
<text>SWI</text>
<text>IN</text>
<text>OUT</text>
<text>SIG</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="SOT23-W">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Wave soldering</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
<library name="semicon-smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Semiconductors&lt;/b&gt;&lt;p&gt;
A few devices defined according to the IPC standard.&lt;p&gt;
Based on:&lt;p&gt;
IPC-SM-782&lt;br&gt;
IRevision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05_LOCK">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="adafruit" package="SOT23-W" value="">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="semicon-smd-ipc" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="10k"/>
<element name="R2" library="adafruit" package="M0805" value="4.7k"/>
<element name="Q3" library="adafruit" package="SOT23-W" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X05_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="Q2" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="Q2" pad="2"/>
<contactref element="JP2" pad="4"/>
<contactref element="TP1" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
