<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="25.39" x2="0" y2="12.7" width="0.3048" layer="20"/>
<text>MISO</text>
<text>VCC</text>
<text>SCK</text>
<text>MOSI</text>
<text>RST</text>
<text>GND</text>
<text>MISO</text>
<text>SCK</text>
<text>RST</text>
<text>VCC</text>
<text>MOSI</text>
<text>GND</text>
<wire x1="48.006" y1="25.4" x2="39.878" y2="25.4" width="0.3048" layer="20"/>
<wire x1="34.798" y1="25.4" x2="24.13" y2="25.4" width="0.3048" layer="20"/>
<wire x1="19.05" y1="25.4" x2="0" y2="25.4" width="0.3048" layer="20"/>
<wire x1="0" y1="12.7" x2="19.05" y2="12.7" width="0.3048" layer="20"/>
<wire x1="24.13" y1="12.7" x2="34.798" y2="12.7" width="0.3048" layer="20"/>
<wire x1="39.878" y1="12.7" x2="47.879" y2="12.7" width="0.3048" layer="20"/>
<wire x1="50.419" y1="15.24" x2="47.879" y2="12.7" width="0.3048" layer="20"/>
<wire x1="39.878" y1="12.7" x2="38.608" y2="13.97" width="0.3048" layer="20"/>
<wire x1="38.608" y1="13.97" x2="36.068" y2="13.97" width="0.3048" layer="20"/>
<wire x1="36.068" y1="13.97" x2="34.798" y2="12.7" width="0.3048" layer="20"/>
<wire x1="39.878" y1="25.4" x2="38.608" y2="24.13" width="0.3048" layer="20"/>
<wire x1="38.608" y1="24.13" x2="36.068" y2="24.13" width="0.3048" layer="20"/>
<wire x1="36.068" y1="24.13" x2="34.798" y2="25.4" width="0.3048" layer="20"/>
<wire x1="24.13" y1="12.7" x2="22.86" y2="13.97" width="0.3048" layer="20"/>
<wire x1="22.86" y1="13.97" x2="20.32" y2="13.97" width="0.3048" layer="20"/>
<wire x1="20.32" y1="13.97" x2="19.05" y2="12.7" width="0.3048" layer="20"/>
<wire x1="19.05" y1="25.4" x2="20.32" y2="24.13" width="0.3048" layer="20"/>
<wire x1="20.32" y1="24.13" x2="22.86" y2="24.13" width="0.3048" layer="20"/>
<wire x1="22.86" y1="24.13" x2="24.13" y2="25.4" width="0.3048" layer="20"/>
<text>tekdemo@gmail.com</text>
<text>tiny-tiny-isp</text>
<text>v2 05JAN2013</text>
<wire x1="48.006" y1="25.4" x2="50.419" y2="22.987" width="0.3048" layer="20"/>
<wire x1="50.419" y1="22.987" x2="50.419" y2="15.24" width="0.3048" layer="20"/>
<text>12V
</text>
<text>RST</text>
<text>VCC</text>
<text>VCC</text>
<text>5V</text>
<text>4</text>
<text>3</text>
<text>4</text>
<text>F</text>
<text>4</text>
<text>4</text>
<text>4</text>
<text>5</text>
<text>2</text>
<text>1</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="SJ_3_PASTE1&amp;2">
</package>
<package name="PAD.02X.02">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
</package>
<package name="SOT323">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="1X03">
</package>
<package name="2X3">
</package>
</packages>
</library>
<library name="tekdemo">
<packages>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny45">
<attribute name="PROD_ID" value="IC-08922"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R.D+" library="SparkFun-Passives" package="0805" value="68">
<attribute name="NAME"/>
</element>
<element name="R.D-" library="SparkFun-Passives" package="0805" value="68">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DZ.D+" library="SparkFun-DiscreteSemi" package="SOD-323" value="3.3V">
<attribute name="NAME"/>
</element>
<element name="DZ.D-" library="SparkFun-DiscreteSemi" package="SOD-323" value="3.3V">
<attribute name="NAME"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT323" value="NMOS">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="SparkFun-Connectors" package="USB-MINIB" value="USB-MINIB">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT323" value="NMOS">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="NAME"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT323" value="NMOS">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="NAME"/>
</element>
<element name="Q4" library="SparkFun-DiscreteSemi" package="SOT323" value="NMOS">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VREG" library="tekdemo" package="SOT23-5L" value="LDO-REGULATORMCP1801">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CBP" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
</element>
<element name="C3V3" library="SparkFun-Capacitors" package="0603-CAP" value="1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
</element>
<element name="C5V" library="SparkFun-Capacitors" package="0603-CAP" value="1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="2X3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value=""/>
<element name="R2" library="SparkFun-Passives" package="0805" value=""/>
<element name="R4" library="SparkFun-Passives" package="0805" value=""/>
<element name="R6" library="SparkFun-Passives" package="0805" value=""/>
<element name="SJ1" library="SparkFun-Passives" package="SJ_3_PASTE1&amp;2" value=""/>
<element name="HV_RST" library="SparkFun-Passives" package="PAD.02X.02" value="TEST-POINT2"/>
</elements>
<signals>
<signal name="VUSB">
<contactref element="U2" pad="8"/>
<contactref element="R3" pad="1"/>
<contactref element="JP1" pad="3"/>
<contactref element="VREG" pad="3"/>
<contactref element="VREG" pad="1"/>
<contactref element="CBP" pad="1"/>
<contactref element="C5V" pad="1"/>
<contactref element="U$1" pad="VBUS"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="4"/>
<contactref element="DZ.D+" pad="2"/>
<contactref element="DZ.D-" pad="2"/>
<contactref element="VREG" pad="2"/>
<contactref element="CBP" pad="2"/>
<contactref element="C5V" pad="2"/>
<contactref element="C3V3" pad="2"/>
<contactref element="JP2" pad="6"/>
<contactref element="U$1" pad="GND"/>
</signal>
<signal name="D-">
<contactref element="R.D-" pad="1"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="D+">
<contactref element="R.D+" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="USB.D+">
<contactref element="R.D+" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="D+"/>
<contactref element="DZ.D+" pad="1"/>
</signal>
<signal name="USB.D-">
<contactref element="R.D-" pad="2"/>
<contactref element="U$1" pad="D-"/>
<contactref element="DZ.D-" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="5"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U2" pad="6"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="U2" pad="7"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="RST">
<contactref element="U2" pad="1"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="J1.MISO">
<contactref element="Q1" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="J4.MOSI">
<contactref element="Q2" pad="2"/>
<contactref element="JP2" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="J3.SCK">
<contactref element="Q3" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="J5.RST">
<contactref element="Q4" pad="2"/>
<contactref element="JP2" pad="5"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="VREG" pad="5"/>
<contactref element="JP1" pad="1"/>
<contactref element="C3V3" pad="1"/>
</signal>
<signal name="J2.VCC">
<contactref element="Q1" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q4" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="SJ1" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="HVRST">
<contactref element="SJ1" pad="3"/>
<contactref element="HV_RST" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
