<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="14.859" width="0.2032" layer="20"/>
<wire x1="0" y1="14.859" x2="16.1544" y2="14.859" width="0.2032" layer="20"/>
<wire x1="16.1544" y1="14.859" x2="16.129" y2="0" width="0.2032" layer="20"/>
<wire x1="16.129" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<text>VIN</text>
<text>Sx/SDA</text>
<text>Sy/SCL</text>
<text>I2</text>
<text>I1</text>
<text>GND</text>
<text>i2c Range 
 Extender</text>
<text>  v1a  1-28-16 
chip@mcclellands.org</text>
<text>Local-Remote</text>
<text>Lx</text>
<text>Ly</text>
<text>P82B715D</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="1X06">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="SparkFun-Passives" package="0805" value="330">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="330">
<attribute name="NAME"/>
</element>
<element name="JP5" library="SparkFun" package="1X06" value="i2c Header"/>
<element name="JP3" library="SparkFun" package="1X06" value="Buffer Header"/>
<element name="P82B715D" library="Texas Instruments_By_element14_Batch_1" package="SOIC127P600X175-8N" value="P82B715D">
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="MPN" value="P82B715D"/>
<attribute name="OC_NEWARK" value="84M9793"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="1604945"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP5" pad="6"/>
<contactref element="JP3" pad="6"/>
<contactref element="P82B715D" pad="4"/>
</signal>
<signal name="SY">
<contactref element="JP5" pad="3"/>
<contactref element="P82B715D" pad="6"/>
</signal>
<signal name="SX">
<contactref element="JP5" pad="2"/>
<contactref element="P82B715D" pad="3"/>
</signal>
<signal name="INT2">
<contactref element="JP5" pad="4"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="INT1">
<contactref element="JP5" pad="5"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="JP5" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="P82B715D" pad="8"/>
</signal>
<signal name="LX">
<contactref element="JP3" pad="2"/>
<contactref element="P82B715D" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="LY">
<contactref element="JP3" pad="3"/>
<contactref element="P82B715D" pad="7"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
