<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="24.13" x2="0" y2="1.27" width="0.254" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0.254" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="13.97" y2="0" width="0.254" layer="20"/>
<wire x1="13.97" y1="0" x2="15.24" y2="1.27" width="0.254" layer="20" curve="90"/>
<wire x1="15.24" y1="1.27" x2="15.24" y2="24.13" width="0.254" layer="20"/>
<wire x1="15.24" y1="24.13" x2="13.97" y2="25.4" width="0.254" layer="20" curve="90"/>
<wire x1="13.97" y1="25.4" x2="1.27" y2="25.4" width="0.254" layer="20"/>
<wire x1="1.27" y1="25.4" x2="0" y2="24.13" width="0.254" layer="20" curve="90"/>
<text>xlab.stanford.edu</text>
<text>XTB-20
Holliday
2018</text>
<text>LYR1</text>
<text>LYR2</text>
<text>LYR3</text>
<text>LYR4</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>A6</text>
<text>A7</text>
<text>A8</text>
<text>A9</text>
<text>A10</text>
<text>A11</text>
<text>MOSI</text>
<text>SCK</text>
<text>MISO</text>
<text>!RST</text>
<text>GND</text>
<text>3.3V</text>
<text>CS</text>
<text>START</text>
<text>AVDD</text>
<text>GND</text>
<text>MOSI</text>
<text>SCK</text>
<text>MISO</text>
<text>!RST</text>
<text>GND</text>
<text>3.3V</text>
<text>CS</text>
<text>START</text>
<text>AVDD</text>
<text>GND</text>
<text>github.com/maholli/XTB</text>
<text>AIN11
REFN0</text>
<text>AIN10
REFP0</text>
<text>AIN8
GPIO2</text>
<text>AIN7
GPIO1</text>
<text>REF1-</text>
<text>REF1+</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUMMY">
<description>&lt;h3&gt;Dummy Footprint&lt;/h3&gt;
&lt;p&gt;NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.&lt;/p&gt;

&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;BADGERHACK_LOGO&lt;/li&gt;
&lt;li&gt;FRAME-LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="maholli">
<packages>
<package name="RHB0032H">
</package>
<package name="C_ARRAY_EXB28V">
</package>
<package name="C_ARRAY_EXB24V">
</package>
<package name="HVQFN_B">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="DESIGNER" value="Max Holliday"/>
<attribute name="VERSION" value="1"/>
</element>
<element name="U3" library="maholli" package="RHB0032H" value="Value">
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="PARTNUMBER" value="ADS124S06IRHBR"/>
<attribute name="REFDES" value="RefDes"/>
<attribute name="TYPE" value="TYPE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="0.1UF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603" value="0.33uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="0.1UF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="RA1" library="maholli" package="C_ARRAY_EXB28V" value="EXB-28VR000X">
<attribute name="MANUFACTURER_PART_NUMBER" value="EXB28VR000X"/>
<attribute name="VENDOR" value="Panasonic"/>
</element>
<element name="RA3" library="maholli" package="C_ARRAY_EXB28V" value="EXB-28VR000X">
<attribute name="MANUFACTURER_PART_NUMBER" value="EXB28VR000X"/>
<attribute name="VENDOR" value="Panasonic"/>
</element>
<element name="RA4" library="maholli" package="C_ARRAY_EXB28V" value="EXB-28VR000X">
<attribute name="MANUFACTURER_PART_NUMBER" value="EXB28VR000X"/>
<attribute name="VENDOR" value="Panasonic"/>
</element>
<element name="U1" library="maholli" package="C_ARRAY_EXB24V" value="EXB-24V470JX">
<attribute name="MANUFACTURER_PART_NUMBER" value="EXB24V470JX"/>
<attribute name="VENDOR" value="Panasonic"/>
</element>
<element name="U4" library="maholli" package="HVQFN_B" value="M-QFN28_B">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U3" pad="27"/>
<contactref element="U3" pad="17"/>
<contactref element="C3" pad="1"/>
<contactref element="U3" pad="28"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U3" pad="33"/>
<contactref element="U3" pad="14"/>
<contactref element="C4" pad="1"/>
<contactref element="U3" pad="24"/>
<contactref element="RA4" pad="5"/>
<contactref element="U4" pad="28"/>
<contactref element="U4" pad="15"/>
<contactref element="U4" pad="16"/>
<contactref element="U4" pad="20"/>
<contactref element="U4" pad="21"/>
<contactref element="U4" pad="22"/>
<contactref element="U4" pad="14"/>
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="6"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="C1" pad="2"/>
<contactref element="U3" pad="16"/>
<contactref element="U3" pad="15"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="AVDD">
<contactref element="U3" pad="26"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="C3" pad="2"/>
<contactref element="U3" pad="23"/>
</signal>
<signal name="AINCOM">
<contactref element="U3" pad="1"/>
<contactref element="RA4" pad="4"/>
</signal>
<signal name="AIN11">
<contactref element="U3" pad="29"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="AIN5">
<contactref element="U3" pad="2"/>
<contactref element="RA4" pad="3"/>
</signal>
<signal name="AIN4">
<contactref element="U3" pad="3"/>
<contactref element="RA4" pad="2"/>
</signal>
<signal name="AIN3">
<contactref element="U3" pad="4"/>
<contactref element="RA4" pad="1"/>
</signal>
<signal name="AIN1">
<contactref element="U3" pad="6"/>
<contactref element="RA1" pad="3"/>
</signal>
<signal name="AIN2">
<contactref element="U3" pad="5"/>
<contactref element="RA1" pad="4"/>
</signal>
<signal name="AIN0">
<contactref element="U3" pad="7"/>
<contactref element="RA1" pad="2"/>
</signal>
<signal name="AIN6">
<contactref element="U3" pad="22"/>
<contactref element="RA3" pad="1"/>
</signal>
<signal name="AIN7">
<contactref element="U3" pad="21"/>
<contactref element="RA3" pad="2"/>
</signal>
<signal name="AIN8">
<contactref element="U3" pad="20"/>
<contactref element="RA3" pad="3"/>
</signal>
<signal name="AIN9">
<contactref element="U3" pad="19"/>
<contactref element="RA3" pad="4"/>
</signal>
<signal name="AIN10">
<contactref element="U3" pad="30"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="SPI_CS">
<contactref element="U3" pad="9"/>
</signal>
<signal name="SPI_SCK">
<contactref element="U3" pad="11"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="U3" pad="10"/>
</signal>
<signal name="SPI_MISO">
<contactref element="U3" pad="12"/>
</signal>
<signal name="ADC_START">
<contactref element="U3" pad="8"/>
</signal>
<signal name="ADC_!RST">
<contactref element="U3" pad="18"/>
</signal>
<signal name="REFP1">
<contactref element="U3" pad="32"/>
</signal>
<signal name="REFN1">
<contactref element="U3" pad="31"/>
</signal>
<signal name="AIN3_QFN">
<contactref element="RA4" pad="8"/>
<contactref element="U4" pad="17"/>
</signal>
<signal name="AIN4_QFN">
<contactref element="RA4" pad="7"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="AIN5_QFN">
<contactref element="RA4" pad="6"/>
<contactref element="U4" pad="10"/>
</signal>
<signal name="AIN0_QFN">
<contactref element="RA1" pad="7"/>
<contactref element="U4" pad="26"/>
</signal>
<signal name="AIN1_QFN">
<contactref element="RA1" pad="6"/>
<contactref element="U4" pad="24"/>
</signal>
<signal name="AIN2_QFN">
<contactref element="RA1" pad="5"/>
<contactref element="U4" pad="19"/>
</signal>
<signal name="AIN6_QFN">
<contactref element="RA3" pad="8"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="AIN7_QFN">
<contactref element="RA3" pad="7"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="AIN8_QFN">
<contactref element="RA3" pad="6"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="AIN9_QFN">
<contactref element="RA3" pad="5"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="AIN10_QFN">
<contactref element="U1" pad="4"/>
<contactref element="U4" pad="9"/>
</signal>
<signal name="AIN11_QFN">
<contactref element="U1" pad="3"/>
<contactref element="U4" pad="13"/>
</signal>
<signal name="N$4">
</signal>
<signal name="QFN4">
<contactref element="U4" pad="4"/>
</signal>
<signal name="QFN18">
<contactref element="U4" pad="18"/>
</signal>
<signal name="QFN11">
<contactref element="U4" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
