<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>VTX</text>
<text>CAM</text>
<text>P</text>
<text>S</text>
<text>G</text>
<text>FPV VTX and Camera Power
Adapter + Decoupling Cap</text>
<text>Designed by Henry O'C
in Minnesota</text>
<wire x1="29.21" y1="57.15" x2="49.53" y2="57.15" width="0" layer="20"/>
<wire x1="49.53" y1="57.15" x2="49.53" y2="26.67" width="0" layer="20"/>
<wire x1="49.53" y1="26.67" x2="29.21" y2="26.67" width="0" layer="20"/>
<wire x1="29.21" y1="26.67" x2="29.21" y2="57.15" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
</packages>
</library>
<library name="Henry's Stuff">
<packages>
<package name="XT60CONN">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value="">
<attribute name="PROD_ID" value="CAP-08439"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
<element name="U$4" library="Henry's Stuff" package="XT60CONN" value="XT60"/>
<element name="U$5" library="Henry's Stuff" package="XT60CONN" value="XT60"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="C1" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="U$4" pad="P$4"/>
<contactref element="U$5" pad="P$5"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U$4" pad="P$5"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="6"/>
<contactref element="U$5" pad="P$4"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
