<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="1.016" y1="37.465" x2="35.611" y2="37.465" width="0" layer="20"/>
<wire x1="35.611" y1="37.465" x2="35.636" y2="75.301" width="0" layer="20"/>
<wire x1="35.636" y1="75.301" x2="1.016" y2="75.301" width="0" layer="20"/>
<wire x1="1.016" y1="75.301" x2="1.016" y2="37.465" width="0" layer="20"/>
<text>+</text>
<text>S</text>
<text>E</text>
<text>N</text>
<text>W</text>
<text>C</text>
<text>F</text>
<text>F</text>
<text>N</text>
<text>W</text>
<text>E</text>
<text>S</text>
<text>C</text>
<hole x="2.413" y="40.005" drill="1.524"/>
<hole x="33.782" y="40.005" drill="1.524"/>
<hole x="34.036" y="73.66" drill="1.524"/>
<hole x="2.667" y="73.66" drill="1.524"/>
<text>- +5V</text>
<text>V 3.1 April 2020
IntelliPaddle 
CV Paddle Controller

</text>
<text>Charles Dysert - April 2020</text>
<text>F</text>
<text>A B - +</text>
<text>ON</text>
<text>+</text>
<text>EVG2000</text>
<text>Copyright April 2020
Charles Dysert</text>
<text>rotary control wiring</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X09">
<description>&lt;h3&gt;Plated Through Hole -9 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="resistor-net">
<description>&lt;b&gt;Generic Resistor Networks&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RN-9">
<description>&lt;b&gt;RESISTOR NETWORK&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-02">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="_hhn_attiny25_45_85">
<description>&lt;h3&gt;ATMEL ATtiny 25 / 45 /48&lt;/h3&gt;
&lt;p&gt;&lt;br /&gt;&lt;b&gt;&lt;u&gt;Supplied Packages:&lt;/u&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;P&lt;/b&gt; &amp;nbsp; = PDIP 08 30mil&lt;br /&gt;
&lt;b&gt;S&lt;/b&gt; &amp;nbsp; = SOIC 08 EIAJ 208mil&lt;br /&gt;
&lt;b&gt;SS&lt;/b&gt; = SOIC 08 JEDEC 150mil&lt;br /&gt;
&lt;b&gt;X&lt;/b&gt;&gt; &amp;nbsp; = TSSOP 08 4.4mm&lt;/p&gt;

&lt;p&gt;&lt;u&gt;&lt;b&gt;Revisions / Changelog&lt;/b&gt;&lt;/u&gt;&lt;br /&gt;
&amp;bull; &amp;nbsp;5.0.0 [EAGLE 5]&lt;br /&gt;
&lt;/p&gt;

&lt;hr /&gt;

&lt;author&gt;
&lt;p&gt;&lt;u&gt;Author:&lt;/u&gt;&lt;br /&gt;
Dipl.-Ing. FH Rainer Bayer&lt;br /&gt;
HHN Hochschule Heilbronn (Heilbronn University), &lt;i&gt;rainer.bayer@hs-heilbronn.de&lt;/i&gt;&lt;br /&gt;
Ingenieurbüro ing-rb, &lt;i&gt;mail@ing-rb.de&lt;/i&gt;&lt;/p&gt;&lt;/author&gt;</description>
<packages>
<package name="DIP254P762X533-14">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="5V-IN" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CV_CONNECTOR" library="SparkFun-Connectors" package="1X09" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CV_FIREBTN" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="optocoupler" package="DIL16" value="PC847">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9707735"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="U3" library="optocoupler" package="DIL08" value="PC827">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="INTV_CONNECTOR" library="SparkFun-Connectors" package="1X09" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INTV_FIREBTN" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWERLED" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN1" library="resistor-net" package="RN-9" value="RN - 470">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="ROTARYCNTL" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="special" package="EDG-02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="_hhn_attiny25_45_85" package="DIP254P762X533-14" value="ATTINY84-20PU">
<attribute name="MPN" value="ATTINY84-20PU"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1455160"/>
<attribute name="OC_NEWARK" value="68T3783"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="Atmel"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="7"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="SW1" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="14"/>
<contactref element="SW1" pad="3"/>
<contactref element="SW1" pad="4"/>
<contactref element="ROTARYCNTL" pad="4"/>
<contactref element="5V-IN" pad="1"/>
<contactref element="RN1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="INTV_FIREBTN" pad="1"/>
<contactref element="ROTARYCNTL" pad="3"/>
<contactref element="POWERLED" pad="1"/>
<contactref element="5V-IN" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="RN1" pad="9"/>
<contactref element="POWERLED" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="ROTARYCNTL" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="N$11">
<contactref element="ROTARYCNTL" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="N$13">
<contactref element="INTV_FIREBTN" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="RN1" pad="4"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="U3" pad="4"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="CV_CONNECTOR" pad="3"/>
<contactref element="INTV_CONNECTOR" pad="1"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="N$19">
<contactref element="CV_CONNECTOR" pad="1"/>
<contactref element="INTV_CONNECTOR" pad="2"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="N$20">
<contactref element="CV_CONNECTOR" pad="2"/>
<contactref element="INTV_CONNECTOR" pad="4"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="N$21">
<contactref element="CV_CONNECTOR" pad="4"/>
<contactref element="INTV_CONNECTOR" pad="3"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="N$22">
<contactref element="CV_CONNECTOR" pad="8"/>
<contactref element="INTV_CONNECTOR" pad="5"/>
<contactref element="CV_FIREBTN" pad="2"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="5"/>
<contactref element="U2" pad="15"/>
<contactref element="U2" pad="13"/>
<contactref element="U2" pad="11"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="N$4">
<contactref element="CV_FIREBTN" pad="1"/>
<contactref element="CV_CONNECTOR" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="8"/>
<contactref element="RN1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="U2" pad="6"/>
<contactref element="RN1" pad="6"/>
</signal>
<signal name="N$14">
<contactref element="U2" pad="4"/>
<contactref element="RN1" pad="7"/>
</signal>
<signal name="N$23">
<contactref element="RN1" pad="8"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="U3" pad="6"/>
<contactref element="INTV_CONNECTOR" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="U3" pad="8"/>
<contactref element="INTV_CONNECTOR" pad="8"/>
</signal>
<signal name="N$17">
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$24">
<contactref element="U1" pad="13"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$25">
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$26">
<contactref element="U1" pad="10"/>
<contactref element="U2" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
