<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="11.43" y2="0" width="0" layer="20"/>
<wire x1="11.43" y1="0" x2="11.43" y2="15.24" width="0" layer="20"/>
<wire x1="11.43" y1="15.24" x2="0" y2="15.24" width="0" layer="20"/>
<wire x1="0" y1="15.24" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED5" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED6" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED7" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED8" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="R1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="R1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="R1206" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="LED4" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="1"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="LED6" pad="C"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R7" pad="1"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="LED8" pad="C"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="C"/>
<contactref element="R2" pad="1"/>
<contactref element="LED3" pad="C"/>
<contactref element="R4" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="LED7" pad="C"/>
<contactref element="R6" pad="1"/>
<contactref element="LED5" pad="C"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="LED2" pad="A"/>
<contactref element="R3" pad="2"/>
<contactref element="LED4" pad="A"/>
<contactref element="R5" pad="2"/>
<contactref element="LED6" pad="A"/>
<contactref element="R7" pad="2"/>
<contactref element="LED8" pad="A"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
