<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="89.9668" y2="0" width="0" layer="20"/>
<wire x1="89.9668" y1="0" x2="89.9668" y2="38.608" width="0" layer="20"/>
<wire x1="89.9668" y1="38.608" x2="0" y2="38.608" width="0" layer="20"/>
<wire x1="0" y1="38.608" x2="0" y2="0" width="0" layer="20"/>
<text>Serial</text>
<text>+</text>
<text>SPI Bus</text>
<text>+</text>
<text>chip@seeinsights.com</text>
<text>v1.3-  3-23-20</text>
<text>i2c Programmable Watchdog (open JP1 to disable)</text>
<text>LiPO Battery</text>
<text>Analog</text>
<text>I2C w/ Interrupts</text>
<text>User Btn</text>
<text>Qwiic Connectors x3</text>
<text>Power Switch</text>
<text>DC - IN</text>
<text>ON</text>
<text>Over Voltage Protection -
JP7 must be closed for Argon &amp;
Xenon. Not required for Boron</text>
<text>OFF</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FIDUCIAL-MICRO">
<description>&lt;h3&gt;Fiducial - Circle, 0.25in&lt;/h3&gt;
&lt;p&gt;Point-of-reference for pick-and-place machines and other optical instruments.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FIDUCIAL&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="OSHW-LOGO-M">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="CREATIVE_COMMONS">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Fujitsu_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 15:17:27</description>
<packages>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805@1">
</package>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="Custom Components">
<packages>
<package name="SOT-23-5">
</package>
<package name="0805">
</package>
<package name="XTAL_ECS-.327-6-17X-TR">
</package>
<package name="SOIC8-N_MC">
</package>
<package name="SOT-23-6">
</package>
<package name="STAND-OFF-M2.5">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a M2.5 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF-M2.5&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="TC2030-MCP-NL">
</package>
<package name="CL-SB-12B">
</package>
<package name="JST_BM06B-SRSS-TB(LF)(SN)">
</package>
<package name="CONN_BM04B-SRSS-TBT(LF)(SN)">
</package>
</packages>
</library>
<library name="TMP36">
<packages>
<package name="RJ_5">
</package>
</packages>
</library>
<library name="SparkFun-Fuses">
<description>&lt;h3&gt;SparkFun Fuses&lt;/h3&gt;
In this library you'll find fuses, or fuse like components such as PTCs. Reference designator F.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="MF_Passives">
<packages>
<package name="CP10MM">
<description>&lt;b&gt;Description:&lt;/b&gt; 10MM Round Package for Electrolytic Capacitors. Based on Panasonic Electrolytic Capacitors.
&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="Carrier Board">
<description>Generated from &lt;b&gt;Carrier Board.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="PARTICLE-DEVICES_BORON">
</package>
</packages>
</library>
<library name="MF_Switches">
<packages>
<package name="TACT6MM">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 6MM Tact Switch Package.&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_2_NC_PASTE_SILK">
</package>
</packages>
</library>
<library name="MF_Discrete_Semiconductor">
<packages>
<package name="SOD-123">
<description>&lt;b&gt;Description:&lt;/b&gt; Footprint for Diodes in SOD-123 Standard.&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PANASONIC_SMINI2-F5-B">
<description>From http://www.semicon.panasonic.co.jp/ds4/DZ2J150_E.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_2_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="Fujitsu_By_element14_Batch_1" package="SOIC127P600X175-8N" value="MB85RC64">
<attribute name="MPN" value="MB85RC64APNF-G-JNERE1"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1831995"/>
<attribute name="OC_NEWARK" value="93R5161"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="FUJITSU"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805@1" value="0.1uF">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-CAP-0805-0.1uF"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="G1" library="Custom Components" package="SOT-23-5" value="D5V0L4B5TS">
<attribute name="MPN" value="D5V0L4B5TS-7"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Passives" package="0805" value="4.7k">
<attribute name="MPN" value="MF-RES-0805-4.7K"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="4.7k">
<attribute name="MPN" value="MF-RES-0805-4.7K"/>
<attribute name="NAME"/>
</element>
<element name="V1" library="Custom Components" package="0805" value="VC080505C150DP ">
<attribute name="MPN" value="VC080505C150DP"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="V3" library="Custom Components" package="0805" value="VC080505C150DP ">
<attribute name="MPN" value="VC080505C150DP"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="U1" library="TMP36" package="RJ_5" value="TMP36GRTZ">
<attribute name="MANUFACTURER_PART_NUMBER" value="TMP36GRTZ-REEL7"/>
<attribute name="MPN" value="TMP36GRTZ-REEL7"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Analog Devices Inc"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805@1" value="1uF">
<attribute name="MPN" value="MF-CAP-0805-1uF"/>
<attribute name="NAME"/>
</element>
<element name="FD1" library="SparkFun-Aesthetics" package="FIDUCIAL-MICRO" value="FIDUCIALUFIDUCIAL">
<attribute name="POPULATE" value="0"/>
</element>
<element name="FD2" library="SparkFun-Aesthetics" package="FIDUCIAL-MICRO" value="FIDUCIALUFIDUCIAL">
<attribute name="POPULATE" value="0"/>
</element>
<element name="JP5" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF">
<attribute name="POPULATE" value="0"/>
</element>
<element name="JP3" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF">
<attribute name="POPULATE" value="0"/>
</element>
<element name="JP4" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF">
<attribute name="POPULATE" value="0"/>
</element>
<element name="JP6" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF">
<attribute name="POPULATE" value="0"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="JST-2-SMD" value="S2B-PH-SM4-TB(LF)(SN)">
<attribute name="MFG" value="JST S2B-PH-SM4-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="SF_ID" value="PRT-08612"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="JST-2-SMD" value="S2B-PH-SM4-TB(LF)(SN)">
<attribute name="MFG" value="JST S2B-PH-SM4-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="SF_ID" value="PRT-08612"/>
</element>
<element name="F1" library="SparkFun-Fuses" package="1206" value="63V/1.5A">
<attribute name="MPN" value="046801.5NR"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08585"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0805" value="100k">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-RES-0805-100K"/>
<attribute name="NAME"/>
</element>
<element name="F3" library="SparkFun-Fuses" package="1206" value="6V/0.5A">
<attribute name="MPN" value="0466.500NR"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08585"/>
</element>
<element name="U$2" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="">
<attribute name="POPULATE" value="0"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER">
<attribute name="DESIGNER" value=""/>
<attribute name="POPULATE" value="0"/>
<attribute name="REV" value=""/>
</element>
<element name="FRAME2" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER">
<attribute name="DESIGNER" value=""/>
<attribute name="POPULATE" value="0"/>
<attribute name="REV" value=""/>
</element>
<element name="R7" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-RES-0805-10K"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="MF_Passives" package="CP10MM" value="470uF">
<attribute name="HOUSEPART" value="1"/>
<attribute name="MPN" value="MF-CAP-10MM-470uF"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="P1" library="Carrier Board" package="PARTICLE-DEVICES_BORON" value="Particle Boron / Xenon / Argon">
<attribute name="POPULATE" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="MF_Switches" package="TACT6MM" value="MF-SW-TACT-6MM">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-SW-TACT-6MM"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-SW-TACT-6MM"/>
</element>
<element name="V2" library="Custom Components" package="0805" value="VC080505C150DP ">
<attribute name="MPN" value="VC080505C150DP"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="F2" library="SparkFun-Fuses" package="1206" value="6V/0.5A">
<attribute name="MPN" value="0466.500NR"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08585"/>
</element>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="Y1" library="Custom Components" package="XTAL_ECS-.327-6-17X-TR" value="ECS-.327-6-17X-TR">
<attribute name="DESCRIPTION" value=" ECX-306X Series 32.768 kHz ±20 ppm 6 pF -40 to +85 °C SMT Tuning Fork Crystal "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="XC1307CT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/ecs-inc/ECS-.327-6-17X-TR/XC1307CT-ND/827771?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="ECS Inc."/>
<attribute name="MP" value="ECS-.327-6-17X-TR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="4-4 ECS International"/>
</element>
<element name="U8" library="Custom Components" package="SOIC8-N_MC" value="MCP79410T-I/SN">
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP79410TISN"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="VENDOR" value="Microchip"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0805@1" value="8.2pF">
<attribute name="HOUSEPART" value="No"/>
<attribute name="MPN" value="C0805C829D5GACTU‎"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0805@1" value="10pF">
<attribute name="HOUSEPART" value="No"/>
<attribute name="MPN" value="C0805C100JDGACTU‎"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="U4" library="Custom Components" package="SOT-23-6" value="TPS22810">
<attribute name="MPN" value="TPS22810DBVT"/>
<attribute name="NAME"/>
</element>
<element name="U5" library="Custom Components" package="SOT-23-6" value="TPS22810">
<attribute name="MPN" value="TPS22810DBVT"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805@1" value="10nF">
<attribute name="HOUSEPART" value="No"/>
<attribute name="MPN" value="08051C103K4T2A"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805@1" value="10nF">
<attribute name="HOUSEPART" value="No"/>
<attribute name="MPN" value="08051C103K4T2A"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805@1" value="0.1uF">
<attribute name="HOUSEPART" value="Yes"/>
<attribute name="MPN" value="MF-CAP-0805-0.1uF"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="MF_Discrete_Semiconductor" package="SOD-123" value="BAT42">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-DIO-SOD123-BAT42"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DIO-SOD123-BAT42"/>
</element>
<element name="D2" library="MF_Discrete_Semiconductor" package="SOD-123" value="BAT42">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-DIO-SOD123-BAT42"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DIO-SOD123-BAT42"/>
</element>
<element name="R9" library="SparkFun-Passives" package="0805" value="100">
<attribute name="HOUSEPART" value="Yes"/>
<attribute name="MPN" value="MF-RES-0805-100"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Passives" package="0805" value="100">
<attribute name="HOUSEPART" value="Yes"/>
<attribute name="MPN" value="MF-RES-0805-100"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805@1" value="0.1uF">
<attribute name="HOUSEPART" value="Yes"/>
<attribute name="MPN" value="MF-CAP-0805-0.1uF"/>
<attribute name="NAME"/>
</element>
<element name="FRAME3" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER">
<attribute name="POPULATE" value="0"/>
</element>
<element name="H1" library="Custom Components" package="STAND-OFF-M2.5" value="STAND-OFF-M2.5">
<attribute name="POPULATE" value="0"/>
</element>
<element name="H2" library="Custom Components" package="STAND-OFF-M2.5" value="STAND-OFF-M2.5">
<attribute name="POPULATE" value="0"/>
</element>
<element name="H3" library="Custom Components" package="STAND-OFF-M2.5" value="STAND-OFF-M2.5">
<attribute name="POPULATE" value="0"/>
</element>
<element name="H4" library="Custom Components" package="STAND-OFF-M2.5" value="STAND-OFF-M2.5">
<attribute name="POPULATE" value="0"/>
</element>
<element name="JP7" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_SILK" value="JUMPER-SMT_2_NO_SILK">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="PANASONIC_SMINI2-F5-B" value="6.2V/500mW">
<attribute name="MPN" value="TDZ6V2J,115"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="PROD_ID" value="DIO-12989"/>
</element>
<element name="ATTINY85" library="SparkFun" package="SO08-EIAJ" value="ATTINY85">
<attribute name="MPN" value="ATTINY85-20SUR"/>
<attribute name="NAME"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="MPN" value="MF-CAP-0805-0.1uF"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="MPN" value="MF-RES-0805-100K"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="ICSP" library="Custom Components" package="TC2030-MCP-NL" value="TCP2030-MCP-NL">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="S1" library="Custom Components" package="CL-SB-12B" value="CL-SB-12B-01T">
<attribute name="DESCRIPTION" value=" Switch Slide N.O./N.C. SPDT Top Slide 0.2A 12VDC Gull Wing SMD T/R "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="563-1318-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/nidec-copal-electronics/CL-SB-12B-01T/563-1318-1-ND/3507878?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Nidec Copal"/>
<attribute name="MP" value="CL-SB-12B-01T"/>
<attribute name="PACKAGE" value="None"/>
</element>
<element name="J3" library="Custom Components" package="CONN_BM04B-SRSS-TBT(LF)(SN)" value="BM04B-SRSS-TBT(LF)(SN)">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" 1.0mm Pitch, Ultra-Compact, Low Profile Design, Interchangeable Shrouded Header "/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="BM04B-SRSS-TBT_LF__SN_"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="D4" library="MF_Discrete_Semiconductor" package="SOD-123" value="BAT42">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-DIO-SOD123-BAT42"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DIO-SOD123-BAT42"/>
</element>
<element name="J7" library="Custom Components" package="CONN_BM04B-SRSS-TBT(LF)(SN)" value="BM04B-SRSS-TBT(LF)(SN)">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" 1.0mm Pitch, Ultra-Compact, Low Profile Design, Interchangeable Shrouded Header "/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="BM04B-SRSS-TBT_LF__SN_"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="J4" library="Custom Components" package="JST_BM06B-SRSS-TB(LF)(SN)" value="BM06B-SRSS-TB(LF)(SN)">
<attribute name="MPN" value="BM06B-SRSS-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="J6" library="Custom Components" package="JST_BM06B-SRSS-TB(LF)(SN)" value="BM06B-SRSS-TB(LF)(SN)">
<attribute name="MPN" value="BM06B-SRSS-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="J5" library="Custom Components" package="JST_BM06B-SRSS-TB(LF)(SN)" value="BM06B-SRSS-TB(LF)(SN)">
<attribute name="MPN" value="BM06B-SRSS-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-RES-0805-10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0805@1" value="10nF">
<attribute name="HOUSEPART" value="No"/>
<attribute name="MPN" value="08051C103K4T2A"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="J8" library="Custom Components" package="CONN_BM04B-SRSS-TBT(LF)(SN)" value="BM04B-SRSS-TBT(LF)(SN)">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" 1.0mm Pitch, Ultra-Compact, Low Profile Design, Interchangeable Shrouded Header "/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="BM04B-SRSS-TBT_LF__SN_"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="J9" library="Custom Components" package="CONN_BM04B-SRSS-TBT(LF)(SN)" value="BM04B-SRSS-TBT(LF)(SN)">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" 1.0mm Pitch, Ultra-Compact, Low Profile Design, Interchangeable Shrouded Header "/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="BM04B-SRSS-TBT_LF__SN_"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="G1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="V1" pad="1"/>
<contactref element="V3" pad="1"/>
<contactref element="C8" pad="P$2"/>
<contactref element="P1" pad="GND"/>
<contactref element="V2" pad="1"/>
<contactref element="U8" pad="4"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="Y1" pad="2"/>
<contactref element="Y1" pad="3"/>
<contactref element="U4" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="SW1" pad="P$3"/>
<contactref element="SW1" pad="P$4"/>
<contactref element="D3" pad="A"/>
<contactref element="ICSP" pad="6"/>
<contactref element="ATTINY85" pad="4"/>
<contactref element="C9" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="SH1"/>
<contactref element="J3" pad="SH2"/>
<contactref element="J7" pad="SH1"/>
<contactref element="J7" pad="SH2"/>
<contactref element="J4" pad="S1"/>
<contactref element="J4" pad="S2"/>
<contactref element="J6" pad="S1"/>
<contactref element="J6" pad="S2"/>
<contactref element="J5" pad="S1"/>
<contactref element="J5" pad="S2"/>
<contactref element="J7" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J6" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="J9" pad="1"/>
<contactref element="J8" pad="1"/>
<contactref element="J8" pad="SH1"/>
<contactref element="J8" pad="SH2"/>
<contactref element="J9" pad="SH1"/>
<contactref element="J9" pad="SH2"/>
</signal>
<signal name="SCL">
<contactref element="U2" pad="6"/>
<contactref element="G1" pad="3"/>
<contactref element="R5" pad="1"/>
<contactref element="P1" pad="SCL"/>
<contactref element="U8" pad="6"/>
<contactref element="ATTINY85" pad="7"/>
<contactref element="ICSP" pad="3"/>
<contactref element="J3" pad="4"/>
<contactref element="J4" pad="4"/>
<contactref element="J9" pad="4"/>
<contactref element="J8" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="U2" pad="5"/>
<contactref element="G1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="P1" pad="SDA"/>
<contactref element="U8" pad="5"/>
<contactref element="ATTINY85" pad="5"/>
<contactref element="ICSP" pad="4"/>
<contactref element="J3" pad="3"/>
<contactref element="J4" pad="3"/>
<contactref element="J9" pad="3"/>
<contactref element="J8" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="U2" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="F3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="F2" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="P1" pad="3V3"/>
<contactref element="U8" pad="8"/>
<contactref element="D4" pad="ANODE"/>
</signal>
<signal name="LI+">
<contactref element="P1" pad="LI+"/>
<contactref element="U4" pad="6"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="D2">
<contactref element="G1" pad="5"/>
<contactref element="P1" pad="D2"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="D3">
<contactref element="G1" pad="4"/>
<contactref element="P1" pad="D3"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="TX">
<contactref element="P1" pad="TX"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="A2">
<contactref element="P1" pad="A2"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="!TINY-RST">
<contactref element="ATTINY85" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="ICSP" pad="5"/>
</signal>
<signal name="DONE">
<contactref element="ATTINY85" pad="3"/>
<contactref element="P1" pad="D5"/>
</signal>
<signal name="RX">
<contactref element="P1" pad="RX"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="TEMP">
<contactref element="U1" pad="1"/>
<contactref element="P1" pad="A4"/>
</signal>
<signal name="VCC-EXT">
<contactref element="V3" pad="2"/>
<contactref element="F3" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="USER-SW">
<contactref element="R7" pad="1"/>
<contactref element="P1" pad="D4"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="SW1" pad="P$2"/>
<contactref element="SW1" pad="P$1"/>
</signal>
<signal name="SS">
<contactref element="P1" pad="A5"/>
<contactref element="J6" pad="6"/>
</signal>
<signal name="MD">
<contactref element="P1" pad="MD"/>
</signal>
<signal name="A0">
<contactref element="P1" pad="A0"/>
<contactref element="J5" pad="6"/>
</signal>
<signal name="A1">
<contactref element="P1" pad="A1"/>
<contactref element="J5" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="P1" pad="SCK"/>
<contactref element="J6" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="P1" pad="MO"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="P1" pad="MI"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="WAKE">
<contactref element="P1" pad="D8"/>
<contactref element="ATTINY85" pad="2"/>
</signal>
<signal name="EN">
<contactref element="P1" pad="EN"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="VUSB">
<contactref element="P1" pad="VUSB"/>
<contactref element="F1" pad="2"/>
<contactref element="V1" pad="2"/>
<contactref element="C8" pad="P$1"/>
</signal>
<signal name="VCC2-EXT">
<contactref element="F2" pad="2"/>
<contactref element="V2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J8" pad="2"/>
<contactref element="J9" pad="2"/>
</signal>
<signal name="RTC-INT">
<contactref element="U8" pad="7"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="EN/UVLO">
<contactref element="U4" pad="3"/>
<contactref element="U5" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="BATT-IN">
<contactref element="U4" pad="1"/>
<contactref element="D1" pad="ANODE"/>
<contactref element="J2" pad="2"/>
<contactref element="U8" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="D1" pad="CATHODE"/>
<contactref element="D2" pad="CATHODE"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="DC-IN">
<contactref element="U5" pad="1"/>
<contactref element="D2" pad="ANODE"/>
<contactref element="J1" pad="2"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C6" pad="1"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="U5" pad="5"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U5" pad="6"/>
<contactref element="R8" pad="2"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U4" pad="4"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U4" pad="5"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="DEEP-SLEEP">
<contactref element="P1" pad="D6"/>
</signal>
<signal name="N$15">
<contactref element="U8" pad="1"/>
<contactref element="Y1" pad="1"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U8" pad="2"/>
<contactref element="Y1" pad="4"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D3" pad="C"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="NC2">
</signal>
<signal name="NC1">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="N$8">
<contactref element="ATTINY85" pad="8"/>
<contactref element="C9" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="!RST">
<contactref element="P1" pad="RST"/>
<contactref element="ATTINY85" pad="6"/>
<contactref element="ICSP" pad="1"/>
</signal>
<signal name="A3">
<contactref element="P1" pad="A3"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="VCC-WDT">
<contactref element="JP1" pad="2"/>
<contactref element="ICSP" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="D4" pad="CATHODE"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
