<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="21.57" y2="0" width="0" layer="20"/>
<wire x1="21.57" y1="0" x2="21.57" y2="30.15" width="0" layer="20"/>
<wire x1="21.57" y1="30.15" x2="0" y2="30.15" width="0" layer="20"/>
<wire x1="0" y1="30.15" x2="0" y2="0" width="0" layer="20"/>
<text>GMR</text>
<text>VexToIno</text>
<text>v1.0</text>
<text>5v</text>
<text>Gnd</text>
<text>7.2v</text>
<text>Gnd</text>
<text>SDA</text>
</plain>
<libraries>
<library name="con-tycoelectronics">
<description>&lt;b&gt;Tyco Electronics Connector&lt;/b&gt;&lt;p&gt;
http://catalog.tycoelectronics.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RJ11-NO_SHIELD">
<description>&lt;b&gt;RJ11 Low Profile&lt;/b&gt; No Shield&lt;/b&gt;&lt;p&gt;
For all RJ11 N and Z Series Models&lt;br&gt;
Source: www.tycoelectronics.com .. ENG_DS_1654001_1099_RJ_L_0507.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X11_LOCK">
<description>&lt;h3&gt;Plated Through Hole -11 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Long Pad w/ Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to lock pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="con-tycoelectronics" package="RJ11-NO_SHIELD" value="RJ11-2L-B">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RJ11-2L-B"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="83F4463"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X11_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X03_LOCK_LONGPADS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="J1" pad="4"/>
<contactref element="J3" pad="2"/>
<contactref element="J2" pad="11"/>
</signal>
<signal name="N$3">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="5"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="J2" pad="8"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="J2" pad="7"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="10"/>
<contactref element="J3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
