<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="36.83" y2="0" width="0" layer="20"/>
<wire x1="36.83" y1="0" x2="38.1" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="38.1" y1="1.27" x2="38.08" y2="1.27" width="0" layer="20"/>
<wire x1="38.08" y1="1.27" x2="38.08" y2="30.404" width="0" layer="20"/>
<wire x1="38.08" y1="30.404" x2="37.242" y2="31.242" width="0" layer="20" curve="90"/>
<wire x1="37.242" y1="31.242" x2="0.838" y2="31.242" width="0" layer="20"/>
<wire x1="0.838" y1="31.242" x2="0" y2="30.404" width="0" layer="20" curve="90"/>
<wire x1="0" y1="30.404" x2="0" y2="1.27" width="0" layer="20"/>
<hole x="2.54" y="21.971" drill="2.7"/>
<hole x="35.56" y="21.971" drill="2.7"/>
<hole x="35.56" y="2.54" drill="2.7"/>
<hole x="2.54" y="2.54" drill="2.7"/>
<text>P2</text>
<text>P1</text>
<text>USB Power</text>
<text>v1.0</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-B-MICRO-SMD">
<description>&lt;h3&gt;USB - microB SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Micro-USB.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_MICRO-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT95P280X130-5N">
<description>&lt;b&gt;5-Pin SOT23 (M5)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="QFN50P400X400X100-25N">
<description>&lt;b&gt;USB2422/MJ-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOT95P280X130-3N">
<description>&lt;b&gt;SOT-23&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="UJ2-AH-1-SMT-TR">
<description>&lt;b&gt;UJ2-AH-1-SMT-TR&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="mbed-HDK-Oscillator">
<packages>
<package name="3.2X.2.5">
</package>
</packages>
</library>
<library name="mbed-HDK-Power">
<packages>
<package name="SOT23-6L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C11" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0603" value="18pF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08267"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0603" value="18pF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08267"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="USB-B-MICRO-SMD" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11752"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603" value="12k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-10327"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="U12" library="SamacSys_Parts" package="QFN50P400X400X100-25N" value="USB2422-I_MJ">
<attribute name="DESCRIPTION" value="USB2422-I/MJ, USB Hub USB 2.0, 3  3.6 V, 24-Pin, SQFN"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="USB2422-I/MJ"/>
<attribute name="MOUSER_PART_NUMBER" value="579-USB2422-I/MJ"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=579-USB2422-I%2FMJ"/>
<attribute name="NAME"/>
</element>
<element name="U11" library="SamacSys_Parts" package="SOT95P280X130-3N" value="XC6206P332MR-G">
<attribute name="DESCRIPTION" value="LDO Voltage Regulators"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="MANUFACTURER_NAME" value="Torex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="XC6206P332MR-G"/>
<attribute name="MOUSER_PART_NUMBER" value="865-XC6206P332MR-G"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Torex-Semiconductor/XC6206P332MR-G?qs=AsjdqWjXhJ%2FXxNpRY3zZ8g%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="Y11" library="mbed-HDK-Oscillator" package="3.2X.2.5" value="7M-24.000MAAJ-T">
<attribute name="MF" value="TXC"/>
<attribute name="MFN" value="7M-12.000MAAJ-T"/>
<attribute name="NAME"/>
<attribute name="OC-DIGIKEY" value="887-1121-1-ND"/>
<attribute name="OC-MOUSER" value="717-7M-12.000MAAJ-T"/>
<attribute name="OC-NEWARK" value="84R5706"/>
<attribute name="VALUE"/>
</element>
<element name="U21" library="SamacSys_Parts" package="SOT95P280X130-5N" value="MIC2005A-1YM5-TR">
<attribute name="DESCRIPTION" value="Micrel MIC2005A-1YM5 TR, USB Power Switch, High Side, 275m, 2.5 V min., 5-Pin SOT-23"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MIC2005A-1YM5-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="998-MIC2005A-1YM5TR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Microchip-Technology-Micrel/MIC2005A-1YM5-TR?qs=Y3Q3JoKAO1So3rAZNWgOKw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="U22" library="SamacSys_Parts" package="SOT95P280X130-5N" value="MIC2005A-1YM5-TR">
<attribute name="DESCRIPTION" value="Micrel MIC2005A-1YM5 TR, USB Power Switch, High Side, 275m, 2.5 V min., 5-Pin SOT-23"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MIC2005A-1YM5-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="998-MIC2005A-1YM5TR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Microchip-Technology-Micrel/MIC2005A-1YM5-TR?qs=Y3Q3JoKAO1So3rAZNWgOKw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C23" library="SparkFun-Capacitors" package="PANASONIC_D" value="100uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-12547"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="SparkFun-Capacitors" package="PANASONIC_D" value="100uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-12547"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE"/>
</element>
<element name="U13" library="mbed-HDK-Power" package="SOT23-6L" value="USBLC6-2SC6SC6">
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MFN" value="USBLC6-2SC6"/>
<attribute name="NAME"/>
<attribute name="OC-DIGIKEY" value="497-5235-1-ND"/>
<attribute name="OC-MOUSER" value="511-USBLC6-2SC6"/>
<attribute name="OC-NEWARK" value="26M4748"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="mbed-HDK-Power" package="SOT23-6L" value="USBLC6-2SC6SC6">
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MFN" value="USBLC6-2SC6"/>
<attribute name="NAME"/>
<attribute name="OC-DIGIKEY" value="497-5235-1-ND"/>
<attribute name="OC-MOUSER" value="511-USBLC6-2SC6"/>
<attribute name="OC-NEWARK" value="26M4748"/>
</element>
<element name="U2" library="mbed-HDK-Power" package="SOT23-6L" value="USBLC6-2SC6SC6">
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MFN" value="USBLC6-2SC6"/>
<attribute name="NAME"/>
<attribute name="OC-DIGIKEY" value="497-5235-1-ND"/>
<attribute name="OC-MOUSER" value="511-USBLC6-2SC6"/>
<attribute name="OC-NEWARK" value="26M4748"/>
</element>
<element name="J21" library="SamacSys_Parts" package="UJ2-AH-1-SMT-TR" value="UJ2-AH-1-SMT-TR">
<attribute name="DESCRIPTION" value="USB jack, 4 position, surface mount"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="CUI Devices"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="UJ2-AH-1-SMT-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="490-UJ2-AH-1-SMT-TR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/CUI-Devices/UJ2-AH-1-SMT-TR?qs=%2FacZuiyY%252B4bMRuKlU7nMjQ%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="J22" library="SamacSys_Parts" package="UJ2-AH-1-SMT-TR" value="UJ2-AH-1-SMT-TR">
<attribute name="DESCRIPTION" value="USB jack, 4 position, surface mount"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="CUI Devices"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="UJ2-AH-1-SMT-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="490-UJ2-AH-1-SMT-TR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/CUI-Devices/UJ2-AH-1-SMT-TR?qs=%2FacZuiyY%252B4bMRuKlU7nMjQ%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C18" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0603" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE" value="330"/>
</element>
<element name="C25" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="SparkFun-Resistors" package="0603" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="SparkFun-Resistors" package="0603" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U11" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U12" pad="25"/>
<contactref element="R11" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="C17" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="J11" pad="GND"/>
<contactref element="U21" pad="2"/>
<contactref element="U22" pad="2"/>
<contactref element="C23" pad="-"/>
<contactref element="C24" pad="-"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="U13" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="J21" pad="4"/>
<contactref element="J22" pad="4"/>
<contactref element="R14" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="C25" pad="2"/>
<contactref element="R21" pad="1"/>
<contactref element="C26" pad="2"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U11" pad="3"/>
<contactref element="C12" pad="1"/>
<contactref element="J11" pad="VBUS"/>
<contactref element="U21" pad="1"/>
<contactref element="U22" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="U13" pad="5"/>
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="+3V3">
<contactref element="U11" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="U12" pad="1"/>
<contactref element="U12" pad="18"/>
<contactref element="U12" pad="16"/>
<contactref element="R13" pad="2"/>
<contactref element="U12" pad="9"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="TGT1_USB_D-">
<contactref element="U12" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="TGT1_USB_D+">
<contactref element="U12" pad="3"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="TGT2_USB_D-">
<contactref element="U12" pad="4"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="HUB_USB_D-">
<contactref element="U12" pad="19"/>
<contactref element="U13" pad="3"/>
</signal>
<signal name="HUB_USB_D+">
<contactref element="U12" pad="20"/>
<contactref element="U13" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U12" pad="24"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="HUB_XTAL1">
<contactref element="U12" pad="22"/>
<contactref element="Y11" pad="P$1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="HUB_XTAL2">
<contactref element="U12" pad="21"/>
<contactref element="Y11" pad="P$3"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U12" pad="13"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U12" pad="14"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U12" pad="17"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U12" pad="15"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="C15" pad="1"/>
<contactref element="U12" pad="10"/>
</signal>
<signal name="TGT2_USB_D+">
<contactref element="U12" pad="5"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="TGT1_PWR">
<contactref element="U12" pad="7"/>
<contactref element="U21" pad="3"/>
</signal>
<signal name="TGT2_PWR">
<contactref element="U12" pad="11"/>
<contactref element="U22" pad="3"/>
</signal>
<signal name="TGT1_VCC">
<contactref element="U21" pad="5"/>
<contactref element="C23" pad="+"/>
<contactref element="J21" pad="1"/>
</signal>
<signal name="TGT2_VCC">
<contactref element="U22" pad="5"/>
<contactref element="C24" pad="+"/>
<contactref element="J22" pad="1"/>
</signal>
<signal name="HUB_USB_D-_OUT">
<contactref element="J11" pad="D-"/>
<contactref element="U13" pad="4"/>
</signal>
<signal name="HUB_USB_D+_OUT">
<contactref element="J11" pad="D+"/>
<contactref element="U13" pad="6"/>
</signal>
<signal name="TGT1_USB_D+_OUT">
<contactref element="U1" pad="6"/>
<contactref element="J21" pad="3"/>
</signal>
<signal name="TGT1_USB_D-_OUT">
<contactref element="U1" pad="4"/>
<contactref element="J21" pad="2"/>
</signal>
<signal name="TGT2_USB_D+_OUT">
<contactref element="U2" pad="6"/>
<contactref element="J22" pad="3"/>
</signal>
<signal name="TGT2_USB_D-_OUT">
<contactref element="U2" pad="4"/>
<contactref element="J22" pad="2"/>
</signal>
<signal name="TGT1_FAULT">
<contactref element="U12" pad="8"/>
<contactref element="U21" pad="4"/>
</signal>
<signal name="TGT2_FAULT">
<contactref element="U12" pad="12"/>
<contactref element="U22" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="R16" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="J11" pad="SHIELD2"/>
<contactref element="J11" pad="SHIELD1"/>
<contactref element="J11" pad="SHIELD3"/>
</signal>
<signal name="N$2">
<contactref element="J21" pad="5"/>
<contactref element="J21" pad="6"/>
<contactref element="R21" pad="2"/>
<contactref element="C25" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J22" pad="5"/>
<contactref element="J22" pad="6"/>
<contactref element="R22" pad="2"/>
<contactref element="C26" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
