<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="1.524" y1="0" x2="27.94" y2="0" width="0" layer="20"/>
<wire x1="27.94" y1="0" x2="29.388" y2="1.448" width="0" layer="20" curve="90"/>
<wire x1="29.388" y1="1.448" x2="29.388" y2="22.606" width="0" layer="20"/>
<wire x1="29.388" y1="22.606" x2="27.874" y2="24.12" width="0" layer="20" curve="90"/>
<wire x1="27.874" y1="24.12" x2="1.524" y2="24.12" width="0" layer="20"/>
<wire x1="1.524" y1="24.12" x2="0" y2="22.596" width="0" layer="20" curve="90"/>
<wire x1="0" y1="22.596" x2="0" y2="1.524" width="0" layer="20"/>
<wire x1="0" y1="1.524" x2="1.524" y2="0" width="0" layer="20" curve="90"/>
<text>5V Reg</text>
<text>EL817
Opto</text>
<text>IRMLM2502</text>
<text>(–)</text>
<text>(+)</text>
<text>LED Bias Lighting 
Controller</text>
<text>https://github.com/kauberry/tv_bias_lighting_board</text>
<text>Version 2.0
December 2018</text>
<text>12V DC, 2.0A</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="GDOv5 Board">
<description>Generated from &lt;b&gt;GDOv5 Board.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;
&lt;p&gt;Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140&lt;/p&gt;
&lt;p&gt;SMA is the smallest package in the DO-214 standard (DO-214AC)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="we-transistor">
<description>Transistors, Fets...</description>
<packages>
<package name="SOT23">
</package>
</packages>
</library>
<library name="con-jack">
<description>&lt;b&gt;Jacks&lt;/b&gt;&lt;p&gt;
Power Connectors&lt;br&gt;
Phone Connectors&lt;br&gt;
Cinch Connectors&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DCJ0202">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;&lt;p&gt;
Source: DCJ0202.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-IC-Power">
<description>&lt;h3&gt;SparkFun Power Driver and Management ICs&lt;/h3&gt;
In this library you'll find anything that has to do with power delivery, or making power supplies.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;LDOs&lt;/li&gt;
&lt;li&gt;Boost/Buck controllers&lt;/li&gt;
&lt;li&gt;Charge pump controllers&lt;/li&gt;
&lt;li&gt;Power sequencers&lt;/li&gt;
&lt;li&gt;Power switches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="UX60-MB-5ST">
<description>&lt;b&gt;MINI USB Connector HI-SPEED Certified&lt;/b&gt; Metal Shield SMT Type With Positioning Post&lt;p&gt;
Source: http://www.hirose.co.jp/cataloge_hp/e24000019.pdf</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="GadgetFactory_v1">
<packages>
<package name="PC817SMT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ATTINY85" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="ATTINY45">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="GDOv5 Board" package="C1206K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08053"/>
<attribute name="VALUE"/>
</element>
<element name="IRF740_MOSFET1" library="we-transistor" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-jack" package="DCJ0202" value="DCJ0202">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="1206" value="1kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="1206" value="10kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="1206" value="10kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="1206" value="150Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="1206" value="10kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-IC-Power" package="SOT223" value="V_REG_317SMD">
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-hirose" package="UX60-MB-5ST" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-wago-500" package="W237-102" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="GadgetFactory_v1" package="PC817SMT" value="PC817S">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+12V">
<contactref element="J1" pad="1"/>
<contactref element="X2" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="ATTINY85" pad="8"/>
<contactref element="U1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="LED-">
<contactref element="X2" pad="2"/>
<contactref element="IRF740_MOSFET1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="ATTINY85" pad="4"/>
<contactref element="X3" pad="3"/>
<contactref element="IRF740_MOSFET1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="RST">
<contactref element="ATTINY85" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VUSB-">
<contactref element="X1" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="VUSB+">
<contactref element="X1" pad="1"/>
<contactref element="X3" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="TRIG-">
<contactref element="X3" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="TRIG_IN">
<contactref element="X3" pad="4"/>
<contactref element="R4" pad="1"/>
<contactref element="ATTINY85" pad="7"/>
</signal>
<signal name="CTRL_OUT">
<contactref element="ATTINY85" pad="5"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IRF740_MOSFET1" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
