<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="1.777821875" y1="15.746425" x2="1.777821875" y2="2.963290625" width="0.1524" layer="20"/>
<wire x1="1.777821875" y1="2.963290625" x2="4.317821875" y2="0.423290625" width="0.1524" layer="20" curve="90"/>
<wire x1="4.317821875" y1="0.423290625" x2="38.68520625" y2="0.423290625" width="0.1524" layer="20"/>
<wire x1="38.68520625" y1="0.423290625" x2="41.22520625" y2="2.961184375" width="0.1524" layer="20" curve="89.952489"/>
<wire x1="41.22520625" y1="2.961184375" x2="41.228478125" y2="15.49503125" width="0.1524" layer="20"/>
<wire x1="41.228478125" y1="15.49503125" x2="41.482478125" y2="15.746425" width="0.1524" layer="20" curve="-89.985197"/>
<wire x1="41.482478125" y1="15.746425" x2="43.196809375" y2="15.746425" width="0.1524" layer="20"/>
<wire x1="43.196809375" y1="15.746425" x2="43.514309375" y2="16.063925" width="0.1524" layer="20" curve="90"/>
<wire x1="43.514309375" y1="16.063925" x2="43.514309375" y2="17.46071875" width="0.1524" layer="20"/>
<wire x1="43.514309375" y1="17.46071875" x2="43.196809375" y2="17.77821875" width="0.1524" layer="20" curve="90"/>
<wire x1="43.196809375" y1="17.77821875" x2="41.7643375" y2="17.77821875" width="0.1524" layer="20"/>
<wire x1="41.7643375" y1="17.77821875" x2="41.716484375" y2="18.163946875" width="0.1524" layer="20" curve="-121.239393"/>
<wire x1="24.29703125" y1="39.6200375" x2="38.68854375" y2="39.6200375" width="0.1524" layer="20"/>
<wire x1="38.68854375" y1="39.6200375" x2="41.22854375" y2="37.0800375" width="0.1524" layer="20" curve="-90"/>
<wire x1="41.22854375" y1="37.0800375" x2="41.22854375" y2="23.259871875" width="0.1524" layer="20"/>
<wire x1="41.22854375" y1="23.259871875" x2="41.54604375" y2="22.942371875" width="0.1524" layer="20" curve="90"/>
<wire x1="41.54604375" y1="22.942371875" x2="43.487028125" y2="22.942371875" width="0.1524" layer="20"/>
<wire x1="43.487028125" y1="22.942371875" x2="44.029959375" y2="21.978053125" width="0.1524" layer="20" curve="-121.239199"/>
<wire x1="44.029959375" y1="21.978053125" x2="41.716484375" y2="18.163946875" width="0.1524" layer="20"/>
<wire x1="24.29703125" y1="39.6200375" x2="23.916240625" y2="40.599003125" width="0.1524" layer="20"/>
<wire x1="23.916240625" y1="40.599003125" x2="23.450665625" y2="40.6171125" width="0.1524" layer="20" curve="133.035628"/>
<wire x1="23.450665625" y1="40.6171125" x2="22.603740625" y2="38.8581125" width="0.1524" layer="20"/>
<wire x1="22.603740625" y1="38.8581125" x2="21.907728125" y2="40.56650625" width="0.1524" layer="20"/>
<wire x1="21.907728125" y1="40.56650625" x2="21.437271875" y2="40.56650625" width="0.1524" layer="20" curve="135.667018"/>
<wire x1="21.437271875" y1="40.56650625" x2="20.741259375" y2="38.8581125" width="0.1524" layer="20"/>
<wire x1="20.741259375" y1="38.8581125" x2="19.95746875" y2="40.6216375" width="0.1524" layer="20"/>
<wire x1="19.95746875" y1="40.6216375" x2="19.49325" y2="40.6216375" width="0.1524" layer="20" curve="132.075165"/>
<wire x1="19.49325" y1="40.6216375" x2="18.7094625" y2="38.8581125" width="0.1524" layer="20"/>
<wire x1="18.7094625" y1="38.8581125" x2="18.054778125" y2="40.6257625" width="0.1524" layer="20"/>
<wire x1="18.054778125" y1="40.6257625" x2="17.594553125" y2="40.660896875" width="0.1524" layer="20" curve="130.62222"/>
<wire x1="17.594553125" y1="40.660896875" x2="17.016296875" y2="39.6200375" width="0.1524" layer="20"/>
<wire x1="2.8882875" y1="19.05495" x2="2.886571875" y2="18.362046875" width="0.1524" layer="20"/>
<wire x1="2.886571875" y1="18.362046875" x2="2.63138125" y2="18.10829375" width="0.1524" layer="20" curve="-90.126481"/>
<wire x1="2.63138125" y1="18.10829375" x2="1.31524375" y2="18.11446875" width="0.1524" layer="20"/>
<wire x1="2.8882875" y1="19.05495" x2="2.6335375" y2="19.309153125" width="0.1524" layer="20" curve="90.311152"/>
<wire x1="2.6335375" y1="19.309153125" x2="0.55224375" y2="19.3030125" width="0.1524" layer="20"/>
<wire x1="0.55224375" y1="19.3030125" x2="-0.08463125" y2="19.938009375" width="0.1524" layer="20" curve="-90.143446"/>
<wire x1="-0.08463125" y1="19.938009375" x2="-0.08463125" y2="20.6965625" width="0.1524" layer="20" locked="yes"/>
<wire x1="-0.08463125" y1="20.6965625" x2="0.554946875" y2="21.33154375" width="0.1524" layer="20" curve="-90.413087"/>
<wire x1="0.554946875" y1="21.33154375" x2="1.52981875" y2="21.324515625" width="0.1524" layer="20"/>
<wire x1="1.52981875" y1="21.324515625" x2="1.78565" y2="21.57916875" width="0.1524" layer="20" curve="90.561113"/>
<wire x1="1.78565" y1="21.57916875" x2="1.769590625" y2="37.086928125" width="0.1524" layer="20"/>
<wire x1="1.31524375" y1="18.11446875" x2="0.677265625" y2="17.479475" width="0.1524" layer="20" curve="90.265883"/>
<wire x1="0.677265625" y1="17.479475" x2="0.677265625" y2="17.1855875" width="0.1524" layer="20"/>
<wire x1="1.769590625" y1="37.086928125" x2="4.311375" y2="39.628965625" width="0.1524" layer="20" curve="-90.099614"/>
<wire x1="4.311375" y1="39.628965625" x2="17.016296875" y2="39.6200375" width="0.1524" layer="20"/>
<wire x1="0.677265625" y1="17.1855875" x2="0.677265625" y2="17.058690625" width="0.1524" layer="20"/>
<wire x1="0.677265625" y1="17.058690625" x2="1.312265625" y2="16.423690625" width="0.1524" layer="20" curve="90"/>
<wire x1="1.312265625" y1="16.423690625" x2="1.523821875" y2="16.423690625" width="0.1524" layer="20"/>
<wire x1="1.523821875" y1="16.423690625" x2="1.777821875" y2="16.169690625" width="0.1524" layer="20" curve="-90"/>
<wire x1="1.777821875" y1="16.169690625" x2="1.777821875" y2="15.831084375" width="0.1524" layer="20"/>
<wire x1="1.777821875" y1="15.831084375" x2="1.777821875" y2="15.746425" width="0.1524" layer="20"/>
<wire x1="1.777821875" y1="15.746425" x2="1.777821875" y2="15.831084375" width="0.1524" layer="20"/>
<hole x="37.87" y="35.88" drill="3.5"/>
<text>github.com/alswnet/HelloALSW.git</text>
</plain>
<libraries>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_24.5MM">
</package>
<package name="KPS-1290">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BATT" library="SparkFun-Retired" package="BATTCON_24.5MM" value="3V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED" library="SparkFun-LED" package="LED-1206" value="BLUE">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09911"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08787"/>
<attribute name="VALUE"/>
</element>
<element name="SWITCH" library="SparkFun-Retired" package="KPS-1290" value="SWITCH_SPDT">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-10651"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="BATT" pad="1"/>
<contactref element="SWITCH" pad="O"/>
</signal>
<signal name="N$2">
<contactref element="SWITCH" pad="P"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="LED" pad="A"/>
</signal>
<signal name="GND">
<contactref element="BATT" pad="2"/>
<contactref element="LED" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
