<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="2.54" x2="25.38" y2="2.54" width="0" layer="20"/>
<wire x1="25.38" y1="2.54" x2="25.38" y2="25.832" width="0" layer="20"/>
<wire x1="25.38" y1="25.832" x2="0" y2="25.832" width="0" layer="20"/>
<wire x1="0" y1="25.832" x2="0" y2="2.54" width="0" layer="20"/>
<text>sourDough Boards
LM9022 VFD Filament PSU
Phantomic Labs 2017</text>
</plain>
<libraries>
<library name="Seeed-Capacitor">
<packages>
<package name="PC-D5.3MM">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="Fuzz01">
<description>Generated from &lt;b&gt;Fuzz01.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="ICS_SOP08">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_2.54_SCREWTERM">
<description>&lt;h3&gt;2 Pin Screw Terminal - 2.54mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Seeed-Resistor">
<packages>
<package name="R0805">
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C2.5-2">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 2.5 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="capacitor-wima" package="C2.5-2" value=".01uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Seeed-Capacitor" package="PC-D5.3MM" value="1uf">
<attribute name="MPN" value="KS 100uF/16V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Seeed-Capacitor" package="PC-D5.3MM" value="10uf">
<attribute name="MPN" value="KS 100uF/16V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Seeed-Capacitor" package="PC-D5.3MM" value=".1uf">
<attribute name="MPN" value="KS 100uF/16V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-1206" value="BLUE">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09911"/>
</element>
<element name="IC2" library="Fuzz01" package="ICS_SOP08" value="ICS_LM9022">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Seeed-Resistor" package="R0805" value="2.2K">
<attribute name="MPN" value="RC0805JR-072K2L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RL0805JR-070R1L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RL0805JR-070R1L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RL0805JR-070R1L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Seeed-Resistor" package="R0805" value="2.2K">
<attribute name="MPN" value="RL0805JR-070R1L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="Seeed-Resistor" package="R0805" value="0.1R">
<attribute name="MPN" value="RL0805JR-070R1L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Seeed-Resistor" package="R0805" value="470">
<attribute name="MPN" value="RL0805JR-070R1L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="8"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="2"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="GND">
<contactref element="R3" pad="1"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="1"/>
<contactref element="C2" pad="-"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="-"/>
<contactref element="J2" pad="P1"/>
<contactref element="C4" pad="-"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="R2" pad="2"/>
<contactref element="IC2" pad="6"/>
<contactref element="C3" pad="+"/>
<contactref element="J2" pad="P2"/>
<contactref element="C4" pad="+"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="P1"/>
</signal>
<signal name="N$10">
<contactref element="R6" pad="2"/>
<contactref element="J1" pad="P2"/>
</signal>
<signal name="N$14">
<contactref element="R7" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
