<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="1.24913125" y1="10.004425" x2="40.45665625" y2="10.004425" width="0" layer="20"/>
<wire x1="41.58" y1="16.51891875" x2="41.58" y2="49.9706875" width="0" layer="20"/>
<wire x1="38.2206875" y1="53.33" x2="3.5850375" y2="53.33" width="0" layer="20"/>
<wire x1="0" y1="49.7449625" x2="0" y2="11.2776" width="0" layer="20"/>
<text>evilgeniuslabs.org</text>
<text>D8</text>
<text>D7</text>
<text>D6</text>
<text>D5</text>
<text>G</text>
<text>G</text>
<text>GND</text>
<text>5V</text>
<text>5V</text>
<text>GND</text>
<text>5V</text>
<text>D4</text>
<text>D3</text>
<text>D2</text>
<text>D1</text>
<text>RX</text>
<text>TX</text>
<text>3V3</text>
<text>D8</text>
<text>D7</text>
<text>D6</text>
<text>D5</text>
<text>D0</text>
<text>A0</text>
<text>RST</text>
<text>Antenna</text>
<text>Wemos D1 Mini 6x
Level Shifter Shield v1.4
evilgeniuslabs.org</text>
<text>TX</text>
<text>RX</text>
<text>D1</text>
<text>D2</text>
<text>D3</text>
<text>D4</text>
<text>GND</text>
<text>5V</text>
<text>RST</text>
<text>A0</text>
<text>D0</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>D8</text>
<text>3V3</text>
<text>D8</text>
<text>GND</text>
<text>D7</text>
<text>5V</text>
<text>D6</text>
<text>G</text>
<text>D5</text>
<text>5V</text>
<text>Antenna</text>
<wire x1="0" y1="11.2776" x2="1.27" y2="10.0076" width="0" layer="20" curve="90"/>
<wire x1="41.5798" y1="16.5608" x2="41.5798" y2="11.2776" width="0" layer="20"/>
<wire x1="41.5798" y1="11.2776" x2="40.3098" y2="10.0076" width="0" layer="20" curve="-90"/>
<wire x1="0.0254" y1="49.7078" x2="0.0254" y2="52.07" width="0" layer="20"/>
<wire x1="0.0254" y1="52.07" x2="1.2954" y2="53.34" width="0" layer="20" curve="-90"/>
<wire x1="1.2954" y1="53.34" x2="3.683" y2="53.34" width="0" layer="20"/>
<wire x1="38.2016" y1="53.34" x2="40.3098" y2="53.34" width="0" layer="20"/>
<wire x1="40.3098" y1="53.34" x2="41.5798" y2="52.07" width="0" layer="20" curve="-90"/>
<wire x1="41.5798" y1="52.07" x2="41.5798" y2="49.8602" width="0" layer="20"/>
<text>D2</text>
<text>D1</text>
<text>D2</text>
<text>D1</text>
<text>G</text>
<text>Wemos D1 Mini 6x
Level Shifter Shield v1.4
evilgeniuslabs.org</text>
<text>SN74HCT245N</text>
<text>0.1uF</text>
<text>1000µF</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.1">
</package>
</packages>
</library>
<library name="1455413453956-wemos">
<packages>
<package name="WEMOS">
<description>WEMOS Controller socket</description>
</package>
</packages>
</library>
<library name="EH DIC-00289 - SN74HCT245 OCTAL BUS TRANSCEIVERS WITH 3-STATE OUTPUTS">
<packages>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector PTH&lt;/h3&gt;
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Barrel-Connector-PJ-202A.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -8 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-1000UF-25V" value="1000µF"/>
<element name="J1" library="SparkFun-Connectors" package="1X08_NO_SILK" value="J1">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X08_NO_SILK" value="J2">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω"/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω"/>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="1455413453956-wemos" package="WEMOS" value="WEMOS"/>
<element name="U$2" library="EH DIC-00289 - SN74HCT245 OCTAL BUS TRANSCEIVERS WITH 3-STATE OUTPUTS" package="DIL20" value="SN74HCT245N"/>
<element name="U$4" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="U$5" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="J8" library="SparkFun-Connectors" package="1X08_NO_SILK" value="J2">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X08_NO_SILK" value="J1">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="0.1uF"/>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω"/>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω"/>
<element name="J3" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACK">
<attribute name="PROD_ID" value="CONN-08197"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X06_NO_SILK" value="J4">
<attribute name="PROD_ID" value="CONN-08437"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X06_NO_SILK" value="J5">
<attribute name="PROD_ID" value="CONN-08437"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X06_NO_SILK" value="J6">
<attribute name="PROD_ID" value="CONN-08437"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="5V"/>
<contactref element="J1" pad="1"/>
<contactref element="C2" pad="+"/>
<contactref element="J9" pad="1"/>
<contactref element="U$2" pad="20"/>
<contactref element="C1" pad="1"/>
<contactref element="J3" pad="PWR"/>
<contactref element="J5" pad="6"/>
<contactref element="J5" pad="5"/>
<contactref element="J5" pad="4"/>
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="2"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$2" pad="19"/>
<contactref element="U$2" pad="1"/>
<contactref element="C2" pad="-"/>
<contactref element="J9" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="J3" pad="GND"/>
<contactref element="J3" pad="GNDBREAK"/>
<contactref element="J6" pad="6"/>
<contactref element="J6" pad="5"/>
<contactref element="J6" pad="4"/>
<contactref element="J6" pad="3"/>
<contactref element="J6" pad="2"/>
<contactref element="J6" pad="1"/>
<contactref element="U$2" pad="8"/>
<contactref element="U$2" pad="12"/>
<contactref element="U$2" pad="11"/>
<contactref element="U$2" pad="9"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="P$1"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="P$1"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="J2" pad="8"/>
<contactref element="U$1" pad="RST"/>
<contactref element="J8" pad="8"/>
</signal>
<signal name="A0">
<contactref element="U$1" pad="A0"/>
<contactref element="J2" pad="7"/>
<contactref element="J8" pad="7"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="3V3"/>
<contactref element="J2" pad="1"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="J1" pad="4"/>
<contactref element="U$1" pad="D3"/>
<contactref element="J9" pad="4"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="RX"/>
<contactref element="J1" pad="7"/>
<contactref element="J9" pad="7"/>
</signal>
<signal name="N$25">
<contactref element="J1" pad="8"/>
<contactref element="U$1" pad="TX"/>
<contactref element="J9" pad="8"/>
</signal>
<signal name="B1">
<contactref element="U$2" pad="18"/>
<contactref element="U$1" pad="D8"/>
<contactref element="J2" pad="2"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="B2">
<contactref element="U$2" pad="17"/>
<contactref element="U$1" pad="D7"/>
<contactref element="J2" pad="3"/>
<contactref element="J8" pad="3"/>
</signal>
<signal name="B3">
<contactref element="U$2" pad="16"/>
<contactref element="U$1" pad="D6"/>
<contactref element="J2" pad="4"/>
<contactref element="J8" pad="4"/>
</signal>
<signal name="B4">
<contactref element="U$2" pad="15"/>
<contactref element="U$1" pad="D5"/>
<contactref element="J2" pad="5"/>
<contactref element="J8" pad="5"/>
</signal>
<signal name="A1">
<contactref element="U$2" pad="2"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="A2">
<contactref element="U$2" pad="3"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="A3">
<contactref element="U$2" pad="4"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="A4">
<contactref element="U$2" pad="5"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="P$1"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="R4" pad="P$1"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="IR">
<contactref element="U$1" pad="D4"/>
<contactref element="J1" pad="3"/>
<contactref element="J9" pad="3"/>
</signal>
<signal name="D0">
<contactref element="J2" pad="6"/>
<contactref element="U$1" pad="D0"/>
<contactref element="J8" pad="6"/>
</signal>
<signal name="A5">
<contactref element="U$2" pad="6"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="A6">
<contactref element="U$2" pad="7"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="B6">
<contactref element="U$2" pad="13"/>
<contactref element="J1" pad="6"/>
<contactref element="U$1" pad="D1"/>
<contactref element="J9" pad="6"/>
</signal>
<signal name="B5">
<contactref element="U$2" pad="14"/>
<contactref element="U$1" pad="D2"/>
<contactref element="J1" pad="5"/>
<contactref element="J9" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="R5" pad="P$1"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R6" pad="P$1"/>
<contactref element="J4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
