<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="63.551" y2="-0.127" width="0" layer="20"/>
<wire x1="63.551" y1="-0.127" x2="63.424" y2="69.586" width="0" layer="20"/>
<wire x1="63.424" y1="69.586" x2="-0.127" y2="69.713" width="0" layer="20"/>
<wire x1="-0.127" y1="69.713" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMA-SMD">
<description>&lt;b&gt;SMA 50 Ohm Straight Jack Receptacle - Surface Mount&lt;/b&gt;&lt;p&gt;
www.johnsoncomponents.com&lt;br&gt;
Source:  http://catalog.digikey.com .. 142-0711-201, 205, 202, 206.pdf</description>
</package>
</packages>
</library>
<library name="TI_by_element14">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOT95P280X145-5N">
</package>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="fmc_zed">
<packages>
<package name="FMC-LPC-MALE">
<description>&lt;b&gt;FMC-LPC&lt;/b&gt;
&lt;p&gt;Outline and mounting holes consistent with Xilinx SP605 board&lt;/p&gt;
&lt;p&gt;http://www.samtec.com/search/vita57fmc.aspx&lt;/p&gt;
&lt;p&gt;http://www.samtec.com/documents/webfiles/Cpdf/ASP-127797-01.pdf&lt;/p&gt;
&lt;p&gt;ASP-127797-01 / MC-LPC-10L&lt;/p&gt;
&lt;p&gt;ASP-134604-01 / MC-LPC-10&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X5" library="con-coax" package="SMA-SMD" value="SMA-SMD">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X4" library="con-coax" package="SMA-SMD" value="SMA-SMD">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X3" library="con-coax" package="SMA-SMD" value="SMA-SMD">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X2" library="con-coax" package="SMA-SMD" value="SMA-SMD">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X1" library="con-coax" package="SMA-SMD" value="SMA-SMD">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="U2" library="TI_by_element14" package="SOT95P280X145-5N" value="SN65LVDT2DBVT">
<attribute name="MPN" value="SN65LVDT2DBVT"/>
<attribute name="OC_FARNELL" value="1575586"/>
<attribute name="OC_NEWARK" value="76C0822"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</element>
<element name="U1" library="TI_by_element14" package="SOT95P280X145-5N" value="SN65LVDT2DBVT">
<attribute name="MPN" value="SN65LVDT2DBVT"/>
<attribute name="OC_FARNELL" value="1575586"/>
<attribute name="OC_NEWARK" value="76C0822"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</element>
<element name="U3" library="TI_by_element14" package="SOT95P280X145-5N" value="SN65LVDT2DBVT">
<attribute name="MPN" value="SN65LVDT2DBVT"/>
<attribute name="OC_FARNELL" value="1575586"/>
<attribute name="OC_NEWARK" value="76C0822"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</element>
<element name="U4" library="TI_by_element14" package="SOT95P280X145-5N" value="SN65LVDT2DBVT">
<attribute name="MPN" value="SN65LVDT2DBVT"/>
<attribute name="OC_FARNELL" value="1575586"/>
<attribute name="OC_NEWARK" value="76C0822"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</element>
<element name="U5" library="TI_by_element14" package="SOIC127P600X175-8N" value="SN65LVDS100D">
<attribute name="MPN" value="SN65LVDS100D"/>
<attribute name="OC_FARNELL" value="8452393"/>
<attribute name="OC_NEWARK" value="02E6875"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="5.62k">
<attribute name="PROD_ID" value="RES-09823"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="5.62k">
<attribute name="PROD_ID" value="RES-09823"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="15pF">
<attribute name="PROD_ID" value="CAP-07881"/>
</element>
<element name="J1" library="fmc_zed" package="FMC-LPC-MALE" value="FMC-LPC"/>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="2.2k">
<attribute name="PROD_ID" value="RES-09823"/>
</element>
<element name="C6" library="SparkFun-Passives" package="0603-CAP" value="1uF"/>
<element name="C10" library="SparkFun-Passives" package="0603-CAP" value="1uF"/>
<element name="C14" library="SparkFun-Passives" package="0603-CAP" value="1uF"/>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="1uF"/>
<element name="C18" library="SparkFun-Passives" package="0603-CAP" value="1uF"/>
<element name="C4" library="SparkFun-Capacitors" package="1206" value="10uF"/>
<element name="C8" library="SparkFun-Capacitors" package="1206" value="10uF"/>
<element name="C12" library="SparkFun-Capacitors" package="1206" value="10uF"/>
<element name="C16" library="SparkFun-Capacitors" package="1206" value="10uF"/>
<element name="C20" library="SparkFun-Capacitors" package="1206" value="10uF"/>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
<element name="C7" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
<element name="C11" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
<element name="C15" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
<element name="C19" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="1nF"/>
<element name="C9" library="SparkFun-Capacitors" package="0603-CAP" value="1nF"/>
<element name="C13" library="SparkFun-Capacitors" package="0603-CAP" value="1nF"/>
<element name="C17" library="SparkFun-Capacitors" package="0603-CAP" value="1nF"/>
<element name="C21" library="SparkFun-Capacitors" package="0603-CAP" value="1nF"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="U5" pad="8"/>
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="J1" pad="C39"/>
<contactref element="J1" pad="D38"/>
<contactref element="J1" pad="D40"/>
<contactref element="J1" pad="D36"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="U5" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U5" pad="5"/>
<contactref element="X1" pad="2@4"/>
<contactref element="X1" pad="2@5"/>
<contactref element="X1" pad="2@2"/>
<contactref element="X1" pad="2@3"/>
<contactref element="X1" pad="2@6"/>
<contactref element="X1" pad="2@1"/>
<contactref element="X5" pad="2@4"/>
<contactref element="X5" pad="2@5"/>
<contactref element="X5" pad="2@2"/>
<contactref element="X5" pad="2@3"/>
<contactref element="X5" pad="2@6"/>
<contactref element="X5" pad="2@1"/>
<contactref element="X4" pad="2@4"/>
<contactref element="X4" pad="2@5"/>
<contactref element="X4" pad="2@2"/>
<contactref element="X4" pad="2@3"/>
<contactref element="X4" pad="2@6"/>
<contactref element="X4" pad="2@1"/>
<contactref element="X3" pad="2@4"/>
<contactref element="X3" pad="2@5"/>
<contactref element="X3" pad="2@2"/>
<contactref element="X3" pad="2@3"/>
<contactref element="X3" pad="2@6"/>
<contactref element="X3" pad="2@1"/>
<contactref element="X2" pad="2@4"/>
<contactref element="X2" pad="2@5"/>
<contactref element="X2" pad="2@2"/>
<contactref element="X2" pad="2@3"/>
<contactref element="X2" pad="2@6"/>
<contactref element="X2" pad="2@1"/>
<contactref element="U4" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="C1"/>
<contactref element="J1" pad="C4"/>
<contactref element="J1" pad="C5"/>
<contactref element="J1" pad="C8"/>
<contactref element="J1" pad="C9"/>
<contactref element="J1" pad="C12"/>
<contactref element="J1" pad="C13"/>
<contactref element="J1" pad="C16"/>
<contactref element="J1" pad="C17"/>
<contactref element="J1" pad="C20"/>
<contactref element="J1" pad="C21"/>
<contactref element="J1" pad="C24"/>
<contactref element="J1" pad="C25"/>
<contactref element="J1" pad="C28"/>
<contactref element="J1" pad="C29"/>
<contactref element="J1" pad="C32"/>
<contactref element="J1" pad="C33"/>
<contactref element="J1" pad="C36"/>
<contactref element="J1" pad="C38"/>
<contactref element="J1" pad="C40"/>
<contactref element="J1" pad="D2"/>
<contactref element="J1" pad="D3"/>
<contactref element="J1" pad="D6"/>
<contactref element="J1" pad="D7"/>
<contactref element="J1" pad="D10"/>
<contactref element="J1" pad="D13"/>
<contactref element="J1" pad="D16"/>
<contactref element="J1" pad="D19"/>
<contactref element="J1" pad="D22"/>
<contactref element="J1" pad="D25"/>
<contactref element="J1" pad="D28"/>
<contactref element="J1" pad="D37"/>
<contactref element="J1" pad="D39"/>
<contactref element="J1" pad="G1"/>
<contactref element="J1" pad="G4"/>
<contactref element="J1" pad="G5"/>
<contactref element="J1" pad="G8"/>
<contactref element="J1" pad="G11"/>
<contactref element="J1" pad="G14"/>
<contactref element="J1" pad="G17"/>
<contactref element="J1" pad="G20"/>
<contactref element="J1" pad="G23"/>
<contactref element="J1" pad="G26"/>
<contactref element="J1" pad="G29"/>
<contactref element="J1" pad="G32"/>
<contactref element="J1" pad="G35"/>
<contactref element="J1" pad="G38"/>
<contactref element="J1" pad="G40"/>
<contactref element="J1" pad="H3"/>
<contactref element="J1" pad="H6"/>
<contactref element="J1" pad="H9"/>
<contactref element="J1" pad="H12"/>
<contactref element="J1" pad="H15"/>
<contactref element="J1" pad="H18"/>
<contactref element="J1" pad="H21"/>
<contactref element="J1" pad="H24"/>
<contactref element="J1" pad="H27"/>
<contactref element="J1" pad="H30"/>
<contactref element="J1" pad="H33"/>
<contactref element="J1" pad="H36"/>
<contactref element="J1" pad="H39"/>
<contactref element="R3" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C18" pad="2"/>
</signal>
<signal name="SMA_IN">
<contactref element="X1" pad="1"/>
<contactref element="U5" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SMA_OUT1">
<contactref element="X2" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="SMA_OUT2">
<contactref element="X3" pad="1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="SMA_OUT3">
<contactref element="X4" pad="1"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="SMA_OUT4">
<contactref element="X5" pad="1"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="2"/>
<contactref element="J1" pad="H2"/>
</signal>
<signal name="SMA_IN_M_N">
<contactref element="U5" pad="6"/>
<contactref element="J1" pad="C23"/>
</signal>
<signal name="SMA_IN_M_P">
<contactref element="U5" pad="7"/>
<contactref element="J1" pad="C22"/>
</signal>
<signal name="SMA_OUTM2_N">
<contactref element="U2" pad="4"/>
<contactref element="J1" pad="H11"/>
</signal>
<signal name="SMA_OUTM3_P">
<contactref element="U3" pad="3"/>
<contactref element="J1" pad="H13"/>
</signal>
<signal name="SMA_OUTM3_N">
<contactref element="U3" pad="4"/>
<contactref element="J1" pad="H14"/>
</signal>
<signal name="SMA_OUTM2_P">
<contactref element="U2" pad="3"/>
<contactref element="J1" pad="H10"/>
</signal>
<signal name="SMA_OUTM1_P">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="H7"/>
</signal>
<signal name="SMA_OUTM1_N">
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="H8"/>
</signal>
<signal name="SMA_OUTM4_P">
<contactref element="U4" pad="3"/>
<contactref element="J1" pad="H16"/>
</signal>
<signal name="SMA_OUTM4_N">
<contactref element="U4" pad="4"/>
<contactref element="J1" pad="H17"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
