<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="7.62" y1="59.6799625" x2="7.62" y2="5.60605" width="0" layer="20"/>
<wire x1="7.62" y1="5.60605" x2="9.41605" y2="3.81" width="0" layer="20" curve="90"/>
<wire x1="9.41605" y1="3.81" x2="41.26996875" y2="3.81" width="0" layer="20"/>
<wire x1="41.26996875" y1="3.81" x2="42.85" y2="5.39003125" width="0" layer="20" curve="90"/>
<wire x1="42.85" y1="5.39003125" x2="42.85" y2="59.377996875" width="0" layer="20"/>
<wire x1="42.85" y1="59.377996875" x2="41.277996875" y2="60.95" width="0" layer="20" curve="90"/>
<wire x1="41.277996875" y1="60.95" x2="8.8900375" y2="60.95" width="0" layer="20"/>
<wire x1="8.8900375" y1="60.95" x2="7.62" y2="59.6799625" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X13-SHROUDED">
</package>
</packages>
</library>
<library name="Seeed-OPL-Connector">
<packages>
<package name="HW4-2.0-90D">
</package>
<package name="HW4-2.0">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Boards" package="2X13-SHROUDED" value="RASPBERRYPI-GPIOPTH">
<attribute name="DIST" value="sparkfun"/>
<attribute name="DIST_ID" value="PRT-11490"/>
</element>
<element name="I2C3" library="Seeed-OPL-Connector" package="HW4-2.0-90D" value="4P-2.0-90D"/>
<element name="I2C1" library="Seeed-OPL-Connector" package="HW4-2.0-90D" value="4P-2.0-90D"/>
<element name="I2C2" library="Seeed-OPL-Connector" package="HW4-2.0-90D" value="4P-2.0-90D"/>
<element name="GPIO_18_22" library="Seeed-OPL-Connector" package="HW4-2.0" value="4P-2.0"/>
<element name="GPIO_22_23" library="Seeed-OPL-Connector" package="HW4-2.0" value="4P-2.0"/>
<element name="GPIO_4_17" library="Seeed-OPL-Connector" package="HW4-2.0" value="4P-2.0"/>
<element name="GPIO_17_18" library="Seeed-OPL-Connector" package="HW4-2.0" value="4P-2.0"/>
<element name="SERIAL" library="Seeed-OPL-Connector" package="HW4-2.0-90D" value="4P-2.0-90D"/>
<element name="I2C4" library="Seeed-OPL-Connector" package="HW4-2.0-90D" value="4P-2.0-90D"/>
<element name="3.3V_5V" library="SparkFun-Retired" package="1X03" value="JUMPER-3PTH"/>
<element name="GPIO_23_24" library="Seeed-OPL-Connector" package="HW4-2.0" value="4P-2.0"/>
<element name="GPIO_24_25" library="Seeed-OPL-Connector" package="HW4-2.0" value="4P-2.0"/>
<element name="GPIO_25_27" library="Seeed-OPL-Connector" package="HW4-2.0" value="4P-2.0"/>
</elements>
<signals>
<signal name="GP4">
<contactref element="J1" pad="7"/>
<contactref element="GPIO_4_17" pad="1"/>
</signal>
<signal name="GP17">
<contactref element="J1" pad="11"/>
<contactref element="GPIO_4_17" pad="2"/>
<contactref element="GPIO_17_18" pad="1"/>
</signal>
<signal name="GP18#">
<contactref element="J1" pad="12"/>
<contactref element="GPIO_17_18" pad="2"/>
<contactref element="GPIO_18_22" pad="1"/>
</signal>
<signal name="GP22">
<contactref element="J1" pad="15"/>
<contactref element="GPIO_18_22" pad="2"/>
<contactref element="GPIO_22_23" pad="1"/>
</signal>
<signal name="GP23">
<contactref element="J1" pad="16"/>
<contactref element="GPIO_22_23" pad="2"/>
<contactref element="GPIO_23_24" pad="1"/>
</signal>
<signal name="GP24">
<contactref element="J1" pad="18"/>
<contactref element="GPIO_23_24" pad="2"/>
<contactref element="GPIO_24_25" pad="1"/>
</signal>
<signal name="GP25">
<contactref element="J1" pad="22"/>
<contactref element="GPIO_24_25" pad="2"/>
<contactref element="GPIO_25_27" pad="1"/>
</signal>
<signal name="GP27">
<contactref element="J1" pad="13"/>
<contactref element="GPIO_25_27" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="17"/>
<contactref element="3.3V_5V" pad="1"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="2"/>
<contactref element="3.3V_5V" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="5"/>
<contactref element="I2C3" pad="1"/>
<contactref element="I2C2" pad="1"/>
<contactref element="I2C1" pad="1"/>
<contactref element="I2C4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="3"/>
<contactref element="I2C3" pad="2"/>
<contactref element="I2C2" pad="2"/>
<contactref element="I2C1" pad="2"/>
<contactref element="I2C4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="10"/>
<contactref element="SERIAL" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="8"/>
<contactref element="SERIAL" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="14"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="9"/>
<contactref element="J1" pad="20"/>
<contactref element="J1" pad="25"/>
<contactref element="GPIO_25_27" pad="4"/>
<contactref element="GPIO_24_25" pad="4"/>
<contactref element="GPIO_23_24" pad="4"/>
<contactref element="GPIO_22_23" pad="4"/>
<contactref element="GPIO_18_22" pad="4"/>
<contactref element="I2C1" pad="4"/>
<contactref element="I2C2" pad="4"/>
<contactref element="I2C3" pad="4"/>
<contactref element="GPIO_17_18" pad="4"/>
<contactref element="GPIO_4_17" pad="4"/>
<contactref element="I2C4" pad="4"/>
<contactref element="SERIAL" pad="4"/>
</signal>
<signal name="VDD">
<contactref element="GPIO_24_25" pad="3"/>
<contactref element="3.3V_5V" pad="2"/>
<contactref element="SERIAL" pad="3"/>
<contactref element="I2C4" pad="3"/>
<contactref element="I2C3" pad="3"/>
<contactref element="I2C2" pad="3"/>
<contactref element="I2C1" pad="3"/>
<contactref element="GPIO_18_22" pad="3"/>
<contactref element="GPIO_22_23" pad="3"/>
<contactref element="GPIO_23_24" pad="3"/>
<contactref element="GPIO_25_27" pad="3"/>
<contactref element="GPIO_17_18" pad="3"/>
<contactref element="GPIO_4_17" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
