<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.2">
<drawing>
<board>
<plain>
<text>https://goo.gl/nvudE9</text>
<hole x="15.238475" y="50.79491875" drill="3.197859375"/>
<hole x="66.033396875" y="35.55644375" drill="3.197859375"/>
<hole x="66.033396875" y="7.6192375" drill="3.197859375"/>
<hole x="13.968603125" y="2.539746875" drill="3.197859375"/>
<text>Credit to Z-Hut_arduino</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SO08">
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="ARDUINOR3">
<description>The new Arduino R3 'classic' adds duplicate I2C pins and an IORef pin (and an unused pin</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Large - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="PANASONIC_C" value=""/>
<element name="C2" library="adafruit" package="C0603" value=""/>
<element name="IC1" library="adafruit" package="SO08" value="LM555D"/>
<element name="LED1" library="adafruit" package="CHIPLED_1206" value=""/>
<element name="R1" library="adafruit" package="R1206" value=""/>
<element name="R2" library="adafruit" package="R1206" value=""/>
<element name="R3" library="adafruit" package="R1206" value=""/>
<element name="U1" library="adafruit" package="ARDUINOR3" value="ARDUINOR3-DIMENSION"/>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="GND"/>
<contactref element="U1" pad="GND1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="U1" pad="GND2"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="VIN"/>
</signal>
<signal name="3V">
<contactref element="U1" pad="3V"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="5V"/>
<contactref element="IC1" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="D11"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="5"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
