<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="66.02" y2="0" width="0" layer="20"/>
<wire x1="66.02" y1="0" x2="66.02" y2="87.3" width="0" layer="20"/>
<wire x1="66.02" y1="87.3" x2="0" y2="87.3" width="0" layer="20"/>
<wire x1="0" y1="87.3" x2="0" y2="0" width="0" layer="20"/>
<text>IN</text>
<text>OUT</text>
<text>5V</text>
<text>3.3V</text>
<text>REVA</text>
</plain>
<libraries>
<library name="DUElib130425">
<packages>
<package name="DUE(NORMAL)">
</package>
</packages>
</library>
<library name="_hhn_78xx_79xx_NCV78xx_d2pak_dpak">
<description>&lt;h2&gt;78xx 79xx NCV78xx SMD (D2PAK, DPAK)&lt;/h2&gt;
&lt;p&gt;&lt;b&gt;Linear Voltage Regulators&lt;/b&gt;&lt;/p&gt;
Source: ONSEMI (http://onsemi.com)&lt;br /&gt;
&lt;hr&gt;
&lt;p&gt;&lt;i&gt;Author: Dipl.-Ing. FH Rainer Bayer&lt;br /&gt;
HHN Hochschule Heilbronn, rainer.bayer@hs-heilbronn.de&lt;br /&gt;
Ingenieurbüro ing-rb, mail@ing-rb.de&lt;/p&gt;</description>
<packages>
<package name="D2PAK-3">
<description>&lt;b&gt;D2PAK-3&lt;/b&gt; (acc. to. ON Semiconductor specs)</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_2.54_SCREWTERM">
<description>&lt;h3&gt;2 Pin Screw Terminal - 2.54mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0402-TIGHT">
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA05-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="DUElib130425" package="DUE(NORMAL)" value="DUE(NORMAL)"/>
<element name="U2" library="_hhn_78xx_79xx_NCV78xx_d2pak_dpak" package="D2PAK-3" value="MC7805ACD2T"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.33µF">
<attribute name="PROD_ID" value="CAP-08469"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0402-TIGHT" value="0.1uF">
<attribute name="PROD_ID" value="CAP-12416"/>
</element>
<element name="AD7734" library="con-lstb" package="MA05-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="14"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="15V"/>
<element name="J2" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="5V"/>
<element name="J3" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="3.3V"/>
<element name="J4" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="5V"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND_A"/>
<contactref element="U$1" pad="GND_B"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$1" pad="5V_ICSP"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="J2" pad="P2"/>
<contactref element="J3" pad="P1"/>
<contactref element="J4" pad="P1"/>
<contactref element="U$1" pad="GND_1"/>
<contactref element="U$1" pad="GND_2"/>
<contactref element="J1" pad="P1"/>
</signal>
<signal name="VOUT">
<contactref element="U2" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="J2" pad="P1"/>
</signal>
<signal name="RDY">
<contactref element="AD7734" pad="8"/>
<contactref element="U$1" pad="34"/>
</signal>
<signal name="CS">
<contactref element="AD7734" pad="6"/>
<contactref element="U$1" pad="30"/>
</signal>
<signal name="RESET">
<contactref element="AD7734" pad="4"/>
<contactref element="U$1" pad="26"/>
</signal>
<signal name="MOSI">
<contactref element="AD7734" pad="2"/>
<contactref element="U$1" pad="MOSI_ICSP"/>
</signal>
<signal name="MISO">
<contactref element="AD7734" pad="7"/>
<contactref element="U$1" pad="MISO_ICSP"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="SCK_ICSP"/>
<contactref element="AD7734" pad="10"/>
</signal>
<signal name="N$1">
<contactref element="J3" pad="P2"/>
<contactref element="U$1" pad="3V3"/>
</signal>
<signal name="N$4">
<contactref element="J4" pad="P2"/>
<contactref element="U$1" pad="5V"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="P2"/>
<contactref element="U2" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
