<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="21.59" y2="0" width="0" layer="20"/>
<wire x1="21.59" y1="0" x2="21.59" y2="43.18" width="0" layer="20"/>
<wire x1="0" y1="43.18" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="43.18" x2="21.59" y2="43.18" width="0" layer="20"/>
<text>OUT</text>
<text>IN</text>
<text>NE5U
DC-DC
Supply</text>
<text>NE5U</text>
<text>Power 
Indicator
LED</text>
</plain>
<libraries>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD2,54-5,08">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="D2PACK/A">
<description>&lt;h3&gt;D&lt;sup&gt;2&lt;/sup&gt;PAK/A V-reg Package&lt;/h3&gt;
3-pins w/ tab&lt;br&gt;&lt;br&gt;
&lt;b&gt;***Unproven***&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;b&gt;Used on:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;LD1085xx Adjustable 3A Regulator
&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="153CLV-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0605">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_3MM">
<description>&lt;h3&gt;LED 3MM PTH&lt;/h3&gt;

3 mm, round.

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="153CLV-0605" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="1206" value="1kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="1206" value="3.01kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,0" value="3mm"/>
<element name="H2" library="holes" package="3,0" value="3mm"/>
<element name="PAD1" library="wirepad" package="SMD2,54-5,08" value="IN+">
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="SMD2,54-5,08" value="5VOUT+">
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="SMD2,54-5,08" value="IN-">
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad" package="SMD2,54-5,08" value="5VOUT-">
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="D2PACK/A" value="LD1085D2">
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="153CLV-0810" value="220µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="1206" value="150Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STATUS" library="SparkFun-LED" package="LED_3MM" value="RED">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="ADJ">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="PAD3" pad="1"/>
<contactref element="PAD4" pad="1"/>
<contactref element="C3" pad="-"/>
<contactref element="STATUS" pad="K"/>
</signal>
<signal name="IN">
<contactref element="C1" pad="+"/>
<contactref element="PAD1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="OUT">
<contactref element="R1" pad="2"/>
<contactref element="PAD2" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="TAB"/>
<contactref element="C3" pad="+"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="1"/>
<contactref element="STATUS" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
