<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.2">
<drawing>
<board>
<plain>
<wire x1="6.35" y1="0" x2="50.927" y2="0" width="0" layer="20"/>
<wire x1="54.102" y1="3.175" x2="54.102" y2="22.606" width="0" layer="20"/>
<wire x1="47.752" y1="28.956" x2="3.175" y2="28.956" width="0" layer="20"/>
<hole x="17.018" y="26.162" drill="2.54"/>
<hole x="37.084" y="2.54" drill="2.54"/>
<wire x1="3.175" y1="6.35" x2="0" y2="6.35" width="0" layer="20"/>
<wire x1="0" y1="6.35" x2="0" y2="25.781" width="0" layer="20"/>
<wire x1="6.35" y1="0" x2="6.35" y2="3.175" width="0" layer="20"/>
<wire x1="47.752" y1="28.956" x2="47.752" y2="25.781" width="0" layer="20"/>
<hole x="3.175" y="19.558" drill="3.175"/>
<hole x="3.175" y="9.398" drill="3.175"/>
<text>VIN
GPS RX
GPS TX
GND</text>
<wire x1="50.927" y1="22.606" x2="54.102" y2="22.606" width="0" layer="20"/>
<wire x1="6.35" y1="3.175" x2="3.175" y2="6.35" width="0" layer="20" curve="90"/>
<wire x1="47.752" y1="25.781" x2="50.927" y2="22.606" width="0" layer="20" curve="90"/>
<wire x1="29.5275" y1="2.032" x2="10.16" y2="2.032" width="0" layer="20"/>
<wire x1="10.16" y1="2.032" x2="10.16" y2="21.59" width="0" layer="20"/>
<wire x1="10.16" y1="21.59" x2="29.5275" y2="21.59" width="0" layer="20"/>
<wire x1="29.5275" y1="21.59" x2="29.5275" y2="2.032" width="0" layer="20"/>
<wire x1="3.175" y1="28.956" x2="0" y2="25.781" width="0" layer="20" curve="90"/>
<wire x1="50.927" y1="0" x2="54.102" y2="3.175" width="0" layer="20" curve="90"/>
<text>CUT OUT</text>
</plain>
<libraries>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DPAK">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LONGPADS">
</package>
</packages>
</library>
<library name="SUP800F">
<packages>
<package name="SUP800F">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_12MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="." library="SparkFun-Connectors" package="1X04_LONGPADS" value=""/>
<element name="U$1" library="SparkFun-PowerIC" package="DPAK" value="LM2931_FIXED"/>
<element name="U$2" library="SUP800F" package="SUP800F" value="SUP800F_GPS"/>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCON_12MM" value="">
<attribute name="PROD_ID" value="BATT-08044"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="." pad="4"/>
<contactref element="U$2" pad="GND"/>
<contactref element="BAT1" pad="GND"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="12V">
<contactref element="." pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="GPS_RX">
<contactref element="." pad="2"/>
<contactref element="U$2" pad="RX"/>
</signal>
<signal name="GPS_TX">
<contactref element="." pad="3"/>
<contactref element="U$2" pad="TX"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="VIN"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="BAT1" pad="PWR@1"/>
<contactref element="U$2" pad="VBAT"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
