<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="39.548" y2="0" width="0" layer="20"/>
<wire x1="39.548" y1="0" x2="39.548" y2="11.166" width="0" layer="20"/>
<wire x1="39.548" y1="11.166" x2="0" y2="11.166" width="0" layer="20"/>
<wire x1="0" y1="11.166" x2="0" y2="0" width="0" layer="20"/>
<hole x="15.24" y="5.588" drill="3.19999375"/>
<text>U1</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>LED</text>
<text>LED</text>
<text>LED</text>
<text>LED</text>
<text>COL</text>
<text>COL</text>
<text>COL</text>
<text>COL</text>
<text>3.3V</text>
<text>GND</text>
<text>ENC_A</text>
<text>ENC_B</text>
<text>WHEEL_ENCODER V2</text>
<text>2013-04-23</text>
</plain>
<libraries>
<library name="jleichty">
<packages>
<package name="HLC1395">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOT95P280X145-6N">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LONGPADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1A" library="jleichty" package="HLC1395" value="HLC1395"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Texas Instruments_By_element14_Batch_1" package="SOT95P280X145-6N" value="SN74LVC2G17DBVR">
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="OC_NEWARK" value="76C4207"/>
<attribute name="MPN" value="SN74LVC2G17DBVR"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="1470776"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="S1D" library="jleichty" package="HLC1395" value="HLC1395"/>
<element name="S2A" library="jleichty" package="HLC1395" value="HLC1395"/>
<element name="R2" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="S2D" library="jleichty" package="HLC1395" value="HLC1395"/>
</elements>
<signals>
<signal name="GND">
<contactref element="S1A" pad="2"/>
<contactref element="S1D" pad="2"/>
<contactref element="S2A" pad="2"/>
<contactref element="S2D" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="S1A" pad="1"/>
<contactref element="S1D" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="COL1">
<contactref element="S1A" pad="3"/>
<contactref element="S1D" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="S2A" pad="1"/>
<contactref element="S2D" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="COL2">
<contactref element="S2A" pad="3"/>
<contactref element="S2D" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="OUT1">
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="OUT2">
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
