<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="-1.447328125" y1="42.915715625" x2="-1.42465" y2="23.293803125" width="0" layer="20"/>
<wire x1="-1.42465" y1="23.293803125" x2="-0.78323125" y2="22.7161625" width="0" layer="20" curve="89.933812"/>
<wire x1="-0.78323125" y1="22.7161625" x2="23.49881875" y2="22.7161625" width="0" layer="20"/>
<wire x1="23.49881875" y1="22.7161625" x2="24.28000625" y2="23.591228125" width="0" layer="20" curve="89.993129"/>
<wire x1="24.28000625" y1="23.591228125" x2="24.25778125" y2="42.82108125" width="0" layer="20"/>
<wire x1="24.25778125" y1="42.82108125" x2="23.753178125" y2="43.324" width="0" layer="20" curve="89.933291"/>
<wire x1="23.753178125" y1="43.324" x2="-1.039571875" y2="43.324" width="0" layer="20"/>
<wire x1="-1.039571875" y1="43.324" x2="-1.447328125" y2="42.915715625" width="0" layer="20" curve="90.074209"/>
<text>Res</text>
<text>A0</text>
<text>D0</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>D8</text>
<text>3V3</text>
<text>TX</text>
<text>RX</text>
<text>D1</text>
<text>D2</text>
<text>D3</text>
<text>D4</text>
<text>GND</text>
<text>5V</text>
<text>By Chris 01/02/18 </text>
<text>V1.00</text>
<text>D5</text>
<text>3V3</text>
<text>GND</text>
</plain>
<libraries>
<library name="cny70">
<packages>
<package name="4">
</package>
</packages>
</library>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOT95P280X145-5N">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
<package name="1X03">
</package>
</packages>
</library>
<library name="Ava">
<packages>
<package name="DS1820">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA6032">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="cny70" package="4" value="CNY70">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Texas Instruments_By_element14_Batch_1" package="SOT95P280X145-5N" value="SN74LVC1G17DBVR">
<attribute name="MPN" value="SN74LVC1G17DBVR"/>
<attribute name="OC_FARNELL" value="1470773"/>
<attribute name="OC_NEWARK" value="76C4089"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="3.3 k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="Ava" package="DS1820" value="DS1820TO92"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="4.7 k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="EIA6032" value="47 µF"/>
<element name="JP3" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="E"/>
<contactref element="U$1" pad="K"/>
<contactref element="U1" pad="3"/>
<contactref element="LED2" pad="C"/>
<contactref element="JP1" pad="2"/>
<contactref element="U$2" pad="GND"/>
<contactref element="C1" pad="P$2"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="D2">
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="A"/>
</signal>
<signal name="N$22">
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="C"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="R4" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="3V3">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="LED1" pad="A"/>
<contactref element="JP2" pad="8"/>
<contactref element="U$2" pad="VDD"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="P$1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="A0">
<contactref element="JP2" pad="2"/>
</signal>
<signal name="D0">
<contactref element="JP2" pad="3"/>
</signal>
<signal name="D5">
<contactref element="JP2" pad="4"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="D6">
<contactref element="JP2" pad="5"/>
<contactref element="U1" pad="4"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="D7">
<contactref element="JP2" pad="6"/>
</signal>
<signal name="D8">
<contactref element="JP2" pad="7"/>
</signal>
<signal name="RESET">
<contactref element="JP2" pad="1"/>
</signal>
<signal name="D4">
<contactref element="JP1" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="DQ"/>
</signal>
<signal name="D3">
<contactref element="JP1" pad="4"/>
</signal>
<signal name="D1">
<contactref element="JP1" pad="6"/>
</signal>
<signal name="DX">
<contactref element="JP1" pad="7"/>
</signal>
<signal name="TX">
<contactref element="JP1" pad="8"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
