<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="28.956" y2="0" width="0" layer="20"/>
<wire x1="28.956" y1="0" x2="28.956" y2="40.64" width="0" layer="20"/>
<wire x1="28.956" y1="40.64" x2="0" y2="40.64" width="0" layer="20"/>
<wire x1="0" y1="40.64" x2="0" y2="0" width="0" layer="20"/>
<text>BC548B</text>
<text>BC558B</text>
<text>1K</text>
<text>Type 1</text>
<text>INPUT</text>
<text>680</text>
<text>220</text>
<text>100nF</text>
<text>+5V</text>
<text>VI</text>
<text>GND</text>
<text>GND</text>
<text>AI</text>
<text>AO</text>
<text>VO</text>
<text>Ikrananka - Apr 2019 (v1.1)</text>
<hole x="15.477996875" y="35.4584" drill="4.953"/>
<hole x="13.4780125" y="5.45591875" drill="4.953"/>
<text>Video Mod</text>
<text>Composite</text>
<text>Odyssey 2</text>
<text>OUTPUT</text>
<text>Type 1</text>
<text>Video Mod</text>
<text>Composite</text>
<text>Odyssey 2</text>
<text>This side
visible
when
installed</text>
<text>Ikrananka
Apr 2019
(v1.1)</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL2">
</package>
</packages>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92-EBC">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
 grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="transistor-pnp">
<description>&lt;b&gt;PNP Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92-EBC">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2031">
<description>&lt;b&gt;KK® 254 Solid Header, Vertical, with Friction Lock, 3 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/022232031_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="22-23-2041">
<description>&lt;b&gt;KK® 254 Solid Header, Vertical, with Friction Lock, 4 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/022232041_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CT6">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="Q1" library="transistor-npn" package="TO92-EBC" value="BC548B"/>
<element name="Q2" library="transistor-pnp" package="TO92-EBC" value="BC558B"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="680">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="X2" library="con-molex" package="22-23-2031" value="22-23-2031">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2031"/>
<attribute name="OC_FARNELL" value="1462950"/>
<attribute name="OC_NEWARK" value="30C0862"/>
</element>
<element name="X1" library="con-molex" package="22-23-2041" value="22-23-2041">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2041"/>
<attribute name="OC_FARNELL" value="1462920"/>
<attribute name="OC_NEWARK" value="38C0355"/>
</element>
<element name="R3" library="pot" package="CT6" value="1K"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="Q2" pad="B"/>
<contactref element="Q1" pad="C"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="AUDIO">
<contactref element="X2" pad="3"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="X2" pad="2"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="VI">
<contactref element="Q1" pad="B"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="Q2" pad="E"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="P$2"/>
<contactref element="Q1" pad="E"/>
<contactref element="R3" pad="S"/>
</signal>
<signal name="VO">
<contactref element="Q2" pad="C"/>
<contactref element="X2" pad="1"/>
<contactref element="R3" pad="E"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
