<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="20.3" y2="0" width="0" layer="20"/>
<wire x1="20.3" y1="0" x2="20.3" y2="23.8" width="0" layer="20"/>
<wire x1="20.3" y1="23.8" x2="0" y2="23.8" width="0" layer="20"/>
<wire x1="0" y1="23.8" x2="0" y2="0" width="0" layer="20"/>
<text>This board was 
designed by osok</text>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,15/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CS" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MISO" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MOSI" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HOLD" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SCK" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-DigitalIC" package="SO08" value="W25Q##BV">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="VCC" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="WP" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
</elements>
<signals>
<signal name="PIN1">
<contactref element="U1" pad="1"/>
<contactref element="CS" pad="1"/>
</signal>
<signal name="PIN2">
<contactref element="U1" pad="2"/>
<contactref element="MISO" pad="1"/>
</signal>
<signal name="PIN3">
<contactref element="U1" pad="3"/>
<contactref element="WP" pad="1"/>
</signal>
<signal name="PIN4">
<contactref element="U1" pad="4"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="PIN5">
<contactref element="U1" pad="5"/>
<contactref element="MOSI" pad="1"/>
</signal>
<signal name="PIN6">
<contactref element="U1" pad="6"/>
<contactref element="SCK" pad="1"/>
</signal>
<signal name="PIN8">
<contactref element="U1" pad="8"/>
<contactref element="VCC" pad="1"/>
</signal>
<signal name="PIN7">
<contactref element="U1" pad="7"/>
<contactref element="HOLD" pad="1"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
