<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="-15.875" y1="-9.525" x2="15.875" y2="-9.525" width="0" layer="20"/>
<wire x1="15.875" y1="-9.525" x2="15.875" y2="9.525" width="0" layer="20"/>
<wire x1="15.875" y1="9.525" x2="-15.875" y2="9.525" width="0" layer="20"/>
<wire x1="-15.875" y1="9.525" x2="-15.875" y2="-9.525" width="0" layer="20"/>
<hole x="12.7" y="-6.35" drill="3"/>
<text>V1.1</text>
<text>Copyright (C) 2015 H.Pötzl
Licensed under CERN OHL v1.2</text>
<hole x="-12.7" y="-6.35" drill="3"/>
<hole x="12.7" y="6.35" drill="3"/>
<hole x="-12.7" y="6.35" drill="3"/>
<text>11th Order Butterworth
Low-Pass Filter</text>
</plain>
<libraries>
<library name="sma">
<packages>
<package name="SMA_EDGE_2SIDE">
</package>
</packages>
</library>
<library name="generic-rcl">
<packages>
<package name="0402-B">
</package>
<package name="0603-C">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IN" library="sma" package="SMA_EDGE_2SIDE" value="BU-SMA-E-2SIDE">
<attribute name="NAME"/>
</element>
<element name="OUT" library="sma" package="SMA_EDGE_2SIDE" value="BU-SMA-E-2SIDE">
<attribute name="NAME"/>
</element>
<element name="L1'" library="generic-rcl" package="0603-C" value="">
<attribute name="VALUE"/>
</element>
<element name="L5'" library="generic-rcl" package="0603-C" value="">
<attribute name="VALUE"/>
</element>
<element name="C2'" library="generic-rcl" package="0402-B" value="">
<attribute name="VALUE"/>
</element>
<element name="C3'" library="generic-rcl" package="0402-B" value="">
<attribute name="VALUE"/>
</element>
<element name="C4'" library="generic-rcl" package="0402-B" value="">
<attribute name="VALUE"/>
</element>
<element name="C5'" library="generic-rcl" package="0402-B" value="">
<attribute name="VALUE"/>
</element>
<element name="L2'" library="generic-rcl" package="0603-C" value="">
<attribute name="VALUE"/>
</element>
<element name="L3'" library="generic-rcl" package="0603-C" value="">
<attribute name="VALUE"/>
</element>
<element name="L4'" library="generic-rcl" package="0603-C" value="">
<attribute name="VALUE"/>
</element>
<element name="L2" library="generic-rcl" package="0603-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="generic-rcl" package="0603-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="generic-rcl" package="0603-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="generic-rcl" package="0603-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L5" library="generic-rcl" package="0603-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1'" library="generic-rcl" package="0402-B" value="">
<attribute name="VALUE"/>
</element>
<element name="C6" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6'" library="generic-rcl" package="0402-B" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IN" pad="2@2"/>
<contactref element="IN" pad="2@3"/>
<contactref element="IN" pad="2@1"/>
<contactref element="IN" pad="2@4"/>
<contactref element="OUT" pad="2@2"/>
<contactref element="OUT" pad="2@3"/>
<contactref element="OUT" pad="2@1"/>
<contactref element="OUT" pad="2@4"/>
<contactref element="C2'" pad="2"/>
<contactref element="C3'" pad="2"/>
<contactref element="C4'" pad="2"/>
<contactref element="C5'" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C1'" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C6'" pad="2"/>
</signal>
<signal name="OUT">
<contactref element="OUT" pad="1"/>
<contactref element="L5'" pad="2"/>
<contactref element="L5" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C6'" pad="1"/>
</signal>
<signal name="N$18">
</signal>
<signal name="N$16">
</signal>
<signal name="IN">
<contactref element="IN" pad="1"/>
<contactref element="L1'" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C1'" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="L1'" pad="2"/>
<contactref element="L2'" pad="1"/>
<contactref element="C2'" pad="1"/>
<contactref element="L2" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="L2'" pad="2"/>
<contactref element="L3'" pad="1"/>
<contactref element="C3'" pad="1"/>
<contactref element="L2" pad="2"/>
<contactref element="L3" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="L4'" pad="2"/>
<contactref element="L5'" pad="1"/>
<contactref element="C5'" pad="1"/>
<contactref element="L4" pad="2"/>
<contactref element="L5" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="L3" pad="2"/>
<contactref element="L4" pad="1"/>
<contactref element="L4'" pad="1"/>
<contactref element="C4'" pad="1"/>
<contactref element="L3'" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
