<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="11.25875" y2="0" width="0" layer="20"/>
<wire x1="11.25875" y1="0" x2="11.25875" y2="9.03875" width="0" layer="20"/>
<wire x1="11.25875" y1="9.03875" x2="0" y2="9.03875" width="0" layer="20"/>
<wire x1="0" y1="9.03875" x2="0" y2="0" width="0" layer="20"/>
<text>+</text>
<text>(c) packom.net
2016</text>
<text>555 led flasher
v0.1</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="SparkFun-Passives" package="0402-CAP" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0402-RES" value="56R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0402-RES" value="820K">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0402-RES" value="10K">
<attribute name="NAME"/>
</element>
<element name="U1" library="Texas Instruments_By_element14_Batch_1" package="SOIC127P600X175-8N" value="TLC555CD">
<attribute name="OC_FARNELL" value="1106128"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="MPN" value="TLC555CD"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="OC_NEWARK" value="67K1265"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
