<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="100" y1="36" x2="164.5" y2="36" width="0" layer="20"/>
<wire x1="164.5" y1="36" x2="164.5" y2="100" width="0" layer="20"/>
<wire x1="164.5" y1="100" x2="100" y2="100" width="0" layer="20"/>
<wire x1="100" y1="100" x2="100" y2="36" width="0" layer="20"/>
<text>USB 3.0 4-Port Hub</text>
<text>V1.0.0.0</text>
<text>TravisE</text>
<text>BATT Charger</text>
<text>BATT Charger</text>
<text>2A Load MAX</text>
<text>(Per Port. 8A Total)</text>
<text>BATT Charger: Port 1 &amp; Port 2</text>
<text>Power Supply: 5V 5A</text>
<text>Port 1</text>
<text>Port 2</text>
<text>Port 3</text>
<text>Port 4</text>
</plain>
<libraries>
<library name="ti_usb">
<packages>
<package name="VQFN64">
</package>
</packages>
</library>
<library name="AlexW-Eagle-Libraries">
<description>&lt;b&gt;Reference Package&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="AMPHENOLUSB3.0A">
</package>
<package name="AMPHENOLUSB3.0B">
<description>USB 3.0 B
Amphenol USB 3.0 B connector</description>
</package>
</packages>
</library>
<library name="common">
<packages>
<package name="0402L3">
</package>
<package name="0603L3">
</package>
<package name="1206L3">
</package>
<package name="0603L1">
</package>
<package name="0805L3">
</package>
</packages>
</library>
<library name="ti_ldo">
<packages>
<package name="S-PDSO-G8">
</package>
<package name="R-PSFM-G5">
</package>
<package name="S-PVQFN-N20">
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="CT7343">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="DCJACK_2MM_SMT">
<description>2.0/2.1mm DC Jack - SMT
&lt;p&gt;4UConnector: 03267&lt;/p&gt;
&lt;p&gt;Note: Small tRestrict polygon's were added to the ground pads to improve solderability when this part is used in combination with a ground pour.  By default, Eagle will product four large bridges to the ground pour significantly increasing the heat distribution on the pads and preventing lead-free solder from reflowing in certain situations.  For more details, see: http://www.microbuilder.eu/Blog/09-12-14/Reducing_Thermals_for_Large_Pads_in_Eagle.aspx&lt;/p&gt;</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="ti_usb" package="VQFN64" value="">
<attribute name="NAME"/>
</element>
<element name="JP1" library="AlexW-Eagle-Libraries" package="AMPHENOLUSB3.0A" value="USB3.0A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="AlexW-Eagle-Libraries" package="AMPHENOLUSB3.0A" value="USB3.0A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="AlexW-Eagle-Libraries" package="AMPHENOLUSB3.0A" value="USB3.0A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="AlexW-Eagle-Libraries" package="AMPHENOLUSB3.0A" value="USB3.0A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="common" package="0603L3" value="100n"/>
<element name="C6" library="common" package="0603L3" value="10n"/>
<element name="R1" library="common" package="0603L3" value="1M"/>
<element name="R2" library="common" package="0603L3" value="1M"/>
<element name="C7" library="common" package="0603L3" value="10n"/>
<element name="C8" library="common" package="0603L3" value="100n"/>
<element name="C9" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="common" package="0603L3" value="100n"/>
<element name="C12" library="common" package="0603L3" value="10n"/>
<element name="R3" library="common" package="0603L3" value="1M"/>
<element name="C13" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="common" package="0603L3" value="1M"/>
<element name="C15" library="common" package="0603L3" value="10n"/>
<element name="C16" library="common" package="0603L3" value="100n"/>
<element name="C17" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="AlexW-Eagle-Libraries" package="AMPHENOLUSB3.0B" value="USB3.0B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="common" package="0402L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="common" package="0603L3" value="10n"/>
<element name="C32" library="common" package="0603L3" value="100n"/>
<element name="R5" library="common" package="0603L3" value="1m"/>
<element name="C33" library="common" package="1206L3" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB2" library="common" package="0603L1" value="220 @ 100MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB3" library="common" package="0603L1" value="220 @ 100MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB4" library="common" package="0603L1" value="220 @ 100MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB5" library="common" package="0603L1" value="220 @ 100MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="common" package="1206L3" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="common" package="1206L3" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="common" package="1206L3" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="common" package="1206L3" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="ti_ldo" package="S-PDSO-G8" value="">
<attribute name="NAME"/>
</element>
<element name="U3" library="ti_ldo" package="S-PDSO-G8" value="">
<attribute name="NAME"/>
</element>
<element name="U4" library="ti_ldo" package="S-PDSO-G8" value="">
<attribute name="NAME"/>
</element>
<element name="U5" library="ti_ldo" package="S-PDSO-G8" value="">
<attribute name="NAME"/>
</element>
<element name="C38" library="rcl" package="CT7343" value="150u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="common" package="0603L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="rcl" package="CT7343" value="150u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="rcl" package="CT7343" value="150u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="rcl" package="CT7343" value="150u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="common" package="0603L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="common" package="0603L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="common" package="0603L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="common" package="0603L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="common" package="0603L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="common" package="0603L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="common" package="0603L3" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="common" package="0603L3" value=""/>
<element name="R7" library="common" package="0402L3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="common" package="0603L3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="common" package="0603L3" value=""/>
<element name="R10" library="common" package="0603L3" value=""/>
<element name="CN2" library="adafruit" package="DCJACK_2MM_SMT" value=""/>
<element name="C51" library="common" package="1206L3" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="ti_ldo" package="R-PSFM-G5" value=""/>
<element name="C52" library="common" package="1206L3" value="10u"/>
<element name="U8" library="ti_ldo" package="S-PVQFN-N20" value=""/>
<element name="C53" library="common" package="1206L3" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C54" library="common" package="1206L3" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C55" library="common" package="1206L3" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="common" package="0402L3" value="1.87k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="common" package="0402L3" value="4.99k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="adafruit" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="common" package="0603L3" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="common" package="0402L3" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C57" library="common" package="0402L3" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C58" library="common" package="0402L3" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C59" library="common" package="0402L3" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C60" library="common" package="0402L3" value="1n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C61" library="common" package="0402L3" value="1n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C62" library="common" package="0402L3" value="1n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C63" library="common" package="0402L3" value="1n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C64" library="common" package="0402L3" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C65" library="common" package="0402L3" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C66" library="common" package="0402L3" value="1n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C67" library="common" package="0402L3" value="1n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C68" library="common" package="0805L3" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C69" library="common" package="0805L3" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="common" package="0603L3" value="0 ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB6" library="common" package="0603L3" value="220 @ 100MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="HC49US" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R14" library="common" package="0402L3" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="common" package="0402L3" value="20pF"/>
<element name="C70" library="common" package="0402L3" value="20pF"/>
<element name="R15" library="common" package="0402L3" value="4.7K"/>
<element name="R17" library="common" package="0402L3" value="4.7K"/>
<element name="LED6" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="common" package="0402L3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="common" package="0402L3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="P1_SSTX_P">
<contactref element="U1" pad="3"/>
<contactref element="C2" pad="P$2"/>
</signal>
<signal name="P1_SSTX_N">
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="P$2"/>
</signal>
<signal name="P1_SSRX_P">
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="P1_SSRX_N">
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="P1_D_P">
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="P1_D_N">
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="P2_SSTX_N">
<contactref element="U1" pad="12"/>
<contactref element="C4" pad="P$2"/>
</signal>
<signal name="P2_SSRX_P">
<contactref element="U1" pad="14"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="P2_SSRX_N">
<contactref element="U1" pad="15"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="P2_D_P">
<contactref element="U1" pad="9"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="P2_D_N">
<contactref element="U1" pad="10"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="P1_CAP_SSTX_P">
<contactref element="JP1" pad="9"/>
<contactref element="C2" pad="P$1"/>
</signal>
<signal name="P1_CAP_SSTX_N">
<contactref element="JP1" pad="8"/>
<contactref element="C1" pad="P$1"/>
</signal>
<signal name="P2_SSTX_P">
<contactref element="U1" pad="11"/>
<contactref element="C3" pad="P$2"/>
</signal>
<signal name="P2_CAP_SSTX_N">
<contactref element="C4" pad="P$1"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="EARTH_GND">
<contactref element="JP1" pad="10@2"/>
<contactref element="JP1" pad="10@1"/>
<contactref element="C7" pad="P$1"/>
<contactref element="C8" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="JP2" pad="10@2"/>
<contactref element="JP2" pad="10@1"/>
<contactref element="C5" pad="P$2"/>
<contactref element="C6" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="JP4" pad="10@2"/>
<contactref element="JP4" pad="10@1"/>
<contactref element="R4" pad="P$2"/>
<contactref element="C15" pad="P$2"/>
<contactref element="C16" pad="P$2"/>
<contactref element="JP3" pad="10@2"/>
<contactref element="JP3" pad="10@1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="C11" pad="P$1"/>
<contactref element="C12" pad="P$1"/>
<contactref element="JP5" pad="10@2"/>
<contactref element="JP5" pad="10@1"/>
<contactref element="C31" pad="P$1"/>
<contactref element="C32" pad="P$1"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="P3_SSRX_P">
<contactref element="U1" pad="22"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="P3_SSRX_N">
<contactref element="U1" pad="23"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="P3_D_P">
<contactref element="U1" pad="17"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="P3_D_N">
<contactref element="U1" pad="18"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="P4_SSTX_N">
<contactref element="U1" pad="27"/>
<contactref element="C13" pad="P$1"/>
</signal>
<signal name="P4_SSRX_P">
<contactref element="U1" pad="29"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="P4_SSRX_N">
<contactref element="U1" pad="30"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="P4_D_P">
<contactref element="U1" pad="24"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="P4_D_N">
<contactref element="U1" pad="25"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="P3_CAP_SSTX_N">
<contactref element="C10" pad="P$2"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="P3_CAP_SSTX_P">
<contactref element="C9" pad="P$2"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="P3_SSTX_P">
<contactref element="U1" pad="19"/>
<contactref element="C9" pad="P$1"/>
</signal>
<signal name="P3_SSTX_N">
<contactref element="U1" pad="20"/>
<contactref element="C10" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="7"/>
<contactref element="JP1" pad="4"/>
<contactref element="C8" pad="P$2"/>
<contactref element="C7" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP2" pad="7"/>
<contactref element="C5" pad="P$1"/>
<contactref element="C6" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="JP4" pad="4"/>
<contactref element="R4" pad="P$1"/>
<contactref element="C15" pad="P$1"/>
<contactref element="C16" pad="P$1"/>
<contactref element="JP4" pad="7"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP3" pad="7"/>
<contactref element="R3" pad="P$2"/>
<contactref element="C12" pad="P$2"/>
<contactref element="C11" pad="P$2"/>
<contactref element="C18" pad="P$2"/>
<contactref element="C23" pad="P$2"/>
<contactref element="C24" pad="P$2"/>
<contactref element="C21" pad="P$2"/>
<contactref element="C22" pad="P$2"/>
<contactref element="C19" pad="P$2"/>
<contactref element="C20" pad="P$2"/>
<contactref element="C17" pad="P$2"/>
<contactref element="C26" pad="P$2"/>
<contactref element="C27" pad="P$2"/>
<contactref element="C28" pad="P$2"/>
<contactref element="C25" pad="P$2"/>
<contactref element="U1" pad="TP"/>
<contactref element="JP5" pad="7"/>
<contactref element="JP5" pad="4"/>
<contactref element="C32" pad="P$2"/>
<contactref element="C31" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="C33" pad="2"/>
<contactref element="C35" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="C36" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="C39" pad="P$2"/>
<contactref element="C38" pad="-"/>
<contactref element="C43" pad="P$2"/>
<contactref element="C40" pad="-"/>
<contactref element="C44" pad="P$2"/>
<contactref element="C41" pad="-"/>
<contactref element="C45" pad="P$2"/>
<contactref element="C42" pad="-"/>
<contactref element="C46" pad="P$1"/>
<contactref element="C47" pad="P$1"/>
<contactref element="C48" pad="P$1"/>
<contactref element="C49" pad="P$1"/>
<contactref element="R6" pad="P$1"/>
<contactref element="R7" pad="P$1"/>
<contactref element="R8" pad="P$1"/>
<contactref element="R9" pad="P$1"/>
<contactref element="R10" pad="P$1"/>
<contactref element="U2" pad="TP"/>
<contactref element="U3" pad="TP"/>
<contactref element="U4" pad="TP"/>
<contactref element="U5" pad="TP"/>
<contactref element="CN2" pad="GND"/>
<contactref element="CN2" pad="GNDBREAK"/>
<contactref element="C51" pad="2"/>
<contactref element="C52" pad="2"/>
<contactref element="U6" pad="3"/>
<contactref element="U6" pad="TP"/>
<contactref element="C53" pad="2"/>
<contactref element="C55" pad="2"/>
<contactref element="C54" pad="2"/>
<contactref element="R12" pad="P$1"/>
<contactref element="U8" pad="13"/>
<contactref element="U8" pad="14"/>
<contactref element="U8" pad="12"/>
<contactref element="U8" pad="TP"/>
<contactref element="U8" pad="4"/>
<contactref element="U8" pad="2"/>
<contactref element="U8" pad="3"/>
<contactref element="R13" pad="P$1"/>
<contactref element="C62" pad="P$2"/>
<contactref element="C57" pad="P$2"/>
<contactref element="C56" pad="P$2"/>
<contactref element="C59" pad="P$2"/>
<contactref element="C58" pad="P$2"/>
<contactref element="C61" pad="P$2"/>
<contactref element="C60" pad="P$2"/>
<contactref element="C63" pad="P$2"/>
<contactref element="C66" pad="P$2"/>
<contactref element="C67" pad="P$2"/>
<contactref element="C64" pad="P$2"/>
<contactref element="C65" pad="P$2"/>
<contactref element="C68" pad="2"/>
<contactref element="C69" pad="2"/>
<contactref element="C70" pad="P$1"/>
<contactref element="C50" pad="P$2"/>
<contactref element="R16" pad="P$1"/>
<contactref element="R18" pad="P$1"/>
</signal>
<signal name="P4_SSTX_P">
<contactref element="U1" pad="26"/>
<contactref element="C14" pad="P$1"/>
</signal>
<signal name="P4_CAP_SSTX_N">
<contactref element="JP4" pad="8"/>
<contactref element="C13" pad="P$2"/>
</signal>
<signal name="P4_CAP_SSTX_P">
<contactref element="JP4" pad="9"/>
<contactref element="C14" pad="P$2"/>
</signal>
<signal name="P2_CAP_SSTX_P">
<contactref element="JP2" pad="9"/>
<contactref element="C3" pad="P$1"/>
</signal>
<signal name="VDD33">
<contactref element="U1" pad="63"/>
<contactref element="U1" pad="16"/>
<contactref element="U1" pad="34"/>
<contactref element="U1" pad="52"/>
<contactref element="C26" pad="P$1"/>
<contactref element="C27" pad="P$1"/>
<contactref element="C28" pad="P$1"/>
<contactref element="C25" pad="P$1"/>
<contactref element="C66" pad="P$1"/>
<contactref element="C65" pad="P$1"/>
<contactref element="C64" pad="P$1"/>
<contactref element="C67" pad="P$1"/>
<contactref element="C69" pad="1"/>
<contactref element="FB6" pad="P$1"/>
<contactref element="R15" pad="P$2"/>
<contactref element="R17" pad="P$2"/>
</signal>
<signal name="US_CAP_SSTX_N">
<contactref element="JP5" pad="5"/>
<contactref element="C29" pad="P$1"/>
</signal>
<signal name="US_CAP_SSTX_P">
<contactref element="JP5" pad="6"/>
<contactref element="C30" pad="P$1"/>
</signal>
<signal name="US_SSTX_P">
<contactref element="U1" pad="55"/>
<contactref element="C29" pad="P$2"/>
</signal>
<signal name="US_SSTX_N">
<contactref element="U1" pad="56"/>
<contactref element="C30" pad="P$2"/>
</signal>
<signal name="US_SSRX_P">
<contactref element="U1" pad="58"/>
<contactref element="JP5" pad="8"/>
</signal>
<signal name="US_SSRX_N">
<contactref element="U1" pad="59"/>
<contactref element="JP5" pad="9"/>
</signal>
<signal name="US_D_P">
<contactref element="U1" pad="53"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="US_D_N">
<contactref element="U1" pad="54"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="US_VBUS">
<contactref element="JP5" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="U1" pad="48"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="1"/>
<contactref element="FB3" pad="1"/>
<contactref element="C35" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="JP2" pad="1"/>
<contactref element="FB2" pad="2"/>
<contactref element="C34" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="JP3" pad="1"/>
<contactref element="FB4" pad="1"/>
<contactref element="C37" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="FB5" pad="2"/>
<contactref element="C36" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="PWRCTL2">
<contactref element="U1" pad="35"/>
<contactref element="U3" pad="4"/>
<contactref element="R17" pad="P$1"/>
</signal>
<signal name="OVERCUR2Z">
<contactref element="U1" pad="47"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="OVERCUR4Z">
<contactref element="U1" pad="43"/>
<contactref element="U5" pad="5"/>
</signal>
<signal name="PWRCTL4">
<contactref element="U1" pad="32"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="OVERCUR3Z">
<contactref element="U1" pad="44"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="PWRCTL3">
<contactref element="U1" pad="33"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="OVERCUR1Z">
<contactref element="U1" pad="46"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="PWRCTL1">
<contactref element="U1" pad="36"/>
<contactref element="U2" pad="4"/>
<contactref element="R15" pad="P$1"/>
</signal>
<signal name="BOARD_5V">
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="3"/>
<contactref element="U5" pad="2"/>
<contactref element="U5" pad="3"/>
<contactref element="C46" pad="P$2"/>
<contactref element="C47" pad="P$2"/>
<contactref element="C49" pad="P$2"/>
<contactref element="C48" pad="P$2"/>
<contactref element="CN2" pad="PWR1"/>
<contactref element="C51" pad="1"/>
<contactref element="U6" pad="2"/>
<contactref element="U6" pad="1"/>
<contactref element="C52" pad="1"/>
</signal>
<signal name="DN2_VBUS">
<contactref element="U3" pad="8"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="7"/>
<contactref element="FB2" pad="1"/>
<contactref element="C43" pad="P$1"/>
<contactref element="C40" pad="+"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="DN1_VBUS">
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="7"/>
<contactref element="FB3" pad="2"/>
<contactref element="C38" pad="+"/>
<contactref element="C39" pad="P$1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="DN3_VBUS">
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="6"/>
<contactref element="U4" pad="7"/>
<contactref element="FB4" pad="2"/>
<contactref element="C41" pad="+"/>
<contactref element="C44" pad="P$1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="DN4_VBUS">
<contactref element="U5" pad="8"/>
<contactref element="U5" pad="6"/>
<contactref element="U5" pad="7"/>
<contactref element="FB5" pad="1"/>
<contactref element="C45" pad="P$1"/>
<contactref element="C42" pad="+"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="64"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="LED2" pad="C"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="LED3" pad="C"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="N$9">
<contactref element="LED4" pad="C"/>
<contactref element="R10" pad="P$2"/>
</signal>
<signal name="CLK_N">
<contactref element="Y1" pad="2"/>
<contactref element="R14" pad="P$2"/>
<contactref element="U1" pad="62"/>
<contactref element="C70" pad="P$2"/>
</signal>
<signal name="BOARD_3V3">
<contactref element="U6" pad="4"/>
<contactref element="U6" pad="5"/>
<contactref element="C53" pad="1"/>
<contactref element="U8" pad="8"/>
<contactref element="U8" pad="6"/>
<contactref element="U8" pad="7"/>
<contactref element="U8" pad="5"/>
<contactref element="C54" pad="1"/>
<contactref element="U8" pad="10"/>
<contactref element="U8" pad="11"/>
<contactref element="LED5" pad="A"/>
<contactref element="FB6" pad="P$2"/>
</signal>
<signal name="BOARD_1V1">
<contactref element="U8" pad="18"/>
<contactref element="U8" pad="20"/>
<contactref element="U8" pad="19"/>
<contactref element="U8" pad="1"/>
<contactref element="C55" pad="1"/>
<contactref element="R11" pad="P$2"/>
<contactref element="FB1" pad="P$2"/>
</signal>
<signal name="N$15">
<contactref element="R12" pad="P$2"/>
<contactref element="R11" pad="P$1"/>
<contactref element="U8" pad="16"/>
</signal>
<signal name="N$13">
<contactref element="LED5" pad="C"/>
<contactref element="R13" pad="P$2"/>
</signal>
<signal name="VDD11">
<contactref element="C18" pad="P$1"/>
<contactref element="C23" pad="P$1"/>
<contactref element="C17" pad="P$1"/>
<contactref element="C20" pad="P$1"/>
<contactref element="C19" pad="P$1"/>
<contactref element="C22" pad="P$1"/>
<contactref element="C21" pad="P$1"/>
<contactref element="C24" pad="P$1"/>
<contactref element="C62" pad="P$1"/>
<contactref element="C63" pad="P$1"/>
<contactref element="C60" pad="P$1"/>
<contactref element="C61" pad="P$1"/>
<contactref element="C58" pad="P$1"/>
<contactref element="C59" pad="P$1"/>
<contactref element="C56" pad="P$1"/>
<contactref element="C57" pad="P$1"/>
<contactref element="C68" pad="1"/>
<contactref element="FB1" pad="P$1"/>
<contactref element="U1" pad="57"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="31"/>
<contactref element="U1" pad="51"/>
</signal>
<signal name="CLK_P">
<contactref element="Y1" pad="1"/>
<contactref element="R14" pad="P$1"/>
<contactref element="U1" pad="61"/>
<contactref element="C50" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="R16" pad="P$2"/>
<contactref element="LED6" pad="C"/>
</signal>
<signal name="N$11">
<contactref element="R18" pad="P$2"/>
<contactref element="LED7" pad="C"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="42"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="40"/>
<contactref element="LED6" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
